<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="166.25" y2="0" width="0.18" layer="20"/>
<wire x1="166.25" y1="0" x2="166.25" y2="191.516" width="0.18" layer="20"/>
<wire x1="166.25" y1="191.516" x2="0" y2="191.516" width="0.18" layer="20"/>
<wire x1="0" y1="191.516" x2="0" y2="0" width="0.18" layer="20"/>
<text>"Lock"</text>
<text>"Freq On"</text>
<text>"Polarity"</text>
<text>"Lock"</text>
<text>"Freq On"</text>
<text>"Polarity"</text>
<text>Preamp</text>
<text>f -3dB</text>
<text>Lf gain</text>
<text>Gain</text>
<text>Preamp</text>
<text>F -3dB</text>
<text>Gain</text>
<text>LF Gain</text>
<text>F Pol</text>
<text>F Pol</text>
<text>"Schlosser"</text>
<text>Laser Lock</text>
<text>B1</text>
<text>A.Stummer Jan'09</text>
<text>0.18mm (7m")</text>
<text>0.18mm (7m")</text>
<text>0.18mm (7m")</text>
<text>0.127mm (5m")</text>
<text>1mm (39.4m")</text>
<text>Case: Hammond 1598D(GY)</text>
<text>"Freq LED"</text>
<text>"Freq LED"</text>
<text>Set</text>
<text>Set</text>
<text>"Schlosser" Laser Lock   Rev:B</text>
<text>University of Toronto - Physics</text>
<text>A. Steinberg Labs</text>
<text>Use (imperial) #6-32 x 0.25" PH screws for PCB.</text>
</plain>
<libraries>
<library name="QuantumOptics">
<packages>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1.&lt;br&gt;
Don't forget the nut 1-329631-2 and maybe the shoulder washer 330620.&lt;br&gt;
Now with new &amp; improved mtg holes compared to ...TYPE2...!&lt;br&gt;
The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, 0.075" c-c pad spacing.  Preferred grid is 0.025".</description>
</package>
<package name="BOURNS-3296Y">
<description>&lt;b&gt;3296Y Trimpot, Multi-turn&lt;/b&gt;, Bourns.  Staggered pins so can insert trimpot one way only.&lt;br&gt;
http://www.bourns.com/pdf/3296.pdf</description>
</package>
<package name="3225(2510)">
<description>&lt;b&gt;1210 SMT package&lt;/b&gt;, for two terminal passives.</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire.  Has fence (bit larger than other TP) around to allow easier soldering.</description>
</package>
<package name="JUMPER-3">
<description>&lt;b&gt;Jumper 3-pin header&lt;/b&gt;, vertical SIP on 0.1" grid.</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, use 0.0125" grid.</description>
</package>
<package name="SWITCH:E-SWITCH_2??D?AV2?">
<description>&lt;b&gt;Toggle DPDT, right angle PCB, vertical actuation&lt;/b&gt;, C&amp;K E-Switch series, such as E201MD1AV2BE (on-on) or E203MD1AV2BE (on-off-on).</description>
</package>
<package name="SWITCH:E-SWITCH_1??AV2?">
<description>&lt;b&gt;Toggle SPDT, right angle PCB, vertical actuation&lt;/b&gt;, C&amp;K E-Switch series, such as E101MD1AV2BE (on-on) or E103MD1AV2BE (on-off-on).</description>
</package>
<package name="CC3-XXXXX-E(TDK_DC-DC)">
<description>&lt;b&gt;CC3-inoutsR-E&lt;/b&gt;, TDK DC-DC isolated, 3W, uni- or bipolar&lt;br&gt;
"in": Input 05, 12, 24 or 48V.&lt;br&gt;
"out": Output 3.3, 5, 12, ±12 (or 24), ±15 (or30V).&lt;br&gt;
"s": Polarity single or dual.&lt;br&gt;
Case horiz SMD.&lt;br&gt;
http://www.tdk.co.jp/tefe02/ea335_cc_e.pdf</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.&lt;br&gt;
http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="CAP:NIPPONCHEM_H70_H80">
<description>&lt;b&gt;Capacitor, polarized, Nippon Chemi-con Corp, H70 and H80 packages
&lt;/b&gt;.  Round SMT with plastic standoff.  Bit awkward to install.</description>
</package>
<package name="SWITCH:E-SWITCH_2??D?A?">
<description>&lt;b&gt;Toggle DPDT, right angle PCB, horizontal actator&lt;/b&gt;, C&amp;K E-Switch series, such as E201MD1ABE (on-on).</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="CASE:HAMMOND_1598D">
<description>&lt;b&gt;Case, Hammond 1598D&lt;/b&gt;, case is 206mmW x 180D x 64H, http://www.hammondmfg.com/pdf/1598D.pdf.&lt;br&gt;
Has 0.5mm space between PCB and inside of front and back plates, larger gap at sides.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;PD In L&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="4.99M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="QuantumOptics" package="JUMPER-3" value="&quot;Setpoint&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3590S-2-103L"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;Scope Y&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;Preamp&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-103"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;f-3dB&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-104"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="56nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="TP7" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="TP3" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="IC3" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="QuantumOptics" package="2012(0805)" value="499K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R36" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="QuantumOptics" package="JUMPER-3" value="">
<attribute name="NAME"/>
<attribute name="MONIKER" value="&quot;Freq Pol.&quot;"/>
</element>
<element name="R44" library="QuantumOptics" package="2012(0805)" value="2.21M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="QuantumOptics" package="3225(2510)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="ECP-U1C105MA5"/>
</element>
<element name="J9" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;Freq-L&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R50" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;Current-L&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R48" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW6" library="QuantumOptics" package="SWITCH:E-SWITCH_2??D?AV2?" value="&quot;Lock&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="E203MD1AV2BE"/>
</element>
<element name="SW4" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="&quot;Freq On&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="E101MD1AV2BE"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="QuantumOptics" package="2012(0805)" value="34K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="QuantumOptics" package="JUMPER-3" value="WP59EGW">
<attribute name="NAME"/>
<attribute name="MFG" value="Kingbright"/>
</element>
<element name="D2" library="QuantumOptics" package="SOT23" value="BAT46AFILM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="STM Micro."/>
</element>
<element name="R51" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;Gain&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-104"/>
</element>
<element name="R29" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;Lf-Gain&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-104"/>
</element>
<element name="TP5" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH:E-SWITCH_2??D?A?" value="&quot;Channel&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="E201MD1ABE"/>
</element>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="&quot;Polarity&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="E101MD1AV2BE"/>
</element>
<element name="IC5" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;PD In R&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="4.99M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QuantumOptics" package="JUMPER-3" value="&quot;Setpoint&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3590S-2-103L"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;Preamp&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-103"/>
</element>
<element name="IC6" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;f-3dB&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-104"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="56nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="TP9" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="TP4" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="IC7" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="QuantumOptics" package="2012(0805)" value="499K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R40" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="QuantumOptics" package="JUMPER-3" value="">
<attribute name="NAME"/>
<attribute name="MONIKER" value="&quot;Freq Pol.&quot;"/>
</element>
<element name="R45" library="QuantumOptics" package="2012(0805)" value="2.21M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="QuantumOptics" package="3225(2510)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="ECP-U1C105MA5"/>
</element>
<element name="J10" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;Freq-R&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R52" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;Current-R&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R49" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW7" library="QuantumOptics" package="SWITCH:E-SWITCH_2??D?AV2?" value="&quot;Lock&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="E203MD1AV2BE"/>
</element>
<element name="SW5" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="&quot;Freq On&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="E101MD1AV2BE"/>
</element>
<element name="D3" library="QuantumOptics" package="JUMPER-3" value="WP59EGW">
<attribute name="NAME"/>
<attribute name="MFG" value="Kingbright"/>
</element>
<element name="D4" library="QuantumOptics" package="SOT23" value="BAT46AFILM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="STM Micro."/>
</element>
<element name="R53" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;Gain&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-104"/>
</element>
<element name="R31" library="QuantumOptics" package="BOURNS-3296Y" value="&quot;Lf-Gain&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3296Y-1-104"/>
</element>
<element name="TP6" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW3" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="&quot;Polarity&quot;">
<attribute name="NAME"/>
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="E101MD1AV2BE"/>
</element>
<element name="C15" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;Scope X&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ACCES" value="Nut 1-329631-2"/>
<attribute name="MFG" value="Amp"/>
<attribute name="PN" value="5227677-1"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR1" library="QuantumOptics" package="CC3-XXXXX-E(TDK_DC-DC)" value="CC3-0512DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QuantumOptics" package="CAP:NIPPONCHEM_H70_H80" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="United Chemi-Con"/>
<attribute name="PN" value="APXE160ARA101MH70G"/>
</element>
<element name="C4" library="QuantumOptics" package="CAP:NIPPONCHEM_H70_H80" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="United Chemi-Con"/>
<attribute name="PN" value="APXE160ARA101MH70G"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOT23" value="ADR525BRT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="QuantumOptics" package="SOT23" value="ADR525BRT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.5A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Littlefuse"/>
<attribute name="PN" value="2 of 100056"/>
</element>
<element name="+5V_IN" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="IN_COM" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$52" library="QuantumOptics" package="CASE:HAMMOND_1598D" value=""/>
<element name="R46" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$54" library="QuantumOptics" package="TITLEBLOCK_PCB" value=""/>
</elements>
<signals>
<signal name="AGND">
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="J2" pad="SHIELD2"/>
<contactref element="J2" pad="SHIELD1"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R12" pad="CCW"/>
<contactref element="R28" pad="CCW"/>
<contactref element="R29" pad="CCW"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="5"/>
<contactref element="J9" pad="SHIELD2"/>
<contactref element="J9" pad="SHIELD1"/>
<contactref element="J7" pad="SHIELD2"/>
<contactref element="J7" pad="SHIELD1"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC4" pad="6"/>
<contactref element="D1" pad="3"/>
<contactref element="D2" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="SW2" pad="DOWN"/>
<contactref element="R24" pad="1"/>
<contactref element="J4" pad="SHIELD2"/>
<contactref element="J4" pad="SHIELD1"/>
<contactref element="IC5" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="R13" pad="CCW"/>
<contactref element="R30" pad="CCW"/>
<contactref element="R31" pad="CCW"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC7" pad="5"/>
<contactref element="J10" pad="SHIELD2"/>
<contactref element="J10" pad="SHIELD1"/>
<contactref element="J8" pad="SHIELD2"/>
<contactref element="J8" pad="SHIELD1"/>
<contactref element="D3" pad="3"/>
<contactref element="D4" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="SW3" pad="DOWN"/>
<contactref element="R25" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="J3" pad="SHIELD2"/>
<contactref element="J3" pad="SHIELD1"/>
<contactref element="PWR1" pad="COM"/>
<contactref element="C3" pad="NEG"/>
<contactref element="C4" pad="POS"/>
<contactref element="IC8" pad="2"/>
<contactref element="IC9" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="CONDUCTOR"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="CW"/>
<contactref element="SW1" pad="LEFT1"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="CONDUCTOR"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="C3" pad="POS"/>
<contactref element="PWR1" pad="+VOUT"/>
<contactref element="IC1" pad="8"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="C9" pad="1"/>
<contactref element="IC3" pad="8"/>
<contactref element="C11" pad="1"/>
<contactref element="IC4" pad="8"/>
<contactref element="C15" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="C17" pad="1"/>
<contactref element="IC6" pad="8"/>
<contactref element="C19" pad="1"/>
<contactref element="IC7" pad="8"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="-12V">
<contactref element="PWR1" pad="-VOUT"/>
<contactref element="C4" pad="NEG"/>
<contactref element="C6" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="C8" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="C10" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="C12" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="C16" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="C18" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="C20" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="-2.5V">
<contactref element="R6" pad="3"/>
<contactref element="IC9" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="R8" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R14" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R18" pad="2"/>
<contactref element="R20" pad="W"/>
<contactref element="TP3" pad="TP"/>
<contactref element="R20" pad="CCW"/>
<contactref element="IC1" pad="7"/>
<contactref element="R28" pad="CW"/>
</signal>
<signal name="N$8">
<contactref element="R15" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="SW2" pad="COM"/>
</signal>
<signal name="N$10">
<contactref element="R14" pad="1"/>
<contactref element="R12" pad="W"/>
<contactref element="R15" pad="1"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$14">
<contactref element="R37" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="R29" pad="W"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="N$19">
<contactref element="IC3" pad="2"/>
<contactref element="R42" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC3" pad="1"/>
<contactref element="R42" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="SW6" pad="UP1"/>
</signal>
<signal name="N$11">
<contactref element="R35" pad="1"/>
<contactref element="R34" pad="1"/>
<contactref element="R28" pad="W"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="N$17">
<contactref element="R36" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J5" pad="3"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="J5" pad="2"/>
<contactref element="IC3" pad="6"/>
<contactref element="C21" pad="1"/>
<contactref element="R46" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="C21" pad="2"/>
<contactref element="SW4" pad="COM"/>
<contactref element="R50" pad="2"/>
<contactref element="IC3" pad="7"/>
<contactref element="R51" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="J9" pad="CONDUCTOR"/>
<contactref element="R50" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="J7" pad="CONDUCTOR"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="SW6" pad="COM1"/>
<contactref element="R48" pad="2"/>
<contactref element="SW1" pad="LEFT2"/>
</signal>
<signal name="N$27">
<contactref element="R55" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="R56" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="C23" pad="1"/>
<contactref element="IC4" pad="2"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="14VPP@4HZ">
<contactref element="IC4" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="SW6" pad="DN2"/>
<contactref element="SW6" pad="DN1"/>
<contactref element="SW7" pad="DN1"/>
<contactref element="SW7" pad="DN2"/>
</signal>
<signal name="N$28">
<contactref element="D2" pad="3"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R22" pad="2"/>
<contactref element="TP5" pad="TP"/>
<contactref element="R20" pad="CW"/>
</signal>
<signal name="N$13">
<contactref element="R22" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="R29" pad="CW"/>
</signal>
<signal name="N$16">
<contactref element="R56" pad="2"/>
<contactref element="IC4" pad="7"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R55" pad="1"/>
<contactref element="SW6" pad="COM2"/>
<contactref element="SW7" pad="COM2"/>
</signal>
<signal name="N$26">
<contactref element="R3" pad="2"/>
<contactref element="SW1" pad="COM1"/>
</signal>
<signal name="N$31">
<contactref element="R26" pad="2"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$32">
<contactref element="IC2" pad="5"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R26" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$35">
<contactref element="J4" pad="CONDUCTOR"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R5" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="R11" pad="2"/>
<contactref element="R13" pad="CW"/>
<contactref element="IC5" pad="1"/>
<contactref element="SW1" pad="RIGHT1"/>
</signal>
<signal name="N$38">
<contactref element="R8" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="R16" pad="2"/>
<contactref element="IC5" pad="6"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="R19" pad="2"/>
<contactref element="R21" pad="W"/>
<contactref element="TP4" pad="TP"/>
<contactref element="R21" pad="CCW"/>
<contactref element="IC5" pad="7"/>
<contactref element="R30" pad="CW"/>
</signal>
<signal name="N$42">
<contactref element="R17" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="SW3" pad="COM"/>
</signal>
<signal name="N$43">
<contactref element="R16" pad="1"/>
<contactref element="R13" pad="W"/>
<contactref element="R17" pad="1"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$44">
<contactref element="R41" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="R31" pad="W"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="N$45">
<contactref element="IC7" pad="2"/>
<contactref element="R43" pad="1"/>
<contactref element="R41" pad="2"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="IC7" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="R45" pad="2"/>
<contactref element="SW7" pad="UP1"/>
</signal>
<signal name="N$47">
<contactref element="R39" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="R30" pad="W"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="N$48">
<contactref element="R40" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="J6" pad="3"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="J6" pad="2"/>
<contactref element="IC7" pad="6"/>
<contactref element="C22" pad="1"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="C22" pad="2"/>
<contactref element="SW5" pad="COM"/>
<contactref element="R52" pad="2"/>
<contactref element="IC7" pad="7"/>
<contactref element="R53" pad="2"/>
</signal>
<signal name="N$52">
<contactref element="J10" pad="CONDUCTOR"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="J8" pad="CONDUCTOR"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="SW7" pad="COM1"/>
<contactref element="R49" pad="2"/>
<contactref element="SW1" pad="RIGHT2"/>
</signal>
<signal name="N$55">
<contactref element="D4" pad="3"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="D3" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="R23" pad="2"/>
<contactref element="TP6" pad="TP"/>
<contactref element="R21" pad="CW"/>
</signal>
<signal name="N$58">
<contactref element="R23" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="IC6" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="IC6" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="R31" pad="CW"/>
</signal>
<signal name="N$61">
<contactref element="R27" pad="2"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="N$62">
<contactref element="IC6" pad="5"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$63">
<contactref element="R27" pad="1"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="N$34">
<contactref element="J3" pad="CONDUCTOR"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="PWR1" pad="RC"/>
<contactref element="PWR1" pad="-VIN"/>
<contactref element="IN_COM" pad="TP"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="F1" pad="2A"/>
<contactref element="PWR1" pad="+VIN"/>
</signal>
<signal name="N$64">
<contactref element="F1" pad="1A"/>
<contactref element="+5V_IN" pad="TP"/>
</signal>
<signal name="N$65">
<contactref element="SW4" pad="DOWN"/>
<contactref element="R46" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="SW5" pad="DOWN"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="R4" pad="2"/>
<contactref element="SW1" pad="COM2"/>
</signal>
<signal name="+2.5V">
<contactref element="IC8" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
