<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="328.2" y2="0" width="0" layer="20"/>
<wire x1="328.2" y1="0" x2="328.2" y2="68.52" width="0" layer="20"/>
<wire x1="328.2" y1="68.52" x2="0" y2="68.52" width="0" layer="20"/>
<wire x1="0" y1="68.52" x2="0" y2="0" width="0" layer="20"/>
<text>ADWin Digital Buffer</text>
<text>J. Thywissen Labs</text>
<text>Stummer/Myrskog Aug'05</text>
<text>G</text>
<text>0.18mm</text>
<text>0.36mm</text>
<text>0.18mm</text>
<text>0.25mm</text>
<text>0.5mm</text>
<text>0.5A</text>
<text>1A</text>
<text>ADWin Digital Buffer
Rev: G
University of Toronto
J.Thywissen Labs</text>
<text>5V+</text>
<text>5V-</text>
</plain>
<libraries>
<library name="0-UofT-Physics">
<packages>
<package name="0805">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, 0.075" c-c pad spacing.  Preferred grid is 0.025".</description>
</package>
<package name="EIA-B">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, EIA size B, SMT.&lt;br&gt;
Pad 0.100" x 0.070",  overall pads 0.100" x 0.180".</description>
</package>
<package name="TP-HOLE">
<description>&lt;b&gt;Test Point&lt;/b&gt;, with 0.042" through-hole.</description>
</package>
</packages>
</library>
<library name="QuantumOptics">
<packages>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056 or lower profile 01110005MR.</description>
</package>
<package name="SOIC-16W">
<description>&lt;b&gt;SOIC-16 Wide&lt;/b&gt; on 0.050" grid.&lt;br&gt;
http://www.analog.com/UploadedFiles/Packages/37806216RW_16.pdf</description>
</package>
<package name="CONN-BNC-AMP-TYPE1VERT">
<description>&lt;b&gt;BNC PCB mount connector&lt;/b&gt;, Tyco, vertical, 0.1" grid, types such as 227673-1.&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;M=BYPN&amp;PID=4946&amp;PN=227673-1&amp;I=13</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="CONN:DB37-VERT">
<description>&lt;b&gt;Sub-D&lt;/b&gt;, 37 pin, vertical PCB mount.</description>
</package>
<package name="SOIC24">
<description>&lt;b&gt; SOIC-24&lt;/B&gt;, TI's DW package, 0.05" pad spacing with 10mm (0.394") wide case and 10.63WOA.</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="0-UofT-Physics" package="EIA-B" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SUPPLY_+5V" library="0-UofT-Physics" package="TP-HOLE" value=""/>
<element name="SUPPLY_RETURN" library="0-UofT-Physics" package="TP-HOLE" value=""/>
<element name="ZD1" library="0-UofT-Physics" package="EIA-B" value="1N5339">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.5A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$19" library="QuantumOptics" package="TITLEBLOCK_PCB" value=""/>
<element name="C14" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="0-UofT-Physics" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC10" library="QuantumOptics" package="SOIC-16W" value="ADUM1400BRW">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC1" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC2" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC3" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC4" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC5" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC6" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC7" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC8" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC9" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC10" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC11" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC12" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC13" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC14" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC15" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC16" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC17" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC18" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC19" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC20" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC21" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC22" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC23" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC24" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC25" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC26" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC27" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC28" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC29" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC30" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC31" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BNC32" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="AMP 227673-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="QuantumOptics" package="FUSE" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN:DB37-VERT" value="Norcomp 191-037-223R001"/>
<element name="IC11" library="QuantumOptics" package="SOIC24" value="SN64BCT25244DW"/>
<element name="IC12" library="QuantumOptics" package="SOIC24" value="SN64BCT25244DW"/>
<element name="IC6" library="QuantumOptics" package="SOIC24" value="SN64BCT25244DW"/>
<element name="IC3" library="QuantumOptics" package="SOIC24" value="SN64BCT25244DW"/>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R13" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R27" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R28" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R29" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R30" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R31" library="QuantumOptics" package="2012(0805)" value="49.9"/>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="49.9"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC2" pad="14"/>
<contactref element="IC3" pad="23"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="13"/>
<contactref element="IC3" pad="22"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="12"/>
<contactref element="IC3" pad="20"/>
</signal>
<signal name="N$4">
<contactref element="IC2" pad="11"/>
<contactref element="IC3" pad="19"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="11"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="12"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="13"/>
<contactref element="IC3" pad="17"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="14"/>
<contactref element="IC3" pad="18"/>
</signal>
<signal name="WGND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC4" pad="2"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC7" pad="2"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC8" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="IC9" pad="8"/>
<contactref element="IC9" pad="2"/>
<contactref element="IC10" pad="8"/>
<contactref element="IC10" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="21"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="C5" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="ZD1" pad="2"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC4" pad="16"/>
<contactref element="IC5" pad="16"/>
<contactref element="IC8" pad="16"/>
<contactref element="C17" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="IC7" pad="16"/>
<contactref element="IC10" pad="16"/>
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="IC9" pad="16"/>
<contactref element="F2" pad="1A"/>
<contactref element="IC11" pad="21"/>
<contactref element="IC11" pad="16"/>
<contactref element="IC12" pad="21"/>
<contactref element="IC12" pad="16"/>
<contactref element="IC6" pad="21"/>
<contactref element="IC6" pad="16"/>
<contactref element="IC3" pad="21"/>
<contactref element="IC3" pad="16"/>
<contactref element="F2" pad="1B"/>
</signal>
<signal name="AGND">
<contactref element="C5" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="SUPPLY_RETURN" pad="P$1"/>
<contactref element="C6" pad="1"/>
<contactref element="ZD1" pad="1"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="15"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC4" pad="15"/>
<contactref element="IC5" pad="9"/>
<contactref element="IC5" pad="15"/>
<contactref element="IC7" pad="9"/>
<contactref element="IC7" pad="15"/>
<contactref element="IC8" pad="9"/>
<contactref element="IC8" pad="15"/>
<contactref element="C17" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="IC9" pad="9"/>
<contactref element="IC9" pad="15"/>
<contactref element="IC10" pad="9"/>
<contactref element="IC10" pad="15"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="BNC1" pad="SHIELD"/>
<contactref element="BNC8" pad="SHIELD"/>
<contactref element="BNC7" pad="SHIELD"/>
<contactref element="BNC6" pad="SHIELD"/>
<contactref element="BNC5" pad="SHIELD"/>
<contactref element="BNC4" pad="SHIELD"/>
<contactref element="BNC3" pad="SHIELD"/>
<contactref element="BNC2" pad="SHIELD"/>
<contactref element="BNC16" pad="SHIELD"/>
<contactref element="BNC9" pad="SHIELD"/>
<contactref element="BNC15" pad="SHIELD"/>
<contactref element="BNC14" pad="SHIELD"/>
<contactref element="BNC13" pad="SHIELD"/>
<contactref element="BNC12" pad="SHIELD"/>
<contactref element="BNC11" pad="SHIELD"/>
<contactref element="BNC10" pad="SHIELD"/>
<contactref element="BNC24" pad="SHIELD"/>
<contactref element="BNC17" pad="SHIELD"/>
<contactref element="BNC18" pad="SHIELD"/>
<contactref element="BNC19" pad="SHIELD"/>
<contactref element="BNC20" pad="SHIELD"/>
<contactref element="BNC21" pad="SHIELD"/>
<contactref element="BNC22" pad="SHIELD"/>
<contactref element="BNC23" pad="SHIELD"/>
<contactref element="BNC25" pad="SHIELD"/>
<contactref element="BNC30" pad="SHIELD"/>
<contactref element="BNC29" pad="SHIELD"/>
<contactref element="BNC28" pad="SHIELD"/>
<contactref element="BNC27" pad="SHIELD"/>
<contactref element="BNC26" pad="SHIELD"/>
<contactref element="BNC31" pad="SHIELD"/>
<contactref element="BNC32" pad="SHIELD"/>
<contactref element="IC11" pad="11"/>
<contactref element="IC11" pad="2"/>
<contactref element="IC11" pad="5"/>
<contactref element="IC11" pad="8"/>
<contactref element="IC11" pad="24"/>
<contactref element="IC11" pad="13"/>
<contactref element="IC12" pad="11"/>
<contactref element="IC12" pad="2"/>
<contactref element="IC12" pad="5"/>
<contactref element="IC12" pad="8"/>
<contactref element="IC12" pad="24"/>
<contactref element="IC12" pad="13"/>
<contactref element="IC6" pad="11"/>
<contactref element="IC6" pad="2"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC6" pad="8"/>
<contactref element="IC6" pad="24"/>
<contactref element="IC6" pad="13"/>
<contactref element="IC3" pad="11"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="24"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="D28">
<contactref element="IC9" pad="3"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="D26">
<contactref element="IC10" pad="5"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="D24">
<contactref element="IC10" pad="3"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="D22">
<contactref element="IC7" pad="5"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="D20">
<contactref element="IC7" pad="3"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="D16">
<contactref element="IC8" pad="3"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="D10">
<contactref element="IC5" pad="5"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="5"/>
<contactref element="J1" pad="16"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="17"/>
</signal>
<signal name="D2">
<contactref element="IC2" pad="5"/>
<contactref element="J1" pad="18"/>
</signal>
<signal name="D0">
<contactref element="IC2" pad="3"/>
<contactref element="J1" pad="19"/>
</signal>
<signal name="D31">
<contactref element="IC9" pad="6"/>
<contactref element="J1" pad="22"/>
</signal>
<signal name="D29">
<contactref element="IC9" pad="4"/>
<contactref element="J1" pad="23"/>
</signal>
<signal name="D27">
<contactref element="IC10" pad="6"/>
<contactref element="J1" pad="24"/>
</signal>
<signal name="D25">
<contactref element="IC10" pad="4"/>
<contactref element="J1" pad="25"/>
</signal>
<signal name="D23">
<contactref element="IC7" pad="6"/>
<contactref element="J1" pad="26"/>
</signal>
<signal name="D21">
<contactref element="IC7" pad="4"/>
<contactref element="J1" pad="27"/>
</signal>
<signal name="D19">
<contactref element="IC8" pad="6"/>
<contactref element="J1" pad="28"/>
</signal>
<signal name="D17">
<contactref element="IC8" pad="4"/>
<contactref element="J1" pad="29"/>
</signal>
<signal name="D15">
<contactref element="IC4" pad="6"/>
<contactref element="J1" pad="30"/>
</signal>
<signal name="D13">
<contactref element="IC4" pad="4"/>
<contactref element="J1" pad="31"/>
</signal>
<signal name="D11">
<contactref element="IC5" pad="6"/>
<contactref element="J1" pad="32"/>
</signal>
<signal name="D9">
<contactref element="IC5" pad="4"/>
<contactref element="J1" pad="33"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="6"/>
<contactref element="J1" pad="34"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="4"/>
<contactref element="J1" pad="35"/>
</signal>
<signal name="D3">
<contactref element="IC2" pad="6"/>
<contactref element="J1" pad="36"/>
</signal>
<signal name="D1">
<contactref element="IC2" pad="4"/>
<contactref element="J1" pad="37"/>
</signal>
<signal name="W+5V">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="F1" pad="2A"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC8" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="IC9" pad="1"/>
<contactref element="IC10" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="F1" pad="2B"/>
</signal>
<signal name="D18">
<contactref element="IC8" pad="5"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="D14">
<contactref element="IC4" pad="5"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="D12">
<contactref element="IC4" pad="3"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="D8">
<contactref element="IC5" pad="3"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="N$5">
<contactref element="IC5" pad="14"/>
<contactref element="IC6" pad="23"/>
</signal>
<signal name="N$6">
<contactref element="IC5" pad="13"/>
<contactref element="IC6" pad="22"/>
</signal>
<signal name="N$8">
<contactref element="IC5" pad="12"/>
<contactref element="IC6" pad="20"/>
</signal>
<signal name="N$9">
<contactref element="IC5" pad="11"/>
<contactref element="IC6" pad="19"/>
</signal>
<signal name="N$21">
<contactref element="IC4" pad="11"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="N$22">
<contactref element="IC4" pad="12"/>
<contactref element="IC6" pad="15"/>
</signal>
<signal name="N$23">
<contactref element="IC4" pad="13"/>
<contactref element="IC6" pad="17"/>
</signal>
<signal name="N$25">
<contactref element="IC4" pad="14"/>
<contactref element="IC6" pad="18"/>
</signal>
<signal name="N$49">
<contactref element="SUPPLY_+5V" pad="P$1"/>
<contactref element="F2" pad="2A"/>
<contactref element="F2" pad="2B"/>
</signal>
<signal name="D30">
<contactref element="IC9" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
</signal>
<signal name="N$53">
</signal>
<signal name="N$54">
</signal>
<signal name="N$55">
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
<contactref element="F1" pad="1A"/>
<contactref element="J1" pad="2"/>
<contactref element="F1" pad="1B"/>
</signal>
<signal name="N$59">
<contactref element="IC8" pad="14"/>
<contactref element="IC11" pad="23"/>
</signal>
<signal name="N$60">
<contactref element="IC8" pad="13"/>
<contactref element="IC11" pad="22"/>
</signal>
<signal name="N$61">
<contactref element="IC8" pad="12"/>
<contactref element="IC11" pad="20"/>
</signal>
<signal name="N$62">
<contactref element="IC8" pad="11"/>
<contactref element="IC11" pad="19"/>
</signal>
<signal name="N$63">
<contactref element="IC7" pad="11"/>
<contactref element="IC11" pad="14"/>
</signal>
<signal name="N$64">
<contactref element="IC7" pad="12"/>
<contactref element="IC11" pad="15"/>
</signal>
<signal name="N$65">
<contactref element="IC7" pad="13"/>
<contactref element="IC11" pad="17"/>
</signal>
<signal name="N$66">
<contactref element="IC7" pad="14"/>
<contactref element="IC11" pad="18"/>
</signal>
<signal name="N$83">
<contactref element="IC10" pad="14"/>
<contactref element="IC12" pad="23"/>
</signal>
<signal name="N$84">
<contactref element="IC10" pad="13"/>
<contactref element="IC12" pad="22"/>
</signal>
<signal name="N$85">
<contactref element="IC10" pad="12"/>
<contactref element="IC12" pad="20"/>
</signal>
<signal name="N$86">
<contactref element="IC10" pad="11"/>
<contactref element="IC12" pad="19"/>
</signal>
<signal name="N$87">
<contactref element="IC9" pad="11"/>
<contactref element="IC12" pad="14"/>
</signal>
<signal name="N$88">
<contactref element="IC9" pad="12"/>
<contactref element="IC12" pad="15"/>
</signal>
<signal name="N$89">
<contactref element="IC9" pad="13"/>
<contactref element="IC12" pad="17"/>
</signal>
<signal name="N$90">
<contactref element="IC9" pad="14"/>
<contactref element="IC12" pad="18"/>
</signal>
<signal name="N$10">
<contactref element="IC3" pad="6"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC3" pad="4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="IC3" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC3" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC3" pad="7"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC3" pad="9"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="IC3" pad="10"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="IC3" pad="12"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$123">
<contactref element="BNC1" pad="CONDUCTOR"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$132">
<contactref element="BNC2" pad="CONDUCTOR"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$133">
<contactref element="BNC3" pad="CONDUCTOR"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$134">
<contactref element="BNC4" pad="CONDUCTOR"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$135">
<contactref element="BNC5" pad="CONDUCTOR"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$136">
<contactref element="BNC6" pad="CONDUCTOR"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$137">
<contactref element="BNC7" pad="CONDUCTOR"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$138">
<contactref element="BNC8" pad="CONDUCTOR"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="IC6" pad="6"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="IC6" pad="4"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="IC6" pad="3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="IC6" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="IC6" pad="7"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="IC6" pad="9"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="IC6" pad="10"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="IC6" pad="12"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$124">
<contactref element="BNC12" pad="CONDUCTOR"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$125">
<contactref element="BNC11" pad="CONDUCTOR"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$126">
<contactref element="BNC10" pad="CONDUCTOR"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$127">
<contactref element="BNC9" pad="CONDUCTOR"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$128">
<contactref element="BNC13" pad="CONDUCTOR"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$129">
<contactref element="BNC16" pad="CONDUCTOR"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$130">
<contactref element="BNC15" pad="CONDUCTOR"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$131">
<contactref element="BNC14" pad="CONDUCTOR"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$67">
<contactref element="IC11" pad="6"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$68">
<contactref element="IC11" pad="4"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="IC11" pad="3"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="IC11" pad="1"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="IC11" pad="7"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$72">
<contactref element="IC11" pad="9"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="IC11" pad="10"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="IC11" pad="12"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$115">
<contactref element="BNC17" pad="CONDUCTOR"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$116">
<contactref element="BNC18" pad="CONDUCTOR"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$117">
<contactref element="BNC19" pad="CONDUCTOR"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$118">
<contactref element="BNC20" pad="CONDUCTOR"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$119">
<contactref element="BNC24" pad="CONDUCTOR"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$120">
<contactref element="BNC23" pad="CONDUCTOR"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$121">
<contactref element="BNC22" pad="CONDUCTOR"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$122">
<contactref element="BNC21" pad="CONDUCTOR"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$91">
<contactref element="IC12" pad="6"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$92">
<contactref element="IC12" pad="4"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$93">
<contactref element="IC12" pad="3"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="N$94">
<contactref element="IC12" pad="1"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$95">
<contactref element="IC12" pad="7"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$96">
<contactref element="IC12" pad="9"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$97">
<contactref element="IC12" pad="10"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$98">
<contactref element="IC12" pad="12"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$107">
<contactref element="BNC25" pad="CONDUCTOR"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$108">
<contactref element="BNC32" pad="CONDUCTOR"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="BNC31" pad="CONDUCTOR"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$110">
<contactref element="BNC30" pad="CONDUCTOR"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$111">
<contactref element="BNC29" pad="CONDUCTOR"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$112">
<contactref element="BNC26" pad="CONDUCTOR"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$113">
<contactref element="BNC27" pad="CONDUCTOR"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$114">
<contactref element="BNC28" pad="CONDUCTOR"/>
<contactref element="R28" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
