<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.6" y2="0" width="0" layer="20"/>
<wire x1="101.6" y1="0" x2="101.6" y2="44.45" width="0" layer="20"/>
<wire x1="101.6" y1="44.45" x2="0" y2="44.45" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0" layer="20"/>
<text>B1</text>
<text>ALPS - AOM Laser</text>
<text>Power Stabilization</text>
<text>0.2mm(0.008")</text>
<text>0.2mm(0.008")</text>
<text>0.125mm(0.005")</text>
<text>0.125mm(0.005")</text>
<text>0.2mm(0.008")</text>
<text>A. Stummer  July'08</text>
<text>Following are misc parts:</text>
<text>ALPS - AOM Laser Power Stabilization</text>
<text>University of Toronto - Physics</text>
<text>J.Thywissen Labs</text>
<text>Rev: B1</text>
<text>Amp</text>
<text>PD</text>
<text>0.25A</text>
<text>A1 June'08 A.Stummer Initial design on Rev:A1 PCB.</text>
<text>A2 July'08 A.Stummer As assembled on Rev:A1 PCB.</text>
<text>B1 July'08 A.Stummer Redesign.</text>
<text>-</text>
<text>+</text>
<text>Aud</text>
</plain>
<libraries>
<library name="QuantumOptics">
<packages>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, 0.075" c-c pad spacing.  Preferred grid is 0.025".</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, use 0.0125" grid.</description>
</package>
<package name="1209">
<description>&lt;b&gt;1209 SMT&lt;/b&gt;, obscure sorta standard, taken from Lumex LED SML-LXL1209UPGC&lt;br&gt;
http://www.lumex.com/pdf/SML-LXL1209UPGC-TR.pdf</description>
</package>
<package name="EIA-A(SMA)">
<description>&lt;b&gt;EIA size A, AKA SMA&lt;/b&gt;, SMT.</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.&lt;br&gt;
http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point or wire.  Has fence (bit larger than other TP) around to allow easier soldering.</description>
</package>
<package name="PRECISION-SPR-RV8(POT)">
<description>&lt;b&gt;SPR/RV8 Pot&lt;/b&gt;, Precision Electronic Components, 0.5W single turn 1/8" shaft.&lt;br&gt;
Taken from http://www.precisionelectronics.com/MIL%20Style%20RV8%20PDF%20Download_files/MIL%20Style%20RV8.pdf</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;, on 0.025" grid.  Terminal 4 (case) is not connected here, use a polygon with the connection name as a heatsink.</description>
</package>
<package name="JUMPER-3">
<description>&lt;b&gt;Jumper 3-pin header&lt;/b&gt;, vertical SIP on 0.1" grid.</description>
</package>
<package name="CONN-BNC-AMP-TYPE1VERT">
<description>&lt;b&gt;BNC, PCB, vertical&lt;/b&gt;, Amp, e.g. isolated 5227222-6, nut 1-329631-2, lock washer 1-329632-2.&lt;br&gt;
Non-isolated use conn 5227673-1, nut 1-329631-2, lock washer 1-329632-2, shoulder washer 330620.&lt;br&gt;
http://www.tycoelectronics.com</description>
</package>
<package name="SWITCH-ESWITCH_100DP?VS2">
<description>&lt;b&gt;E-Switch 100DPxTxBxVSxxx&lt;/b&gt;, DPDT, PCB mount with metal bracket for support.&lt;br&gt;
http://spec.e-switch.com/T-D/T123032B.pdf&lt;br&gt;
http://www.e-switch.com/pdf/100.pdf</description>
</package>
<package name="3216(1206)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 1206 SMT</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="5227222-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;PD In&quot;"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="5227222-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;Control Input&quot;"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN-BNC-AMP-TYPE1VERT" value="5227222-6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;Output&quot;"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="158">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="QuantumOptics" package="PRECISION-SPR-RV8(POT)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Precision Electronics Components"/>
<attribute name="PN" value="SPRU1021S28"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="402">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH-ESWITCH_100DP?VS2" value="100DP3T2B4VS2RE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;Man/Auto&quot;"/>
<attribute name="MFG" value="E-Switch"/>
</element>
<element name="Q1" library="QuantumOptics" package="SOT23" value="MMBT3906">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="QuantumOptics" package="SOT23" value="MMBT3906">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="3.3uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Yageo"/>
<attribute name="PN" value="CC0805ZKY5V6BB335"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="QuantumOptics" package="1209" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;Unlocked&quot;"/>
<attribute name="MFG" value="Lumex"/>
<attribute name="PN" value="SML-LXL1209SIC"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="6.2nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="QuantumOptics" package="SOT23" value="2N7002TA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Zetex"/>
<attribute name="PKG" value="SOT23"/>
</element>
<element name="IC1" library="QuantumOptics" package="SOT223" value="MIC2920A-5.0WS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Micrel"/>
</element>
<element name="D1" library="QuantumOptics" package="EIA-A(SMA)" value="SMAZ16-13-F">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Diodes Inc"/>
<attribute name="RATING" value="10V/1W"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="2.49K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QuantumOptics" package="3216(1206)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="F951C106MSAAQ2"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.25A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Littlefuse"/>
<attribute name="PN" value="100056"/>
</element>
<element name="+28V" library="QuantumOptics" package="TP-0.042B" value="Keystone 5002">
<attribute name="NAME"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="QuantumOptics" package="JUMPER-3" value="">
<attribute name="NAME"/>
<attribute name="POS1" value="Amplif."/>
<attribute name="POS2" value="PD"/>
</element>
<element name="IC3" library="QuantumOptics" package="SOIC-8" value="AD8032AR(z)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$18" library="QuantumOptics" package="TITLEBLOCK_PCB" value=""/>
<element name="LIGHTPIPE1" library="QuantumOptics" package="MISC" value="PLP2-500">
<attribute name="MFG" value="Bivar inc."/>
</element>
<element name="NUT3" library="QuantumOptics" package="MISC" value="1-329631-2">
<attribute name="MFG" value="Amp"/>
</element>
<element name="WASH3" library="QuantumOptics" package="MISC" value="1-329632-2"/>
<element name="CASE1" library="QuantumOptics" package="MISC" value="1590CFL">
<attribute name="MFG" value="Hammond"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="KNOB1" library="QuantumOptics" package="MISC" value="OESA-50-4-6">
<attribute name="MFG" value="Kilo Int'l"/>
</element>
<element name="R10" library="QuantumOptics" package="PRECISION-SPR-RV8(POT)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="SPRU1031S28"/>
<attribute name="MFG" value="Precision Electronics Components"/>
<attribute name="DESC" value="&quot;Gain&quot;"/>
</element>
<element name="AUD" library="QuantumOptics" package="MISC" value="&quot;Unlocked&quot;">
<attribute name="MFG" value="Mallory"/>
<attribute name="PN" value="MSR516WR"/>
</element>
<element name="AUDIO-" library="QuantumOptics" package="TP-0.042B" value="Keystone 5002">
<attribute name="NAME"/>
</element>
<element name="AUDIO+" library="QuantumOptics" package="TP-0.042B" value="Keystone 5002">
<attribute name="NAME"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-8" value="LM2662M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="AVX"/>
<attribute name="PN" value="TCJR106M006R0500"/>
<attribute name="DESC" value="Low ESR"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="TCJR106M006R0500"/>
<attribute name="MFG" value="AVX"/>
<attribute name="DESC" value="Low ESR"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="9.31K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="Out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="402">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="402">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NUT1" library="QuantumOptics" package="MISC" value="1-329631-2">
<attribute name="MFG" value="Amp"/>
</element>
<element name="WASH1" library="QuantumOptics" package="MISC" value="1-329632-2"/>
<element name="NUT2" library="QuantumOptics" package="MISC" value="1-329631-2">
<attribute name="MFG" value="Amp"/>
</element>
<element name="WASH2" library="QuantumOptics" package="MISC" value="1-329632-2"/>
<element name="KNOB2" library="QuantumOptics" package="MISC" value="OESA-50-4-6">
<attribute name="MFG" value="Kilo Int'l"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="J2" pad="SHIELD2"/>
<contactref element="J2" pad="SHIELD1"/>
<contactref element="C9" pad="2"/>
<contactref element="J4" pad="SHIELD2"/>
<contactref element="J4" pad="SHIELD1"/>
<contactref element="R16" pad="CCW"/>
<contactref element="R12" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="D2" pad="K"/>
<contactref element="R21" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="IC1" pad="2@1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="6"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R19" pad="2"/>
<contactref element="J4" pad="CONDUCTOR"/>
</signal>
<signal name="N$2">
<contactref element="C8" pad="2"/>
<contactref element="SW1" pad="NC1"/>
<contactref element="R14" pad="2"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="+5V">
<contactref element="C9" pad="1"/>
<contactref element="R16" pad="CW"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="IC3" pad="8"/>
<contactref element="AUDIO+" pad="TP"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="C6" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R13" pad="1"/>
<contactref element="IC3" pad="6"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C8" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R19" pad="1"/>
<contactref element="SW1" pad="C1"/>
</signal>
<signal name="N$6">
<contactref element="SW1" pad="NO1"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="CONDUCTOR"/>
</signal>
<signal name="N$8">
<contactref element="R12" pad="2"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="CONDUCTOR"/>
<contactref element="R1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R18" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="SW1" pad="C2"/>
</signal>
<signal name="N$13">
<contactref element="R18" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R21" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="D1" pad="1A"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="F1" pad="2A"/>
<contactref element="D1" pad="2K"/>
</signal>
<signal name="N$19">
<contactref element="+28V" pad="TP"/>
<contactref element="F1" pad="1A"/>
</signal>
<signal name="N$24">
<contactref element="R16" pad="W"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="Q2" pad="3"/>
<contactref element="SW1" pad="NC2"/>
</signal>
<signal name="N$16">
<contactref element="Q3" pad="3"/>
<contactref element="AUDIO-" pad="TP"/>
</signal>
<signal name="N$18">
<contactref element="IC2" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="IC2" pad="4"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="-5V">
<contactref element="IC2" pad="5"/>
<contactref element="C7" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="N$27">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="IC3" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="CW"/>
<contactref element="R10" pad="W"/>
<contactref element="R9" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R10" pad="CCW"/>
<contactref element="IC3" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R4" pad="2"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="J3" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="IC3" pad="3"/>
<contactref element="R8" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
