<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="146.05" y2="0" width="0" layer="20"/>
<wire x1="146.05" y1="0" x2="146.05" y2="177.8" width="0" layer="20"/>
<wire x1="146.05" y1="177.8" x2="0" y2="177.8" width="0" layer="20"/>
<wire x1="0" y1="177.8" x2="0" y2="0" width="0" layer="20"/>
<text>+9V</text>
<text>Com</text>
<text>"PhaseoMatic 2"</text>
<text>RF Source</text>
<text>A2</text>
<text>A. Stummer, March '08</text>
<text>0.007"</text>
<text>0.02"</text>
<text>0.007"</text>
<text>0.005"</text>
<text>0.025"</text>
<text>Standard DRC rules.</text>
<text>MicroMatic II   Rev:A</text>
<text>University of Toronto</text>
<text>J. Thywissen Labs</text>
<text>Mill 24mm</text>
<text>AD9854 Eval Board</text>
<text>Reset</text>
<text>D7</text>
<text>RCM3200 Module</text>
<text>-</text>
<text>+</text>
<text>Fan</text>
<text>-</text>
<text>+</text>
<text>Fan</text>
<text>NTC</text>
<text>NTC</text>
<text>Phase</text>
<text>Drill</text>
<text>Drill</text>
<text>LED+</text>
<text>Sp1</text>
<text>Sp2</text>
<text>Link</text>
<text>Rev:A2 is Rev:A PCB with changes for next spin (Rev:B).</text>
<text>On/Off</text>
<text>Move DDS power connections - cutout?</text>
<text>Move +3.3V POL SMPS nearer to DDS and Rabbit - horizontal under RJ45?</text>
<text>To Do:</text>
<text>Much fatter trace for +3.3V to DDS and Rabbit.</text>
<hole x="76.62" y="74.21" drill="3.175"/>
<hole x="96.62" y="74.21" drill="3.175"/>
<hole x="76.62" y="94.21" drill="3.175"/>
<hole x="96.62" y="94.21" drill="3.175"/>
<hole x="26.67" y="25.4" drill="3.175"/>
<hole x="31.75" y="25.4" drill="3.175"/>
<hole x="36.83" y="25.4" drill="3.175"/>
<hole x="41.91" y="25.4" drill="3.175"/>
<hole x="110.871" y="169.164" drill="3.175"/>
<hole x="21.8694" y="169.164" drill="3.175"/>
<hole x="21.844" y="15.1384" drill="3.175"/>
<hole x="110.871" y="15.1384" drill="3.175"/>
<hole x="127.0762" y="1.3716" drill="0.508"/>
<hole x="127.0762" y="3.9116" drill="0.508"/>
<hole x="128.0922" y="6.4516" drill="0.508"/>
<hole x="130.0226" y="8.1026" drill="0.508"/>
<hole x="132.8166" y="8.9154" drill="0.508"/>
<hole x="135.8646" y="8.3312" drill="0.508"/>
<hole x="138.0236" y="6.5532" drill="0.508"/>
<hole x="139.319" y="3.9116" drill="0.508"/>
<hole x="139.2174" y="1.3716" drill="0.508"/>
<hole x="128.2192" y="177.8762" drill="0.508"/>
<hole x="130.1496" y="176.2252" drill="0.508"/>
<hole x="132.9436" y="175.4124" drill="0.508"/>
<hole x="135.9916" y="175.9966" drill="0.508"/>
<hole x="138.1506" y="177.7746" drill="0.508"/>
<hole x="60.679" y="71.561" drill="3.175"/>
<hole x="69.985" y="98.315" drill="3.175"/>
<hole x="86.6218" y="84.1848" drill="3.175"/>
</plain>
<libraries>
<library name="QuantumOptics">
<packages>
<package name="TP-0.052">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.052" hole, to fit small test point.  Has fence around to allow easier soldering.</description>
</package>
<package name="FUSE_LITTLEFUSE05200002Z">
<description>&lt;b&gt; Fuse Holder, 5x20 mm. &lt;/b&gt;Holes on 0.025" grid, for Littlefuse 520101, second best is 5200002.</description>
</package>
<package name="TO220-VERTICAL">
<description>&lt;b&gt;TO-220, mounted vertically&lt;/b&gt;</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="3216(1206)X2Y_DUAL">
<description>&lt;b&gt;X2Y dual cap in 3216 (old 1206)&lt;/b&gt;, for bypassing bipolar parts.&lt;br&gt;
Based on http://www.yageo.com/pdf/X2Y_series_12.pdf.</description>
</package>
<package name="0504">
<description>&lt;b&gt;0504 package for dual bypass cap&lt;/b&gt;, oddball EIA size used by Panasonic for dual bypass caps.&lt;br&gt;
Based on http://www.panasonic.com/industrial/components/pdf/ABK0000CE1.pdf</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, industry standard 5-pin version of the SOT-23.  On 0.025" grid except for pin 2 which is in 0.0125" grid.</description>
</package>
<package name="PANASONIC-ELL3GM(COIL)">
<description>&lt;b&gt;ELL3GM, Panasonic Coil&lt;/b&gt;, SMT, medium current and inductance.&lt;br&gt;
Based on http://www.panasonic.com/industrial/components/pdf/agb0000ce16.pdf.</description>
</package>
<package name="TI_EFD">
<description>&lt;b&gt;Power Trends (T.I.) DC-DC converter, vertical 3-pin&lt;/b&gt;, e.g. PT78NR105V.</description>
</package>
<package name="PASSIVE_0.4&quot;">
<description>&lt;b&gt;Through-hole Component&lt;/b&gt;, on 0.4" spacing with 0.052" drill, good for most passives, R's up to 0.5W.&lt;br&gt;
Has solder resist around pins to prevent solder jumpers to pours.</description>
</package>
<package name="BOURNS-3296Y">
<description>&lt;b&gt;3296Y Trimpot, Multi-turn&lt;/b&gt;, Bourns.  Staggered pins so can insert trimpot one way only.&lt;br&gt;
http://www.bourns.com/pdf/3296.pdf</description>
</package>
<package name="MSOP10">
<description>&lt;b&gt;MSOP-10&lt;/b&gt;  Use 0.5mm (0.020") grid.&lt;br&gt;
Taken from http://cache.national.com/ds/DC/ADC124S101.pdf&lt;/a&gt;</description>
</package>
<package name="EIA-7343">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, EIA-7343-xx, SMT, such as Kemet T530 case D, X or Y.&lt;br&gt;
&lt;a href="http://www.kemet.com/kemet/web/homepage/kechome.nsf/weben/33821761A656A8D9CA2570A50016091D/$file/F3102T530.pdff"&gt;
http://www.kemet.com/kemet/web/homepage/kechome.nsf/weben/33821761A656A8D9CA2570A50016091D/$file/F3102T530.pdf&lt;/a&gt;</description>
</package>
<package name="FAN25-1">
<description>&lt;b&gt;Fan, 25mm outside square&lt;/b&gt;, 20mm mounting hole pattern.&lt;br&gt;
Based on NMB 1004KL,  http://www.nmbtc.com/pdf/dcfans/1004kl.pdf&lt;br&gt;</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, 0.075" c-c pad spacing.  Preferred grid is 0.025".</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point or wire.  Has fence (bit larger than other TP) around to allow easier soldering.</description>
</package>
<package name="CASE-HAMMOND-1598HJ">
<description>&lt;b&gt;PCB to fit case, Hammond 1598H or J&lt;/b&gt;.  Plastic clamshell case.  Eight PCB short mounting posts, two top to bottom cover posts.&lt;br&gt;
Clearance PCB to inside of lid: 1598H = 28.6mm (1.129"), 1598J = (70.49mm (2.775").&lt;br&gt;
http://www.hammondmfg.com/pdf/1598H.pdf</description>
</package>
<package name="HEATSINK-4">
<description>&lt;b&gt;Heatsink, anodized aluminum, TO-220, vertical&lt;/b&gt;, unknown type but lots in stock.&lt;br&gt;
Estimated 5°/W.  Two versions: 38mm and 51mm high.  Mounts vertically on PCB, hot-glue in place.</description>
</package>
<package name="RABBIT_RCM3XXX">
<description>&lt;b&gt;Rabbit RCM3xxx Module&lt;/b&gt;, Rabbit module with ethernet. Remember connectors Sullins PPPN172AFCN (S5750-17-ND).&lt;br&gt;
&lt;i&gt;http://www.zworld.com/documentation/docs/manuals/RCM3000/UsersManual/index.htm&lt;br&gt;
http://www.zworld.com/documentation/docs/manuals/RCM3000/UsersManual/RC3000UM.pdf&lt;/i&gt;&lt;br&gt;
Connector Sullin Electronics PPPN172AFCN, &lt;i&gt;http://www.sullinselectronics.com/images/PPPNxx2AFCN-RC-10497.pdf&lt;/i&gt;</description>
</package>
<package name="AD9854-EVAL_BOARD">
<description>&lt;b&gt;AD9854 Evaluation Board&lt;/b&gt;, Analog Devices, 300MSPS DDS.&lt;br&gt;
http://www.analog.com/en/content/0,2886,770%255F843%255F11302%255F0,00.html</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;MSOP-8&lt;/b&gt;, A.K.A. RM-8.  Use 0.025" grid.</description>
</package>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1.&lt;br&gt;
Don't forget the nut 1-329631-2 and maybe the shoulder washer 330620.&lt;br&gt;
Now with new &amp; improved mtg holes compared to ...TYPE2...!&lt;br&gt;
The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
<package name="PLACEHOLDER">
<description>&lt;b&gt;Non-existant decal, a Placeholder&lt;/b&gt;, used to make a part which does not need a package but Eagle demands something, e.g. if making schematic only and don't care about PCB.&lt;br&gt;
Pins are labeled "1" through "50".</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MOD1" library="QuantumOptics" package="RABBIT_RCM3XXX" value="RCM3200 &amp; connectors">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="COMMON" library="QuantumOptics" package="TP-0.052" value="">
<attribute name="NAME"/>
</element>
<element name="+9V_IN" library="QuantumOptics" package="TP-0.052" value="">
<attribute name="NAME"/>
</element>
<element name="C22" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE_LITTLEFUSE05200002Z" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LINK_LED" library="QuantumOptics" package="TP-0.052" value="">
<attribute name="NAME"/>
</element>
<element name="LEDS+" library="QuantumOptics" package="TP-0.052" value="">
<attribute name="NAME"/>
</element>
<element name="U$44" library="QuantumOptics" package="TITLEBLOCK_PCB" value=""/>
<element name="C14" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN1" library="QuantumOptics" package="FAN25-1" value=""/>
<element name="MOD2" library="QuantumOptics" package="AD9854-EVAL_BOARD" value=""/>
<element name="U$1" library="QuantumOptics" package="CASE-HAMMOND-1598HJ" value=""/>
<element name="R30" library="QuantumOptics" package="2012(0805)" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="110">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="QuantumOptics" package="2012(0805)" value="1.33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="QuantumOptics" package="2012(0805)" value="4.42K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="QuantumOptics" package="MSOP10" value="VCA822IDGST">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="QuantumOptics" package="2012(0805)" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="110">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="QuantumOptics" package="2012(0805)" value="1.33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="QuantumOptics" package="2012(0805)" value="dns">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="QuantumOptics" package="2012(0805)" value="4.42K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="QuantumOptics" package="MSOP10" value="VCA822IDGST">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="dns">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="QuantumOptics" package="2012(0805)" value="1.33K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="QuantumOptics" package="2012(0805)" value="4.42K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="QuantumOptics" package="MSOP10" value="VCA822IDGST">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="QuantumOptics" package="3216(1206)X2Y_DUAL" value="">
<attribute name="NAME"/>
</element>
<element name="C32" library="QuantumOptics" package="3216(1206)X2Y_DUAL" value="">
<attribute name="NAME"/>
</element>
<element name="C29" library="QuantumOptics" package="3216(1206)X2Y_DUAL" value="">
<attribute name="NAME"/>
</element>
<element name="C26" library="QuantumOptics" package="0504" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="QuantumOptics" package="0504" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="QuantumOptics" package="0504" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOT23-5" value="AD8065ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="QuantumOptics" package="2012(0805)" value="4.42K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="QuantumOptics" package="2012(0805)" value="4.42K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="QuantumOptics" package="PANASONIC-ELL3GM(COIL)" value="8.2uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="QuantumOptics" package="TI_EFD" value="PT78NR105V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="QuantumOptics" package="TO220-VERTICAL" value="LM1086-5.0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="QuantumOptics" package="0504" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HS1" library="QuantumOptics" package="HEATSINK-4" value=""/>
<element name="D1" library="QuantumOptics" package="PASSIVE_0.4&quot;" value="1N5349BRLG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="QuantumOptics" package="PANASONIC-ELL3GM(COIL)" value="8.2uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="QuantumOptics" package="PANASONIC-ELL3GM(COIL)" value="8.2uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="QuantumOptics" package="PANASONIC-ELL3GM(COIL)" value="3.9uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STATUS_LED" library="QuantumOptics" package="TP-0.052" value="">
<attribute name="NAME"/>
</element>
<element name="SPARE_I/O" library="QuantumOptics" package="TP-0.052" value="">
<attribute name="NAME"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="332">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="dns">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="QuantumOptics" package="MSOP8" value="ADG619BRMZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="QuantumOptics" package="TO220-VERTICAL" value="NDP6060L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="QuantumOptics" package="BOURNS-3296Y" value="3296Y-10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="QuantumOptics" package="TO220-VERTICAL" value="NDP6060L">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="QuantumOptics" package="BOURNS-3296Y" value="3296Y-10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FAN2" library="QuantumOptics" package="FAN25-1" value=""/>
<element name="R13" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="QuantumOptics" package="MSOP8" value="ADCMP553BRM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="2.00K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="2.00K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="QuantumOptics" package="BOURNS-3296Y" value="3296Y-1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOIC-8" value="SY100ELT23LZG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="QuantumOptics" package="2012(0805)" value="82.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="QuantumOptics" package="2012(0805)" value="127">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="QuantumOptics" package="2012(0805)" value="127">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="QuantumOptics" package="2012(0805)" value="82.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="QuantumOptics" package="SOT23-5" value="74AUP1G79DBVR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="???">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DDS-I" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="NTC1A" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="NTC1B" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="FAN2+" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="FAN2-" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="NTC2A" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="NTC2B" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="FAN1+" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="DDS-Q" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="FAN1-" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="AVDD" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="DVDD" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="VCC" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="GND" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="C33" library="QuantumOptics" package="2012(0805)" value="0.1uF"/>
<element name="C34" library="QuantumOptics" package="2012(0805)" value="0.1uF"/>
<element name="IC8" library="QuantumOptics" package="PLACEHOLDER" value="78HT233VC"/>
<element name="C35" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="QuantumOptics" package="2012(0805)" value="100pF"/>
</elements>
<signals>
<signal name="D0">
<contactref element="MOD1" pad="1-14"/>
<contactref element="MOD2" pad="D0"/>
</signal>
<signal name="D1">
<contactref element="MOD1" pad="1-13"/>
<contactref element="MOD2" pad="D1"/>
</signal>
<signal name="D2">
<contactref element="MOD1" pad="1-12"/>
<contactref element="MOD2" pad="D2"/>
</signal>
<signal name="D3">
<contactref element="MOD1" pad="1-11"/>
<contactref element="MOD2" pad="D3"/>
</signal>
<signal name="D4">
<contactref element="MOD1" pad="2-9"/>
<contactref element="MOD2" pad="D4"/>
</signal>
<signal name="D5">
<contactref element="MOD1" pad="2-10"/>
<contactref element="MOD2" pad="D5"/>
</signal>
<signal name="D6">
<contactref element="MOD1" pad="2-11"/>
<contactref element="MOD2" pad="D6"/>
</signal>
<signal name="D7">
<contactref element="MOD1" pad="2-12"/>
<contactref element="MOD2" pad="D7"/>
</signal>
<signal name="A0">
<contactref element="MOD1" pad="1-23"/>
<contactref element="MOD2" pad="A0"/>
</signal>
<signal name="A1">
<contactref element="MOD1" pad="1-24"/>
<contactref element="MOD2" pad="A1"/>
</signal>
<signal name="A2">
<contactref element="MOD1" pad="1-25"/>
<contactref element="MOD2" pad="A2"/>
</signal>
<signal name="A3">
<contactref element="MOD1" pad="1-26"/>
<contactref element="MOD2" pad="A3"/>
</signal>
<signal name="A4">
<contactref element="MOD1" pad="2-23"/>
<contactref element="MOD2" pad="A4"/>
</signal>
<signal name="A5">
<contactref element="MOD1" pad="2-22"/>
<contactref element="MOD2" pad="A5"/>
</signal>
<signal name="N$1">
<contactref element="MOD1" pad="2-18"/>
<contactref element="MOD2" pad="UDCLK"/>
</signal>
<signal name="N$4">
<contactref element="MOD1" pad="2-14"/>
<contactref element="MOD2" pad="RESET"/>
</signal>
<signal name="N$6">
<contactref element="MOD1" pad="2-21"/>
<contactref element="MOD2" pad="WRBAR"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="MOD1" pad="2-20"/>
<contactref element="MOD2" pad="RDBAR"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="+3.3V">
<contactref element="MOD1" pad="2-31"/>
<contactref element="C3" pad="2"/>
<contactref element="C25" pad="+"/>
<contactref element="C23" pad="2"/>
<contactref element="MOD2" pad="PMODE"/>
<contactref element="LEDS+" pad="TP"/>
<contactref element="L4" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="IC4" pad="8"/>
<contactref element="R33" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC3" pad="7"/>
<contactref element="DVDD" pad="TP"/>
<contactref element="VCC" pad="TP"/>
</signal>
<signal name="AGND">
<contactref element="C3" pad="1"/>
<contactref element="MOD1" pad="1-1"/>
<contactref element="MOD1" pad="2-34"/>
<contactref element="MOD1" pad="2-32"/>
<contactref element="C5" pad="1"/>
<contactref element="C19" pad="-"/>
<contactref element="C20" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C17" pad="-"/>
<contactref element="C25" pad="-"/>
<contactref element="C24" pad="-"/>
<contactref element="C23" pad="1"/>
<contactref element="COMMON" pad="TP"/>
<contactref element="C14" pad="-"/>
<contactref element="R4" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="MOD2" pad="1"/>
<contactref element="MOD2" pad="2"/>
<contactref element="MOD2" pad="3"/>
<contactref element="MOD2" pad="4"/>
<contactref element="MOD2" pad="5"/>
<contactref element="MOD2" pad="6"/>
<contactref element="MOD2" pad="7"/>
<contactref element="MOD2" pad="8"/>
<contactref element="MOD2" pad="9"/>
<contactref element="MOD2" pad="10"/>
<contactref element="MOD2" pad="11"/>
<contactref element="MOD2" pad="12"/>
<contactref element="MOD2" pad="13"/>
<contactref element="MOD2" pad="14"/>
<contactref element="MOD2" pad="15"/>
<contactref element="MOD2" pad="16"/>
<contactref element="MOD2" pad="17"/>
<contactref element="MOD2" pad="18"/>
<contactref element="MOD2" pad="19"/>
<contactref element="MOD2" pad="20"/>
<contactref element="R27" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R48" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="J6" pad="SHIELD2"/>
<contactref element="J5" pad="SHIELD2"/>
<contactref element="U1" pad="10"/>
<contactref element="R28" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="R49" pad="1"/>
<contactref element="U2" pad="10"/>
<contactref element="R44" pad="1"/>
<contactref element="J7" pad="SHIELD2"/>
<contactref element="J8" pad="SHIELD2"/>
<contactref element="R29" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="U3" pad="10"/>
<contactref element="R47" pad="1"/>
<contactref element="J10" pad="SHIELD2"/>
<contactref element="C28" pad="COM2"/>
<contactref element="C28" pad="COM1"/>
<contactref element="C32" pad="COM2"/>
<contactref element="C32" pad="COM1"/>
<contactref element="C29" pad="COM2"/>
<contactref element="C29" pad="COM1"/>
<contactref element="C26" pad="2A"/>
<contactref element="C26" pad="1A"/>
<contactref element="C30" pad="2A"/>
<contactref element="C30" pad="1A"/>
<contactref element="C27" pad="2A"/>
<contactref element="C27" pad="1A"/>
<contactref element="R17" pad="1"/>
<contactref element="J9" pad="SHIELD2"/>
<contactref element="R46" pad="1"/>
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J2" pad="SHIELD2"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C31" pad="2A"/>
<contactref element="C31" pad="1A"/>
<contactref element="C9" pad="-"/>
<contactref element="D1" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC6" pad="COM"/>
<contactref element="C15" pad="+"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="CCW"/>
<contactref element="Q2" pad="3"/>
<contactref element="R2" pad="CCW"/>
<contactref element="C8" pad="1"/>
<contactref element="IC3" pad="8"/>
<contactref element="R20" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R14" pad="CCW"/>
<contactref element="C10" pad="1"/>
<contactref element="IC4" pad="5"/>
<contactref element="R34" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="IC7" pad="3"/>
<contactref element="J3" pad="SHIELD2"/>
<contactref element="J4" pad="SHIELD2"/>
<contactref element="GND" pad="TP"/>
<contactref element="J3" pad="SHIELD1"/>
<contactref element="J4" pad="SHIELD1"/>
<contactref element="J5" pad="SHIELD1"/>
<contactref element="J6" pad="SHIELD1"/>
<contactref element="J7" pad="SHIELD1"/>
<contactref element="J8" pad="SHIELD1"/>
<contactref element="J9" pad="SHIELD1"/>
<contactref element="J10" pad="SHIELD1"/>
<contactref element="IC8" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="C5" pad="2"/>
<contactref element="C19" pad="+"/>
<contactref element="C20" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C26" pad="2B"/>
<contactref element="C30" pad="2B"/>
<contactref element="C27" pad="2B"/>
<contactref element="IC2" pad="5"/>
<contactref element="C31" pad="2B"/>
<contactref element="L2" pad="1"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="MOD1" pad="2-15"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="MOD1" pad="2-13"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="J2" pad="CONDUCTOR"/>
</signal>
<signal name="+3.3VA">
<contactref element="C24" pad="+"/>
<contactref element="C22" pad="2"/>
<contactref element="L3" pad="1"/>
<contactref element="AVDD" pad="TP"/>
</signal>
<signal name="N$70">
<contactref element="C17" pad="+"/>
<contactref element="C18" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$72">
<contactref element="MOD1" pad="1-33"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="LINK_LED" pad="TP"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$64">
</signal>
<signal name="N$74">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$80">
</signal>
<signal name="N$66">
<contactref element="C21" pad="2"/>
<contactref element="L3" pad="2"/>
<contactref element="L4" pad="2"/>
<contactref element="IC8" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R30" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="R30" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="R27" pad="2"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="R21" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="R38" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R38" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="C35" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="R48" pad="2"/>
<contactref element="R43" pad="2"/>
<contactref element="J6" pad="CONDUCTOR"/>
</signal>
<signal name="N$18">
<contactref element="R50" pad="1"/>
<contactref element="R42" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R50" pad="2"/>
<contactref element="J5" pad="CONDUCTOR"/>
</signal>
<signal name="N$20">
<contactref element="R31" pad="2"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="R31" pad="1"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="R28" pad="2"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="N$23">
<contactref element="R22" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$25">
<contactref element="R39" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R39" pad="2"/>
<contactref element="U2" pad="9"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R49" pad="2"/>
<contactref element="R45" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="C36" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R51" pad="1"/>
<contactref element="R44" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R51" pad="2"/>
<contactref element="J7" pad="CONDUCTOR"/>
</signal>
<signal name="N$30">
<contactref element="R32" pad="2"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="N$31">
<contactref element="R32" pad="1"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$32">
<contactref element="R29" pad="2"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="N$33">
<contactref element="R23" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$35">
<contactref element="R40" pad="1"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R40" pad="2"/>
<contactref element="U3" pad="9"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R52" pad="1"/>
<contactref element="R47" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="R52" pad="2"/>
<contactref element="J10" pad="CONDUCTOR"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="1"/>
<contactref element="C34" pad="1"/>
</signal>
<signal name="-5V">
<contactref element="C28" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="8"/>
<contactref element="U3" pad="8"/>
<contactref element="C26" pad="1B"/>
<contactref element="C30" pad="1B"/>
<contactref element="C27" pad="1B"/>
<contactref element="IC2" pad="2"/>
<contactref element="C31" pad="1B"/>
<contactref element="IC6" pad="OUT"/>
<contactref element="C15" pad="-"/>
<contactref element="IC1" pad="7"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="IC2" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="R18" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="IC2" pad="3"/>
<contactref element="R17" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="R15" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$43">
<contactref element="J9" pad="CONDUCTOR"/>
<contactref element="R46" pad="2"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="QUADRANT">
<contactref element="R37" pad="1"/>
<contactref element="MOD1" pad="2-16"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$42">
<contactref element="F1" pad="1"/>
<contactref element="+9V_IN" pad="TP"/>
</signal>
<signal name="N$44">
<contactref element="F1" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="C9" pad="+"/>
<contactref element="D1" pad="2"/>
<contactref element="IC6" pad="IN"/>
<contactref element="IC8" pad="3"/>
</signal>
<signal name="N$45">
<contactref element="STATUS_LED" pad="TP"/>
<contactref element="R9" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="MOD1" pad="1-27"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="MOD1" pad="1-28"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="SPARE_I/O" pad="TP"/>
<contactref element="R10" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="J1" pad="CONDUCTOR"/>
</signal>
<signal name="N$49">
<contactref element="Q1" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="FAN1-" pad="TP"/>
</signal>
<signal name="N$50">
<contactref element="R1" pad="W"/>
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="CW"/>
<contactref element="NTC1B" pad="TP"/>
</signal>
<signal name="N$51">
<contactref element="Q2" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="FAN2-" pad="TP"/>
</signal>
<signal name="N$52">
<contactref element="R2" pad="W"/>
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="CW"/>
<contactref element="NTC2B" pad="TP"/>
</signal>
<signal name="+5VF">
<contactref element="C1" pad="+"/>
<contactref element="C2" pad="+"/>
<contactref element="C14" pad="+"/>
<contactref element="L1" pad="2"/>
<contactref element="NTC1A" pad="TP"/>
<contactref element="FAN2+" pad="TP"/>
<contactref element="NTC2A" pad="TP"/>
<contactref element="FAN1+" pad="TP"/>
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$78">
</signal>
<signal name="N$60">
<contactref element="IC3" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="R14" pad="W"/>
<contactref element="R14" pad="CW"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R21" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C33" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="R20" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$68">
<contactref element="R34" pad="2"/>
<contactref element="R33" pad="1"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$69">
<contactref element="R35" pad="1"/>
<contactref element="R36" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$61">
<contactref element="IC4" pad="6"/>
<contactref element="IC7" pad="2"/>
<contactref element="C37" pad="2"/>
</signal>
<signal name="N$63">
<contactref element="IC7" pad="4"/>
<contactref element="J4" pad="CONDUCTOR"/>
</signal>
<signal name="N$67">
<contactref element="IC7" pad="1"/>
<contactref element="J3" pad="CONDUCTOR"/>
</signal>
<signal name="N$53">
</signal>
<signal name="N$54">
<contactref element="DDS-I" pad="TP"/>
<contactref element="C33" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="DDS-Q" pad="TP"/>
<contactref element="C34" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="R43" pad="1"/>
<contactref element="C35" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="J8" pad="CONDUCTOR"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="MOD1" pad="2-17"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
