<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="55" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="122" y2="0" width="0" layer="20"/>
<wire x1="122" y1="0" x2="122" y2="55" width="0" layer="20"/>
<wire x1="122" y1="55" x2="0" y2="55" width="0" layer="20"/>
<text>BEC AC Line Sync   Rev: B</text>
<text>University of Toronto - Physics</text>
<text>Æ. Steinberg Labs</text>
<text>BEC AC Line Sync</text>
<text>A.Steinberg Labs</text>
<text>B.1</text>
<text>A. Stummer  Oct 2009</text>
<text>0.18mm</text>
<text>0.18mm</text>
<text>0.18mm</text>
<text>0.25mm</text>
<text>0.125mm</text>
<text>Rev:A   23 Oct 2009  A.S.  As sent to board house, not made.</text>
<text>Rev:B.1  27 Oct 2009  A.S.  Revised dimensions, board assembled.</text>
<hole x="22.81" y="26" drill="3.175"/>
<hole x="99.29" y="25.99" drill="3.175"/>
</plain>
<libraries>
<library name="QuantumOptics">
<packages>
<package name="TSSOP-14">
<description>&lt;b&gt;TSSOP-14&lt;/b&gt;, pins 0.65mm c-c spacing, nominal 6.4mm rows.</description>
</package>
<package name="SOIC-14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, 0.075" c-c pad spacing.  Preferred grid is 0.025".</description>
</package>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1.&lt;br&gt;
Don't forget the nut 1-329631-2 and maybe the shoulder washer 330620.&lt;br&gt;
Now with new &amp; improved mtg holes compared to ...TYPE2...!&lt;br&gt;
The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire.  Has fence (bit larger than other TP) around to allow easier soldering.</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.&lt;br&gt;
http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="EIA-B(SMB)">
<description>&lt;b&gt;R, C, L or D&lt;/b&gt;, EIA size B, A.K.A. SMB.</description>
</package>
<package name="CAP:NICHICON_UPW-8MM">
<description>&lt;b&gt;Capacitor, Nichicon UPW-series 8mm dia x 3.5mm pin c-c&lt;/b&gt;, through-hole.  http://products.nichicon.co.jp/en/pdf/XJA043/e-pw.pdf</description>
</package>
<package name="TO220-VERTICAL">
<description>&lt;b&gt;TO-220, mounted vertically&lt;/b&gt;</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="CSX750(CITIZEN_OSC)">
<description>&lt;b&gt;ASVxxx from Abracon&lt;/b&gt;, formerly CSX750 by Citizen, +3.3V or +5V, 1MHZ to 133MHz.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC4" library="QuantumOptics" package="TSSOP-14" value="CD4085BPWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="QuantumOptics" package="SOIC-14" value="CD4013BM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="5227661-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;Clock Out&quot;"/>
<attribute name="MFG" value="Tyco"/>
</element>
<element name="J5" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="5227661-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;60Hz Out&quot;"/>
<attribute name="MFG" value="Tyco"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-8" value="LT1720CS8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="5227661-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;Clock I/O&quot;"/>
<attribute name="MFG" value="Tyco"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="5227661-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;/Sync&quot;"/>
<attribute name="MFG" value="Tyco"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="2.49K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="5227661-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DESC" value="&quot;Top Sync&quot;"/>
<attribute name="MFG" value="Tyco"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="2.49K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="9VAC" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="COM" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.25A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="QuantumOptics" package="EIA-B(SMB)" value="MBRS130LT3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="QuantumOptics" package="CAP:NICHICON_UPW-8MM" value="220uF/25V">
<attribute name="NAME"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="UPW1E221MPD"/>
</element>
<element name="IC1" library="QuantumOptics" package="TO220-VERTICAL" value="LM1086CT-5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$20" library="QuantumOptics" package="TITLEBLOCK_PCB" value=""/>
<element name="IC5" library="QuantumOptics" package="CSX750(CITIZEN_OSC)" value="ESC-2100A-020"/>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="0.1uF"/>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF"/>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="10K"/>
</elements>
<signals>
<signal name="AGND">
<contactref element="IC3" pad="7"/>
<contactref element="IC4" pad="7"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC4" pad="11"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC3" pad="8"/>
<contactref element="J4" pad="SHIELD2"/>
<contactref element="J4" pad="SHIELD1"/>
<contactref element="J5" pad="SHIELD2"/>
<contactref element="J5" pad="SHIELD1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="J2" pad="SHIELD2"/>
<contactref element="J2" pad="SHIELD1"/>
<contactref element="R4" pad="1"/>
<contactref element="J3" pad="SHIELD2"/>
<contactref element="J3" pad="SHIELD1"/>
<contactref element="IC2" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="COM" pad="TP"/>
<contactref element="C1" pad="-"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="IC3" pad="14"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="IC4" pad="14"/>
<contactref element="R7" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC3" pad="9"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC4" pad="1"/>
<contactref element="IC4" pad="12"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="R9" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="J2" pad="CONDUCTOR"/>
</signal>
<signal name="N$3">
<contactref element="IC4" pad="13"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="N$5">
<contactref element="IC3" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="J3" pad="CONDUCTOR"/>
</signal>
<signal name="N$7">
<contactref element="R10" pad="2"/>
<contactref element="J4" pad="CONDUCTOR"/>
</signal>
<signal name="N$8">
<contactref element="IC3" pad="11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC4" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC3" pad="5"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="1"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="2"/>
<contactref element="J5" pad="CONDUCTOR"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="CONDUCTOR"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R1" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="F1" pad="2A"/>
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="A-"/>
</signal>
<signal name="N$18">
<contactref element="F1" pad="1A"/>
<contactref element="9VAC" pad="TP"/>
</signal>
<signal name="N$19">
<contactref element="C1" pad="+"/>
<contactref element="D1" pad="K+"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="R12" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
