<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="191.5" y1="151.25" x2="0" y2="151.25" width="0" layer="20"/>
<wire x1="0" y1="151.25" x2="0" y2="0" width="0" layer="20"/>
<wire x1="191.5" y1="0" x2="191.5" y2="151.25" width="0" layer="20"/>
<wire x1="0" y1="0" x2="191.5" y2="0" width="0" layer="20"/>
<text>1 2</text>
<text>General Purpose DDS</text>
<text>B1</text>
<text>A. Stummer May'11</text>
<text>0.18mm</text>
<text>0.36mm</text>
<text>0.18mm</text>
<text>0.1mm</text>
<text>0.25mm</text>
<text>General Purpose DDS  Rev:B  University of Toronto  J. Thywissen Labs</text>
<text>58</text>
<text>0</text>
<text>0</text>
<text>198</text>
<text>Hammond 1598D Faceplate (front view, 1.5mm [0.062"] Al)</text>
<text>58</text>
<text>29.1</text>
<text>0</text>
<text>0</text>
<text>20</text>
<text>40</text>
<text>60</text>
<text>80</text>
<text>100</text>
<text>120</text>
<text>198</text>
<text>0.5"</text>
<text>7 pl</text>
<text>Hammond 1598D Backplate (back view, 1.5mm [0.062"] Al)</text>
<text>164</text>
<text>182.5</text>
<text>30</text>
<text>111</text>
<text>183</text>
<text>15.75</text>
<text>42.25</text>
<text>140</text>
<text>0.25"</text>
<text>44</text>
<text>6.2</text>
<text>47</text>
<hole x="20.715" y="128.095" drill="3.175"/>
<hole x="170.717" y="128.105" drill="3.175"/>
<hole x="170.717" y="7.937" drill="3.175"/>
<hole x="70.707" y="7.957" drill="3.175"/>
<text>Rev B1:</text>
<text>Changed ground on OCXO trimpot.</text>
<text>Fixed mirrored OCXO footprint.</text>
<text>Moved Rabbit left 4mm.</text>
<hole x="64.2272" y="69.3768" drill="3.8608"/>
<hole x="76.946" y="69.4022" drill="3.8608"/>
<hole x="76.946" y="56.7088" drill="3.8608"/>
<hole x="64.2272" y="56.7088" drill="3.8608"/>
<text>0.25"</text>
<text>0.25"</text>
<text>ON NEXT SPIN:</text>
<text>Move TB1-2 power connector pins 5-10mm closer to BNCs so can wire in connector.</text>
<text>AD9910 heatsink cutout is too small, make 5-10mm larger.</text>
<text>Plastic shim, 7.5mmH x 1cm sq, 2 pl</text>
<text>Cmd Seq</text>
<text>Running</text>
<text>Ramping</text>
<text>Update</text>
<text>Spare 2</text>
<text>Spare 1</text>
<text>Trigger in</text>
<text>7/16"</text>
</plain>
<libraries>
<library name="QuantumOptics">
<packages>
<package name="CONN-2X5-BLASTER">
<description>&lt;b&gt;Connector, 2 rows of 5 for ByteBlaster, USBBlaster or MasterBlaster&lt;/b&gt;, on 0.1" grid, pins numbering zig-zags top-left to bottom-right.</description>
</package>
<package name="SOIC-8@1">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="HEATSINK:274-2AB(WAKEFIELD,25C/W)">
<description>&lt;b&gt;Heatsink&lt;/b&gt;, Wakefield #274-2AB, through-hole for TO-220 or just on a plane, 0.5"H, 25°/W&lt;br&gt;
Use 0.15" (3.8mm) hole, has 0.52"x0.75" footprint&lt;br&gt;
Can also fit 274-1AB, 0.375"H, 28°/W.&lt;br&gt;
http://www.wakefield.com/pdf/Low%20Power.pdf</description>
</package>
<package name="1608(0603)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0603 SMT</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, 0.075" c-c pad spacing.  Preferred grid is 0.025".</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire.  Has fence (bit larger than other TP) around to allow easier soldering.</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="ZENER:DFLZ_V_(1W)">
<description>&lt;b&gt;DFLZxVx, zener&lt;/b&gt;, Diodes Inc., 5.1V to 39V, 1W.&lt;br&gt;
http://www.diodes.com/datasheets/ds18010.pdf</description>
</package>
<package name="DISPLAY:3WIRE">
<description>&lt;b&gt;LCD display module&lt;/b&gt;, serial (RS232, I2C or SPI), actually just the connector.  e.g. Newhaven Display Intl NHD-0216B3Z-FL-GBW&lt;br&gt;
http://www.newhavendisplay.com/pdf/nhd-0216b3z-fl-gbw.pdf</description>
</package>
<package name="CAP:NIPPONCHEM_E61">
<description>&lt;b&gt;Capacitor, polarized, Nippon Chemi-con Corp, E61 package&lt;/b&gt;.  Round SMT with plastic standoff.  Bit awkward to install.&lt;br&gt;
http://www.chemi-con.com/files/PXE.pdf</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="SOT353">
<description>&lt;b&gt;SOT-353&lt;/b&gt;, 5-pin, same as SC-88A and SC-70.&lt;br&gt;
http://www.onsemi.com/pub_link/Collateral/NL17SZ125-D.PDF</description>
</package>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1.&lt;br&gt;
Don't forget the nut 1-329631-2 and maybe the shoulder washer 330620.&lt;br&gt;
Now with new &amp; improved mtg holes compared to ...TYPE2...!&lt;br&gt;
The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
<package name="CSX750(CITIZEN_OSC)">
<description>&lt;b&gt;CSX750 Oscillators&lt;/b&gt;, Citizen, +3.3V or +5V, 1MHZ to 133MHz.  Uses 0.025" grid.&lt;br&gt;
http://www.citizencrystal.com/images/pdf/os-csx750f.pdf</description>
</package>
<package name="SOT223(C)">
<description>&lt;b&gt;SOT-223&lt;/b&gt;, no centre pin, uses tab.</description>
</package>
<package name="EIA-7343">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, EIA-7343-xx, SMT, such as Kemet T530 case D, X or Y.&lt;br&gt;
&lt;a href="http://www.kemet.com/kemet/web/homepage/kechome.nsf/weben/33821761A656A8D9CA2570A50016091D/$file/F3102T530.pdff"&gt;
http://www.kemet.com/kemet/web/homepage/kechome.nsf/weben/33821761A656A8D9CA2570A50016091D/$file/F3102T530.pdf&lt;/a&gt;</description>
</package>
<package name="CONN:SMA2">
<description>&lt;b&gt;SMA PCB, straight&lt;/b&gt;,e.g. Tyco 5-1814832-1, 1.6mm holes</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, industry standard 5-pin version of the SOT-23.  On 0.025" grid except for pin 2 which is in 0.0125" grid.</description>
</package>
<package name="CASE:HAMMOND_1598D">
<description>&lt;b&gt;Case, Hammond 1598D&lt;/b&gt;, case is 206mmW x 180D x 64H, http://www.hammondmfg.com/pdf/1598D.pdf.&lt;br&gt;
Has 0.5mm space between PCB and inside of front and back plates, larger gap at sides.</description>
</package>
<package name="PANASONIC_EXB-V8V(QUAD-R-PACK)">
<description>&lt;b&gt;EXB-V8V-vvvJV&lt;/b&gt;, Panasonic quad resistor pack, each R is 0603, 5%,&lt;br&gt;
where value "vvv" is two significant digits and decade multiplier.&lt;br&gt;
http://www.panasonic.com/industrial/components/pdf/aoc0000ce1.pdf</description>
</package>
<package name="SWITCH:SPDT-DIP(COPAL)">
<description>&lt;b&gt;DIP (SMT) switch, SPDT&lt;/b&gt;, Copal CJS-1200, fits A1 (J-lead) and B1 (gullwing), http://media.digikey.com/pdf/Data%20Sheets/COPAL%20Electronics%20PDFs/CJS.pdf?cshift_ck=null&amp;client_id=5210&amp;cshift_ck=null&amp;client_id=5210</description>
</package>
<package name="BOURNS:3296Y">
<description>&lt;b&gt;3296Y (multi, top adj), 3296Z (multi, side adj) or 3386X/H (1-turn, top) Trimpot&lt;/b&gt;, Bourns.  Staggered pins so can insert trimpot one way only.  http://www.bourns.com/pdf/3296.pdf</description>
</package>
<package name="RABBIT_RCM42XX(THRU)">
<description>&lt;b&gt;RCM42xx Rabbit module&lt;/b&gt;, really just a 1x25 1.27mm connector such as Samtec SFM(L)-125-01-S-D (if no -125- use -130 30-position and cut short).&lt;br&gt;
Location of pin 1 has been verified on a unit.</description>
</package>
<package name="EQFP144(TQFP_WITH_GROUND_PAD)">
<description>&lt;b&gt;EQFP-144&lt;/b&gt;, Enhanced QFP, similar to TQFP-144 with a ground pad but bit bigger, Altera. &lt;br&gt;
Use 0.5mm grid (2.5m").  Use 0.2mm (8m") max traces and space.&lt;br&gt;
http://www.altera.com/literature/ds/144-EQFP.pdf</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="TO263">
<description>&lt;b&gt;TO-263&lt;/b&gt;, SMT power.  Uses 0.1" grid.  Add large polygon for case connection.  Ignore DRC restrict errors.  e.g. http://cache.national.com/ds/LM/LM1086.pdf</description>
</package>
<package name="OSCILLATOR:AOCJY(ABRACON-OCXO)">
<description>&lt;b&gt;OCXO, Abracon AOCJY series&lt;/b&gt;, ±5ppb/°, +3.3V.</description>
</package>
<package name="DDS:AD9910,EVALBOARD">
<description>&lt;b&gt;AD9910 DDS Eval Board, Rev:G&lt;/b&gt;, Analog Devices 1GSPS 14-bit 3.3V, can ramp to fixed stop frequency.  This is top view with eval below motherboard.  http://www.analog.com/en/rfif-components/direct-digital-synthesis-dds/ad9910/products/product.html.  
Note that the schematic and user manual disagree on pin numbering for TB1-2 (power) but that the physical locations have been confirmed with the picture of the PCB in the user manual.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="QuantumOptics" package="CONN-2X5-BLASTER" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="R2" library="QuantumOptics" package="PANASONIC_EXB-V8V(QUAD-R-PACK)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="QuantumOptics" package="PANASONIC_EXB-V8V(QUAD-R-PACK)" value="1K">
<attribute name="NAME"/>
</element>
<element name="C35" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="QuantumOptics" package="EQFP144(TQFP_WITH_GROUND_PAD)" value="EP3C10E144C7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-8@1" value="EPCS4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="QuantumOptics" package="1608(0603)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DIS1" library="QuantumOptics" package="DISPLAY:3WIRE" value="NHD-0216B3Z-FL-GBW">
<attribute name="NAME"/>
<attribute name="MFG" value="Newhaven Display Intl."/>
</element>
<element name="C36" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Keystone"/>
<attribute name="PN" value="5002K"/>
</element>
<element name="TP1" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Keystone"/>
<attribute name="PN" value="5002K"/>
</element>
<element name="MOD1" library="QuantumOptics" package="RABBIT_RCM42XX(THRU)" value="RCM4200">
<attribute name="NAME"/>
<attribute name="THROUGH_CONN" value="Samtec SFML-125-01-S-D"/>
<attribute name="ALT-THRU-CONN" value="Samtec SFML-125-T1-S-D"/>
</element>
<element name="CONF_DONE" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Keystone"/>
<attribute name="PN" value="5002K"/>
</element>
<element name="IC1" library="QuantumOptics" package="CSX750(CITIZEN_OSC)" value="100MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Abracon"/>
<attribute name="PN" value="ASV-100.000MHZ-E-C-T"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="QuantumOptics" package="SOT223(C)" value="LT3080EST">
<attribute name="NAME"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="121K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="IC4" library="QuantumOptics" package="SOT223(C)" value="LT3080EST">
<attribute name="NAME"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="249K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DDS1" library="QuantumOptics" package="DDS:AD9910,EVALBOARD" value="">
<attribute name="P1" value="P1: Samtec SSW-120-01-G-D"/>
<attribute name="TB1-2" value="TB1,2: Pheonix 1792032"/>
<attribute name="U569" value="U5,6,9: Samtec SSW-110-01-G-D"/>
<attribute name="U8" value="U8: Samtec SSW-108-01-G-D"/>
</element>
<element name="+5V_IN" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="RETURN" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="C47" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="2A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Cooper"/>
<attribute name="PN" value="BK/GMC-2-R"/>
</element>
<element name="D1" library="QuantumOptics" package="ZENER:DFLZ_V_(1W)" value="DFLZ5V6-7">
<attribute name="NAME"/>
</element>
<element name="IC15" library="QuantumOptics" package="TO263" value="LM1086CS-3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C57" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C48" library="QuantumOptics" package="EIA-7343" value="10uF">
<attribute name="NAME"/>
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700V106M016ATE045"/>
</element>
<element name="HS2" library="QuantumOptics" package="HEATSINK:274-2AB(WAKEFIELD,25C/W)" value="274-2AB">
<attribute name="NAME"/>
</element>
<element name="HS1" library="QuantumOptics" package="HEATSINK:274-2AB(WAKEFIELD,25C/W)" value="274-2AB">
<attribute name="NAME"/>
</element>
<element name="C52" library="QuantumOptics" package="EIA-7343" value="10uF">
<attribute name="NAME"/>
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700V106M016ATE045"/>
</element>
<element name="COAX" library="QuantumOptics" package="MISC" value="SMA-SMA coax">
<attribute name="NAME"/>
<attribute name="MFG" value="Amphenol"/>
<attribute name="PN" value="135103-02-06.00"/>
</element>
<element name="IC6" library="QuantumOptics" package="SOT223(C)" value="LT3080EST">
<attribute name="NAME"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="182K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="QuantumOptics" package="CAP:NIPPONCHEM_E61" value="39uF">
<attribute name="NAME"/>
<attribute name="MFG" value="Nippon Chemi"/>
<attribute name="PN" value="APXE160ARA390ME61G"/>
</element>
<element name="C37" library="QuantumOptics" package="2012(0805)" value="12pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="QuantumOptics" package="SOT353" value="NL17SZ125DFT2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="227677-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC10" library="QuantumOptics" package="SOT353" value="NL17SZ125DFT2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="227677-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC12" library="QuantumOptics" package="SOT353" value="NL17SZ125DFT2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="227677-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="IC13" library="QuantumOptics" package="SOT353" value="NL17SZ125DFT2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="227677-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="IC11" library="QuantumOptics" package="SOT353" value="NL17SZ125DFT2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="227677-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC14" library="QuantumOptics" package="SOT353" value="NL17SZ125DFT2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="227677-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Amp"/>
</element>
<element name="OSC1" library="QuantumOptics" package="OSCILLATOR:AOCJY(ABRACON-OCXO)" value="AOCJY-20.000MHZ-E">
<attribute name="NAME"/>
</element>
<element name="C46" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="QuantumOptics" package="BOURNS:3296Y" value="3296Z-10K">
<attribute name="NAME"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN:SMA2" value="Amphenol 132134">
<attribute name="NAME"/>
</element>
<element name="COAX1" library="QuantumOptics" package="MISC" value="SMA plug-SMA bulkhead 30cm">
<attribute name="NAME"/>
<attribute name="MFG" value="Amphenol"/>
<attribute name="PN" value="135110-01-12.00"/>
</element>
<element name="C44" library="QuantumOptics" package="CAP:NIPPONCHEM_E61" value="39uF">
<attribute name="NAME"/>
<attribute name="MFG" value="Nippon Chemi"/>
<attribute name="PN" value="APXE160ARA390ME61G"/>
</element>
<element name="C42" library="QuantumOptics" package="CAP:NIPPONCHEM_E61" value="39uF">
<attribute name="NAME"/>
<attribute name="MFG" value="Nippon Chemi"/>
<attribute name="PN" value="APXE160ARA390ME61G"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Yageo"/>
<attribute name="PN" value="PT0805FR-7W0R1L"/>
</element>
<element name="IC7" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="12.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="121">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OCXO+" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="OCXO-" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="LED" library="QuantumOptics" package="MISC" value="OCXO LED">
<attribute name="NAME"/>
<attribute name="MFG" value="Dialight"/>
<attribute name="PN" value="558-0102-007F"/>
</element>
<element name="U$21" library="QuantumOptics" package="CASE:HAMMOND_1598D" value=""/>
<element name="HTSNK" library="QuantumOptics" package="MISC" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Advanced Thermal"/>
<attribute name="PN" value="ATS-5417W-C2-R0"/>
</element>
<element name="U5" library="QuantumOptics" package="MISC" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Samtec"/>
<attribute name="PN" value="TSW-110-08-G-D"/>
</element>
<element name="P1" library="QuantumOptics" package="MISC" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Samtec"/>
<attribute name="PN" value="TSW-120-23-S-D"/>
</element>
<element name="U6" library="QuantumOptics" package="MISC" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Samtec"/>
<attribute name="PN" value="TSW-110-08-G-D"/>
</element>
<element name="U9" library="QuantumOptics" package="MISC" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Samtec"/>
<attribute name="PN" value="TSW-110-08-G-D"/>
</element>
<element name="CASE" library="QuantumOptics" package="MISC" value="1598D">
<attribute name="NAME"/>
<attribute name="MFG" value="Hammond"/>
<attribute name="PN" value=""/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
<attribute name="DESC" value="50 Ohm"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
<attribute name="DESC" value="50 Ohm"/>
</element>
<element name="SW3" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
<attribute name="DESC" value="50 Ohm"/>
</element>
<element name="IC8" library="QuantumOptics" package="TO263" value="LM1086CS-3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$20" library="QuantumOptics" package="TITLEBLOCK_PCB" value="">
<attribute name="LAST_DATE_TIME"/>
<attribute name="DRAWING_NAME"/>
</element>
<element name="PWR" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="SL Power"/>
<attribute name="PN" value="MENB1010A0503B01"/>
<attribute name="NAME"/>
</element>
<element name="SWTCH" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="C&amp;K"/>
<attribute name="PN" value="T102SHZQE"/>
<attribute name="NAME"/>
</element>
<element name="GROMT" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Richco Plastics"/>
<attribute name="PN" value="SRB-F-7"/>
<attribute name="NAME"/>
</element>
<element name="CLIP1" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Littlefuse"/>
<attribute name="PN" value="100056"/>
<attribute name="NAME"/>
</element>
<element name="CLIP2" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Littlefuse"/>
<attribute name="PN" value="100056"/>
<attribute name="NAME"/>
</element>
<element name="SHIMS" library="QuantumOptics" package="MISC" value="See notes below.">
<attribute name="PN" value=""/>
</element>
</elements>
<signals>
<signal name="+3.3V">
<contactref element="IC5" pad="17"/>
<contactref element="IC5" pad="26"/>
<contactref element="IC5" pad="40"/>
<contactref element="IC5" pad="47"/>
<contactref element="IC5" pad="56"/>
<contactref element="IC5" pad="62"/>
<contactref element="IC5" pad="81"/>
<contactref element="IC5" pad="93"/>
<contactref element="IC5" pad="117"/>
<contactref element="IC5" pad="122"/>
<contactref element="IC5" pad="130"/>
<contactref element="IC5" pad="139"/>
<contactref element="J1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="R2" pad="3B"/>
<contactref element="R2" pad="1B"/>
<contactref element="R2" pad="4B"/>
<contactref element="C3" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="8"/>
<contactref element="R1" pad="1A"/>
<contactref element="R1" pad="2A"/>
<contactref element="C35" pad="1"/>
<contactref element="MOD1" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="DDS1" pad="U5.17"/>
<contactref element="DDS1" pad="TB1.2"/>
<contactref element="DDS1" pad="TB1.4"/>
<contactref element="DDS1" pad="TB2.3"/>
<contactref element="IC15" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="IC6" pad="3"/>
<contactref element="C38" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="IC9" pad="5"/>
<contactref element="C50" pad="1"/>
<contactref element="IC10" pad="5"/>
<contactref element="C51" pad="1"/>
<contactref element="IC11" pad="5"/>
</signal>
<signal name="+2.5V">
<contactref element="IC5" pad="35"/>
<contactref element="IC5" pad="75"/>
<contactref element="IC5" pad="96"/>
<contactref element="IC5" pad="107"/>
<contactref element="IC4" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="+1.2V">
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="29"/>
<contactref element="IC5" pad="37"/>
<contactref element="IC5" pad="45"/>
<contactref element="IC5" pad="61"/>
<contactref element="IC5" pad="73"/>
<contactref element="IC5" pad="78"/>
<contactref element="IC5" pad="102"/>
<contactref element="IC5" pad="109"/>
<contactref element="IC5" pad="116"/>
<contactref element="IC5" pad="134"/>
<contactref element="IC3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C28" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="DIS1" pad="VDD"/>
<contactref element="C36" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="C52" pad="+"/>
<contactref element="IC15" pad="3"/>
<contactref element="C56" pad="2"/>
<contactref element="C48" pad="+"/>
<contactref element="D1" pad="C"/>
<contactref element="F1" pad="2A"/>
<contactref element="C53" pad="1"/>
<contactref element="IC12" pad="5"/>
<contactref element="C54" pad="1"/>
<contactref element="IC13" pad="5"/>
<contactref element="C55" pad="1"/>
<contactref element="IC14" pad="5"/>
<contactref element="C41" pad="1"/>
<contactref element="IC7" pad="5"/>
<contactref element="R12" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="IC5" pad="19"/>
<contactref element="IC5" pad="27"/>
<contactref element="IC5" pad="36"/>
<contactref element="IC5" pad="41"/>
<contactref element="IC5" pad="48"/>
<contactref element="IC5" pad="57"/>
<contactref element="IC5" pad="63"/>
<contactref element="IC5" pad="74"/>
<contactref element="IC5" pad="82"/>
<contactref element="IC5" pad="94"/>
<contactref element="IC5" pad="95"/>
<contactref element="IC5" pad="97"/>
<contactref element="IC5" pad="108"/>
<contactref element="IC5" pad="118"/>
<contactref element="IC5" pad="123"/>
<contactref element="IC5" pad="131"/>
<contactref element="IC5" pad="140"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R2" pad="2B"/>
<contactref element="IC2" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="R1" pad="3A"/>
<contactref element="MOD1" pad="50"/>
<contactref element="MOD1" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="C17" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="DIS1" pad="COM"/>
<contactref element="C36" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="DDS1" pad="P1.2"/>
<contactref element="DDS1" pad="P1.4"/>
<contactref element="DDS1" pad="P1.6"/>
<contactref element="DDS1" pad="P1.8"/>
<contactref element="DDS1" pad="P1.10"/>
<contactref element="DDS1" pad="P1.12"/>
<contactref element="DDS1" pad="P1.14"/>
<contactref element="DDS1" pad="P1.16"/>
<contactref element="DDS1" pad="P1.18"/>
<contactref element="DDS1" pad="P1.20"/>
<contactref element="DDS1" pad="P1.22"/>
<contactref element="DDS1" pad="P1.24"/>
<contactref element="DDS1" pad="P1.26"/>
<contactref element="DDS1" pad="P1.28"/>
<contactref element="DDS1" pad="P1.30"/>
<contactref element="DDS1" pad="P1.32"/>
<contactref element="DDS1" pad="P1.34"/>
<contactref element="DDS1" pad="P1.36"/>
<contactref element="DDS1" pad="P1.38"/>
<contactref element="DDS1" pad="P1.40"/>
<contactref element="DDS1" pad="U6.2"/>
<contactref element="DDS1" pad="U6.4"/>
<contactref element="DDS1" pad="U6.6"/>
<contactref element="DDS1" pad="U6.8"/>
<contactref element="DDS1" pad="U6.10"/>
<contactref element="DDS1" pad="U6.12"/>
<contactref element="DDS1" pad="U6.14"/>
<contactref element="DDS1" pad="U6.16"/>
<contactref element="DDS1" pad="U6.18"/>
<contactref element="DDS1" pad="U6.20"/>
<contactref element="DDS1" pad="U5.2"/>
<contactref element="DDS1" pad="U5.4"/>
<contactref element="DDS1" pad="U5.6"/>
<contactref element="DDS1" pad="U5.8"/>
<contactref element="DDS1" pad="U5.10"/>
<contactref element="DDS1" pad="U5.12"/>
<contactref element="DDS1" pad="U5.14"/>
<contactref element="DDS1" pad="U5.16"/>
<contactref element="DDS1" pad="U5.18"/>
<contactref element="DDS1" pad="U5.20"/>
<contactref element="DDS1" pad="U9.2"/>
<contactref element="DDS1" pad="U9.4"/>
<contactref element="DDS1" pad="U9.6"/>
<contactref element="DDS1" pad="U9.8"/>
<contactref element="DDS1" pad="U9.10"/>
<contactref element="DDS1" pad="U9.12"/>
<contactref element="DDS1" pad="U9.14"/>
<contactref element="DDS1" pad="U9.16"/>
<contactref element="DDS1" pad="U9.18"/>
<contactref element="DDS1" pad="U9.20"/>
<contactref element="DDS1" pad="U5.3"/>
<contactref element="DDS1" pad="U9.13"/>
<contactref element="DDS1" pad="TB2.2"/>
<contactref element="DDS1" pad="TB1.3"/>
<contactref element="DDS1" pad="TB2.4"/>
<contactref element="R14" pad="2"/>
<contactref element="RETURN" pad="TP"/>
<contactref element="C47" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C56" pad="1"/>
<contactref element="IC15" pad="1"/>
<contactref element="C57" pad="1"/>
<contactref element="C48" pad="-"/>
<contactref element="C42" pad="NEG"/>
<contactref element="C52" pad="-"/>
<contactref element="R7" pad="1"/>
<contactref element="C38" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="C40" pad="2"/>
<contactref element="C39" pad="NEG"/>
<contactref element="C37" pad="2"/>
<contactref element="IC9" pad="3"/>
<contactref element="C49" pad="2"/>
<contactref element="IC9" pad="1"/>
<contactref element="J3" pad="SHIELD2"/>
<contactref element="J3" pad="SHIELD1"/>
<contactref element="IC10" pad="3"/>
<contactref element="C50" pad="2"/>
<contactref element="IC10" pad="1"/>
<contactref element="J4" pad="SHIELD2"/>
<contactref element="J4" pad="SHIELD1"/>
<contactref element="IC12" pad="3"/>
<contactref element="C53" pad="2"/>
<contactref element="IC12" pad="1"/>
<contactref element="J6" pad="SHIELD2"/>
<contactref element="J6" pad="SHIELD1"/>
<contactref element="IC13" pad="3"/>
<contactref element="C54" pad="2"/>
<contactref element="IC13" pad="1"/>
<contactref element="J7" pad="SHIELD2"/>
<contactref element="J7" pad="SHIELD1"/>
<contactref element="IC11" pad="3"/>
<contactref element="C51" pad="2"/>
<contactref element="IC11" pad="1"/>
<contactref element="J5" pad="SHIELD2"/>
<contactref element="J5" pad="SHIELD1"/>
<contactref element="IC14" pad="3"/>
<contactref element="C55" pad="2"/>
<contactref element="IC14" pad="1"/>
<contactref element="J8" pad="SHIELD2"/>
<contactref element="J8" pad="SHIELD1"/>
<contactref element="OSC1" pad="COM"/>
<contactref element="C46" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="R13" pad="CCW"/>
<contactref element="J2" pad="COM1"/>
<contactref element="J2" pad="COM2"/>
<contactref element="J2" pad="COM3"/>
<contactref element="J2" pad="COM4"/>
<contactref element="C44" pad="NEG"/>
<contactref element="C41" pad="2"/>
<contactref element="IC7" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="OCXO-" pad="TP"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW2" pad="2"/>
<contactref element="SW3" pad="2"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC5" pad="PAD"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="7"/>
<contactref element="IC5" pad="13"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="1"/>
<contactref element="IC5" pad="12"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="9"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="CONF_DONE">
<contactref element="R2" pad="1A"/>
<contactref element="J1" pad="3"/>
<contactref element="IC5" pad="92"/>
<contactref element="CONF_DONE" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="5"/>
<contactref element="R2" pad="3A"/>
<contactref element="IC5" pad="14"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="6"/>
<contactref element="R2" pad="2A"/>
<contactref element="IC5" pad="21"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="4A"/>
<contactref element="IC5" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="3B"/>
<contactref element="IC5" pad="16"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="2B"/>
<contactref element="IC5" pad="18"/>
</signal>
<signal name="N$13">
<contactref element="R1" pad="1B"/>
<contactref element="IC5" pad="15"/>
</signal>
<signal name="D0">
<contactref element="MOD1" pad="8"/>
<contactref element="IC5" pad="135"/>
</signal>
<signal name="D1">
<contactref element="MOD1" pad="9"/>
<contactref element="IC5" pad="133"/>
</signal>
<signal name="D2">
<contactref element="MOD1" pad="10"/>
<contactref element="IC5" pad="132"/>
</signal>
<signal name="D3">
<contactref element="MOD1" pad="11"/>
<contactref element="IC5" pad="125"/>
</signal>
<signal name="D4">
<contactref element="MOD1" pad="12"/>
<contactref element="IC5" pad="121"/>
</signal>
<signal name="D5">
<contactref element="MOD1" pad="13"/>
<contactref element="IC5" pad="120"/>
</signal>
<signal name="D6">
<contactref element="MOD1" pad="14"/>
<contactref element="IC5" pad="119"/>
</signal>
<signal name="D7">
<contactref element="MOD1" pad="15"/>
<contactref element="IC5" pad="115"/>
</signal>
<signal name="CMD0">
<contactref element="MOD1" pad="17"/>
<contactref element="IC5" pad="104"/>
</signal>
<signal name="CMD2">
<contactref element="MOD1" pad="19"/>
<contactref element="IC5" pad="100"/>
</signal>
<signal name="CS">
<contactref element="IC5" pad="98"/>
<contactref element="MOD1" pad="21"/>
</signal>
<signal name="CMD1">
<contactref element="MOD1" pad="18"/>
<contactref element="IC5" pad="103"/>
</signal>
<signal name="CMD3">
<contactref element="MOD1" pad="20"/>
<contactref element="IC5" pad="99"/>
</signal>
<signal name="P2">
<contactref element="IC5" pad="52"/>
<contactref element="DDS1" pad="U6.9"/>
</signal>
<signal name="IO_UPDATE">
<contactref element="IC5" pad="51"/>
<contactref element="DDS1" pad="U6.3"/>
</signal>
<signal name="IO_RST">
<contactref element="IC5" pad="50"/>
<contactref element="DDS1" pad="U5.1"/>
</signal>
<signal name="SCLK">
<contactref element="IC5" pad="49"/>
<contactref element="DDS1" pad="U5.5"/>
</signal>
<signal name="DRCTL">
<contactref element="IC5" pad="42"/>
<contactref element="DDS1" pad="U5.13"/>
</signal>
<signal name="DROVER">
<contactref element="IC5" pad="39"/>
<contactref element="DDS1" pad="U5.15"/>
</signal>
<signal name="DRHOLD">
<contactref element="IC5" pad="43"/>
<contactref element="DDS1" pad="U5.11"/>
</signal>
<signal name="N$30">
<contactref element="DIS1" pad="RXD"/>
<contactref element="MOD1" pad="24"/>
</signal>
<signal name="P1">
<contactref element="IC5" pad="53"/>
<contactref element="DDS1" pad="U6.7"/>
</signal>
<signal name="P0">
<contactref element="IC5" pad="54"/>
<contactref element="DDS1" pad="U6.5"/>
</signal>
<signal name="PLL_LOCK">
<contactref element="IC5" pad="55"/>
<contactref element="DDS1" pad="U9.15"/>
</signal>
<signal name="RAM_SWP_OVR">
<contactref element="IC5" pad="58"/>
<contactref element="DDS1" pad="U9.19"/>
</signal>
<signal name="TX_EN">
<contactref element="IC5" pad="59"/>
<contactref element="DDS1" pad="U6.13"/>
</signal>
<signal name="RESET">
<contactref element="IC5" pad="60"/>
<contactref element="DDS1" pad="U9.11"/>
</signal>
<signal name="N$62">
<contactref element="TP1" pad="TP"/>
<contactref element="IC5" pad="114"/>
</signal>
<signal name="N$66">
<contactref element="TP2" pad="TP"/>
<contactref element="IC5" pad="113"/>
</signal>
<signal name="SDIO">
<contactref element="IC5" pad="44"/>
<contactref element="DDS1" pad="U5.9"/>
</signal>
<signal name="SDO">
<contactref element="IC5" pad="46"/>
<contactref element="DDS1" pad="U5.7"/>
</signal>
<signal name="SP0">
<contactref element="IC5" pad="83"/>
<contactref element="MOD1" pad="22"/>
</signal>
<signal name="SP1">
<contactref element="IC5" pad="84"/>
<contactref element="MOD1" pad="23"/>
</signal>
<signal name="SP2">
<contactref element="IC5" pad="85"/>
<contactref element="MOD1" pad="32"/>
</signal>
<signal name="CSEQOVR">
<contactref element="MOD1" pad="36"/>
<contactref element="IC5" pad="86"/>
</signal>
<signal name="N$16">
<contactref element="IC5" pad="22"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="OUT3">
<contactref element="IC5" pad="80"/>
<contactref element="IC14" pad="2"/>
</signal>
<signal name="OUT2">
<contactref element="IC5" pad="79"/>
<contactref element="IC13" pad="2"/>
</signal>
<signal name="OUT1">
<contactref element="IC5" pad="77"/>
<contactref element="IC12" pad="2"/>
</signal>
<signal name="IN3">
<contactref element="IC5" pad="76"/>
<contactref element="IC11" pad="4"/>
</signal>
<signal name="IN2">
<contactref element="IC5" pad="72"/>
<contactref element="IC10" pad="4"/>
</signal>
<signal name="IN1">
<contactref element="IC5" pad="71"/>
<contactref element="IC9" pad="4"/>
</signal>
<signal name="N$29">
<contactref element="IC3" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="IC4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="+1.8V">
<contactref element="IC6" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C40" pad="1"/>
<contactref element="C39" pad="POS"/>
<contactref element="DDS1" pad="TB2.1"/>
<contactref element="DDS1" pad="TB1.1"/>
</signal>
<signal name="N$33">
<contactref element="R14" pad="1"/>
<contactref element="DDS1" pad="P1.9"/>
<contactref element="DDS1" pad="P1.11"/>
<contactref element="DDS1" pad="P1.13"/>
<contactref element="DDS1" pad="P1.15"/>
<contactref element="DDS1" pad="P1.17"/>
<contactref element="DDS1" pad="P1.19"/>
<contactref element="DDS1" pad="P1.21"/>
<contactref element="DDS1" pad="P1.23"/>
<contactref element="DDS1" pad="P1.25"/>
<contactref element="DDS1" pad="P1.27"/>
<contactref element="DDS1" pad="P1.29"/>
<contactref element="DDS1" pad="P1.31"/>
<contactref element="DDS1" pad="P1.33"/>
<contactref element="DDS1" pad="P1.35"/>
<contactref element="DDS1" pad="P1.37"/>
<contactref element="DDS1" pad="P1.39"/>
<contactref element="DDS1" pad="U6.17"/>
<contactref element="DDS1" pad="U6.19"/>
</signal>
<signal name="N$5">
<contactref element="+5V_IN" pad="TP"/>
<contactref element="C47" pad="2"/>
<contactref element="F1" pad="1A"/>
</signal>
<signal name="N$42">
<contactref element="R7" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="J3" pad="CONDUCTOR"/>
<contactref element="R18" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="IC9" pad="2"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="J4" pad="CONDUCTOR"/>
<contactref element="R19" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="IC10" pad="2"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="J6" pad="CONDUCTOR"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="R21" pad="1"/>
<contactref element="IC12" pad="4"/>
</signal>
<signal name="N$27">
<contactref element="J7" pad="CONDUCTOR"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R22" pad="1"/>
<contactref element="IC13" pad="4"/>
</signal>
<signal name="N$35">
<contactref element="J5" pad="CONDUCTOR"/>
<contactref element="R20" pad="2"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="IC11" pad="2"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="J8" pad="CONDUCTOR"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="R23" pad="1"/>
<contactref element="IC14" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="OSC1" pad="OUT"/>
<contactref element="J2" pad="CONDUCTOR"/>
</signal>
<signal name="N$17">
<contactref element="C43" pad="1"/>
<contactref element="OSC1" pad="CTRL"/>
<contactref element="R13" pad="W"/>
</signal>
<signal name="N$18">
<contactref element="R13" pad="CW"/>
<contactref element="OSC1" pad="VREF"/>
</signal>
<signal name="N$19">
<contactref element="C44" pad="POS"/>
<contactref element="OSC1" pad="VDD"/>
<contactref element="C46" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="IC8" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R12" pad="2"/>
<contactref element="C42" pad="POS"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC8" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="R9" pad="2"/>
<contactref element="IC7" pad="1"/>
<contactref element="OCXO+" pad="TP"/>
</signal>
<signal name="N$31">
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="SW1" pad="COM"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="SW2" pad="COM"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R17" pad="1"/>
<contactref element="SW3" pad="COM"/>
</signal>
<signal name="N$39">
</signal>
<signal name="N$40">
</signal>
<signal name="N$41">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
</signals>
</board>
</drawing>
</eagle>
