<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="166.3" y2="0" width="0" layer="20"/>
<wire x1="166.3" y1="0" x2="166.3" y2="191.5" width="0" layer="20"/>
<wire x1="166.3" y1="191.5" x2="0" y2="191.5" width="0" layer="20"/>
<wire x1="0" y1="191.5" x2="0" y2="0" width="0" layer="20"/>
<text>AC</text>
<text>Plug</text>
<text>Up:Monitor</text>
<text>Dn:Feedfwd</text>
<text>PD</text>
<text>Current Gain 2</text>
<text>Current Gain 1</text>
<text>Current Range</text>
<text>Current</text>
<text>Up:Current</text>
<text>Dn:Piezo</text>
<text>Piezo Gain</text>
<text>Crossing</text>
<text>Scan</text>
<text>Scan/Run</text>
<text>Piezo P-Gain</text>
<text>Piezo P-Range</text>
<text>Piezo D-Gain</text>
<text>Piezo I-Gain</text>
<text>Piezo Integrator</text>
<text>Feed Forward</text>
<text>Pandora Wavelength PID</text>
<text>University of Toronto</text>
<text>Rev:B</text>
<text>Æ. Steinberg Labs</text>
<text>Pandora Wavelength PID</text>
<text>B2</text>
<text>X.X./A.S.</text>
<text>0.18mm</text>
<text>0.18mm</text>
<text>0.1mm</text>
<text>0.5mm/0.18sp</text>
<text>0.25mm</text>
<text>Rev-B1:  Initial release</text>
<text>Caution: 110VAC</text>
<text>Rev-B2:  Various minor mods after assembly and testing.</text>
<hole x="23.1648" y="20.701" drill="3.175"/>
<hole x="143.3322" y="170.7134" drill="3.175"/>
<hole x="143.3068" y="120.7008" drill="3.175"/>
<hole x="143.3322" y="20.701" drill="3.175"/>
<hole x="23.1648" y="70.7136" drill="3.175"/>
<hole x="23.1714" y="170.72" drill="3.175"/>
</plain>
<libraries>
<library name="QuantumOptics">
<packages>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, based on Kemet's description.</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, based on TI's version of JEDEC MO-175 Variant AA.</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, based on Vishay.</description>
</package>
<package name="SWITCH:DPDT-DIP(COPAL-CS4_6-PAD)">
<description>&lt;b&gt;DIP (SMT) switch, DPDT&lt;/b&gt;, Copal CS-4- footprint for 3mm J-hook or 5mm gullwing.  http://media.digikey.com/pdf/Data%20Sheets/COPAL%20Electronics%20PDFs/CS-4.pdf</description>
</package>
<package name="BOURNS:3296Y">
<description>&lt;b&gt;3296Y (multi, top adj), 3296Z (multi, side adj) or 3386X/H (1-turn, top) Trimpot&lt;/b&gt;, Bourns.  Staggered pins so can insert trimpot one way only.  http://www.bourns.com/pdf/3296.pdf</description>
</package>
<package name="SWITCH:SPDT-DIP(COPAL)">
<description>&lt;b&gt;DIP (SMT) switch, SPDT&lt;/b&gt;, Copal CJS-1200, fits A1 (J-lead) and B1 (gullwing), http://media.digikey.com/pdf/Data%20Sheets/COPAL%20Electronics%20PDFs/CJS.pdf?cshift_ck=null&amp;client_id=5210&amp;cshift_ck=null&amp;client_id=5210</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;, 16 pin on 0.1" x 0.3" grid, 0.028" holes (less plating). Can take gullwing SMT.</description>
</package>
<package name="DIODE:BRIDGE,MMC_MB??S">
<description>&lt;b&gt;Diode bridge, Micro Commercial MBxxS package&lt;/b&gt;, http://61.222.192.61/mccsemi/up_pdf/MB05S-MB10S(MBS-1).pdf</description>
</package>
<package name="CAP:NICHICON_UPW-12.5MM">
<description>&lt;b&gt;Capacitor, Nichicon UPW-series 12.5mm dia x 5mm pin c-c&lt;/b&gt;, through-hole.  http://products.nichicon.co.jp/en/pdf/XJA043/e-pw.pdf</description>
</package>
<package name="SOD323">
<description>&lt;b&gt;SOD-323, Diode&lt;/b&gt;Taken from http://www.nxp.com/documents/data_sheet/BZX384_SERIES.pdf</description>
</package>
<package name="EIA-A(SMA)">
<description>&lt;b&gt;EIA size A, AKA SMA&lt;/b&gt;, SMT.</description>
</package>
<package name="TO263">
<description>&lt;b&gt;TO-263&lt;/b&gt;, SMT power.  Uses 0.1" grid.  Add large polygon for case connection.  Ignore DRC restrict errors.  e.g. http://cache.national.com/ds/LM/LM1086.pdf</description>
</package>
<package name="SOT223(C)">
<description>&lt;b&gt;SOT-223&lt;/b&gt;, no centre pin, uses tab.</description>
</package>
<package name="CAP:5MM-THROUGH">
<description>&lt;b&gt;Cap, 5mm c-c throughole, 10mm can&lt;/b&gt;, e.g. Nichicon http://nichicon-us.com/english/products/pdf/e-lv.pdf</description>
</package>
<package name="CONN-BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, 0.1" grid, types such as 227677-1,  nut 1-329631-2, shoulder washer 330620.  The section of the BNC hanging over the edge of the PCB is in layer 49 (Reference).&lt;br&gt;
http://catalog.tycoelectronics.com/TE/bin/TE.Connect?C=1&amp;PN=227677-1&amp;M=STARTSWITH&amp;LG=1&amp;I=13&amp;button.x=0&amp;button.y=0</description>
</package>
<package name="SWITCH:E-SWITCH_1??AV2?">
<description>&lt;b&gt;Toggle SPDT, right angle PCB, vertical actuation&lt;/b&gt;, C&amp;K E-Switch series, such as E101MD1AV2BE (on-on) or E103MD1AV2BE (on-off-on).</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire.  Has fence (bit larger than other TP) around to allow easier soldering.  Drilled 0.0465, plated down to 1.1mm.</description>
</package>
<package name="CASE:HAMMOND_1598D">
<description>&lt;b&gt;Case, Hammond 1598D&lt;/b&gt;, case is 206mmW x 180D x 64H, http://www.hammondmfg.com/pdf/1598D.pdf.&lt;br&gt;
Has 0.5mm space between PCB and inside of front and back plates, larger gap at sides.</description>
</package>
<package name="RF-SHIELD:44X44X9.75MM(BMI-S-207-F)">
<description>&lt;b&gt;RF Shield, 44 x 44 x 9.75mm, Laird Tech BMI-S-207-F&lt;/b&gt;, SMT, fits QFP160, http://media.digikey.com/pdf/Data%20Sheets/Laird%20Technologies/BMI-S-207.pdf and http://lairdtech.thomasnet.com/item/all-categories/standard-surface-mount-shields-two-piece/bmis-207?plpver=10&amp;categid=100&amp;prodid=3001092&amp;origin=keyword#.</description>
</package>
<package name="TP-0.125">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.125" hole, to fit terminal such as Keystone 1502-2.  Has fence around to allow easier soldering.&lt;br&gt;
http://www.keyelco.com/kec/pdfs/p80.pdf</description>
</package>
<package name="BOURNS_3590">
<description>&lt;b&gt;Pot&lt;/b&gt;, 10-turn, Bourns 3590, mounted on side.  Panel, when mounted, is shown with diagonal lines.&lt;br&gt;
&lt;a href="http://www.bourns.com/pdf/3590.pdf"&gt;http://www.bourns.com/pdf/3590.pdf&lt;/a&gt;&lt;br&gt;
Also remember turns counting dial H-22-6a.</description>
</package>
<package name="TO263-5(TYPE2)">
<description>&lt;b&gt;TO-263-5, AKA "KTT"&lt;/b&gt;, SMT power.  Ignore DRC errors for pads, connected to centre pin.  http://www.ti.com/litv/pdf/mpsf007d</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="PASSIVE_0.4&quot;">
<description>&lt;b&gt;Through-hole Component&lt;/b&gt;, on 0.4" spacing with 0.052" drill, good for most passives, R's up to 0.5W.&lt;br&gt;
Has solder resist around pins to prevent solder jumpers to pours.</description>
</package>
<package name="TRANSFORMER:TAMURA_3FD-3">
<description>&lt;b&gt;Transformer, dual primary and dual secondary&lt;/b&gt;, Tamura 3FD-3xx (dual pri) or 3FS-3xx (single pri), http://www.tamuracorp.com/clientuploads/pdfs/engineeringdocs/3FD-3XX.pdf</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="SOT89">
<description>&lt;b&gt;SOT-89&lt;/b&gt;, like a grownup SOT23. e.g.  http://www.zetex.com/3.0/pdf/SOT89P.pdf</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="CONN:BNC,DUAL(BOMAR)">
<description>&lt;b&gt;Dual BNC, vertical throughhole, isolated&lt;/b&gt;, Bomar, e.g. 364A2595, H=29.3mm, http://media.digikey.com/pdf/Data%20Sheets/Bomar%20PDFs/BNC_Products_Spec.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="QuantumOptics" package="CONN-BNC-AMP-TYPE3HORIZ" value="&quot;PD&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Tyco"/>
<attribute name="PN" value="5227161-6"/>
</element>
<element name="C19" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW4" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Z-P&quot;"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="QuantumOptics" package="SOT23-5" value="AD8065ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C21" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="IC9" library="QuantumOptics" package="SOIC-8" value="AD8066ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="QuantumOptics" package="2012(0805)" value="5.6pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-2K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;C-Gain1&quot;"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="QuantumOptics" package="2012(0805)" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="SW6" library="QuantumOptics" package="SWITCH:DPDT-DIP(COPAL-CS4_6-PAD)" value="CS-4-22YTB">
<attribute name="NAME"/>
<attribute name="MFG" value="Copal"/>
<attribute name="DESC" value="&quot;C-Pol&quot;"/>
</element>
<element name="C40" library="QuantumOptics" package="2012(0805)" value="5.6pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="15nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-2K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;C-Gain2&quot;"/>
</element>
<element name="R45" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-1K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;C-Range&quot;"/>
</element>
<element name="R16" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Z-Gain&quot;"/>
</element>
<element name="IC7" library="QuantumOptics" package="SOIC-8" value="AD8066ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="QuantumOptics" package="2012(0805)" value="15nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Z-Dgain&quot;"/>
</element>
<element name="C24" library="QuantumOptics" package="2012(0805)" value="15nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Z-Pgain&quot;"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="QuantumOptics" package="2012(0805)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW5" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Z-D&quot;"/>
</element>
<element name="R13" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW3" library="QuantumOptics" package="DIL16" value="KAP1108E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="AVX: 0805YD106KAT2A"/>
</element>
<element name="C33" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="QuantumOptics" package="2012(0805)" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOIC-8" value="AD8066ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="QuantumOptics" package="2012(0805)" value="15nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="QuantumOptics" package="2012(0805)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Z-Igain&quot;"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH:DPDT-DIP(COPAL-CS4_6-PAD)" value="CS-4-22YTB">
<attribute name="NAME"/>
<attribute name="MFG" value="Copal"/>
<attribute name="DESC" value="&quot;Z-Pol&quot;"/>
</element>
<element name="R50" library="QuantumOptics" package="2012(0805)" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C104K1RACTU"/>
<attribute name="VOLTAGE" value="100V"/>
</element>
<element name="R42" library="QuantumOptics" package="2012(0805)" value="18.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="QuantumOptics" package="2012(0805)" value="33.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW7" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="100AWSP3T2B4M7RE"/>
<element name="IC10" library="QuantumOptics" package="TO263-5(TYPE2)" value="OPA544F">
<attribute name="NAME"/>
</element>
<element name="C47" library="QuantumOptics" package="2012(0805)" value="1.5nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="AVX"/>
<attribute name="PN" value="08051C152KAT2A"/>
<attribute name="VOLTAGE" value="100V"/>
</element>
<element name="TR1" library="QuantumOptics" package="TRANSFORMER:TAMURA_3FD-3" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Tamura"/>
<attribute name="PN" value="3FD-356"/>
<attribute name="VOLTAGE" value="56Vct"/>
</element>
<element name="AC1" library="QuantumOptics" package="TP-0.125" value=""/>
<element name="AC2" library="QuantumOptics" package="TP-0.125" value=""/>
<element name="TR2" library="QuantumOptics" package="TRANSFORMER:TAMURA_3FD-3" value="">
<attribute name="NAME"/>
<attribute name="MFG" value="Tamura"/>
<attribute name="PN" value="3FD-320"/>
<attribute name="VOLTAGE" value="20Vct"/>
</element>
<element name="PWR" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Bulgin"/>
<attribute name="PN" value="PF0011/10/28"/>
</element>
<element name="SWTCH" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="E-Switch"/>
<attribute name="PN" value="100SP1T1B1M1QEH"/>
</element>
<element name="D1" library="QuantumOptics" package="DIODE:BRIDGE,MMC_MB??S" value="MB4S">
<attribute name="NAME"/>
</element>
<element name="D2" library="QuantumOptics" package="DIODE:BRIDGE,MMC_MB??S" value="MB4S">
<attribute name="NAME"/>
</element>
<element name="C3" library="QuantumOptics" package="CAP:NICHICON_UPW-12.5MM" value="100uF/160V">
<attribute name="NAME"/>
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEU-EE2C101"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="6.65K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="QuantumOptics" package="SOD323" value="68V">
<attribute name="NAME"/>
<attribute name="MFG" value="Philips"/>
<attribute name="PN" value="BZX384-B68,115"/>
</element>
<element name="C7" library="QuantumOptics" package="CAP:NICHICON_UPW-12.5MM" value="100uF/160V">
<attribute name="NAME"/>
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEU-EE2C101"/>
</element>
<element name="D4" library="QuantumOptics" package="EIA-A(SMA)" value="S1D-13-F">
<attribute name="NAME"/>
</element>
<element name="Q1" library="QuantumOptics" package="SOT89" value="FCX495">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="QuantumOptics" package="2012(0805)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Z-Prange&quot;"/>
</element>
<element name="R40" library="QuantumOptics" package="2012(0805)" value="14K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="100AWSP1T2B4M7RE">
<attribute name="ALT-PN" value="100SP1T2B4M7RE"/>
<attribute name="MFG" value="E-Switch"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="QuantumOptics" package="CAP:5MM-THROUGH" value="270uF/25V">
<attribute name="NAME"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="PLV1E271MDL1TD"/>
</element>
<element name="IC2" library="QuantumOptics" package="TO263" value="LM7909CT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW8" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="100AWSP5T2B4M7RE"/>
<element name="J2" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Current&quot;"/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value="364A2595"/>
</element>
<element name="IC1" library="QuantumOptics" package="SOT223(C)" value="LM2937IMP-10">
<attribute name="NAME"/>
</element>
<element name="C2" library="QuantumOptics" package="CAP:5MM-THROUGH" value="270uF/25V">
<attribute name="NAME"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="PLV1E271MDL1TD"/>
</element>
<element name="C5" library="QuantumOptics" package="CAP:5MM-THROUGH" value="270uF/25V">
<attribute name="NAME"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="PLV1E271MDL1TD"/>
</element>
<element name="C4" library="QuantumOptics" package="CAP:5MM-THROUGH" value="270uF/25V">
<attribute name="NAME"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="PLV1E271MDL1TD"/>
</element>
<element name="IC3" library="QuantumOptics" package="SOT223(C)" value="LM2937IMP-10">
<attribute name="NAME"/>
</element>
<element name="C6" library="QuantumOptics" package="CAP:5MM-THROUGH" value="270uF/25V">
<attribute name="NAME"/>
<attribute name="MFG" value="Nichicon"/>
<attribute name="PN" value="PLV1E271MDL1TD"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="QuantumOptics" package="SOT23" value="LM4040A50DBZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="QuantumOptics" package="SOT23" value="LM4040A50DBZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="QuantumOptics" package="SOIC-8" value="AD8066ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Crossing&quot;"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOIC-8" value="AD8066ARZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="12K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;Scan&quot;"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;PD Monitor&quot;"/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value="364A2595"/>
</element>
<element name="R49" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC11" library="QuantumOptics" package="SOT23-5" value="AD8065ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="QuantumOptics" package="BOURNS:3296Y" value="3386X-10K">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;FeedFwd&quot;"/>
</element>
<element name="C49" library="QuantumOptics" package="2012(0805)" value="1.5nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="QuantumOptics" package="2012(0805)" value="57.6K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW9" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
<attribute name="DESC" value="&quot;FeedFwd Pol&quot;"/>
</element>
<element name="R48" library="QuantumOptics" package="2012(0805)" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$27" library="QuantumOptics" package="CASE:HAMMOND_1598D" value=""/>
<element name="CASE" library="QuantumOptics" package="MISC" value="1598D">
<attribute name="MFG" value="Hammond"/>
<attribute name="PN" value="1598D"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="QuantumOptics" package="BOURNS_3590" value="&quot;Setpoint&quot;">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3590S-2-103L"/>
</element>
<element name="R52" library="QuantumOptics" package="2012(0805)" value="6.65K"/>
<element name="PWR-LED" library="QuantumOptics" package="TP-0.042B" value=""/>
<element name="LED-COM" library="QuantumOptics" package="TP-0.042B" value=""/>
<element name="PWRLED" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Dialight"/>
<attribute name="PN" value="558-0102-007F"/>
</element>
<element name="R53" library="QuantumOptics" package="2012(0805)" value="6.65K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED+" library="QuantumOptics" package="TP-0.042B" value=""/>
<element name="LED-" library="QuantumOptics" package="TP-0.042B" value=""/>
<element name="INTLED" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Kingbright"/>
<attribute name="PN" value="WP59EGC"/>
</element>
<element name="DUAL-D" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Diodes Inc"/>
<attribute name="PN" value="BAT54ATA"/>
</element>
<element name="SHLD-COV" library="QuantumOptics" package="RF-SHIELD:44X44X9.75MM(BMI-S-207-F)" value="BMI-S-207-C">
<attribute name="MFG" value="Larid Tech."/>
</element>
<element name="U$39" library="QuantumOptics" package="TITLEBLOCK_PCB" value=""/>
<element name="R54" library="QuantumOptics" package="PASSIVE_0.4&quot;" value="out">
<attribute name="NAME"/>
</element>
<element name="R55" library="QuantumOptics" package="2012(0805)" value="82.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="QuantumOptics" package="CAP:NICHICON_UPW-12.5MM" value="22uF/100V"/>
<element name="C53" library="QuantumOptics" package="2012(0805)" value="1nF"/>
<element name="SHLD1" library="QuantumOptics" package="RF-SHIELD:44X44X9.75MM(BMI-S-207-F)" value="BMI-S-207-F">
<attribute name="MFG" value="Laird Tech."/>
</element>
</elements>
<signals>
<signal name="+10V">
<contactref element="C19" pad="1"/>
<contactref element="IC6" pad="5"/>
<contactref element="C43" pad="1"/>
<contactref element="IC9" pad="8"/>
<contactref element="C27" pad="1"/>
<contactref element="IC7" pad="8"/>
<contactref element="C41" pad="1"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="+"/>
<contactref element="R2" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="C10" pad="1"/>
<contactref element="IC4" pad="8"/>
<contactref element="C50" pad="1"/>
<contactref element="IC11" pad="5"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="N$091">
<contactref element="R15" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="R12" pad="2"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="R15" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="!1"/>
</signal>
<signal name="-9V">
<contactref element="C20" pad="1"/>
<contactref element="IC6" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="IC9" pad="4"/>
<contactref element="C28" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="C42" pad="1"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC2" pad="3"/>
<contactref element="C5" pad="-"/>
<contactref element="R3" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="C11" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="C51" pad="1"/>
<contactref element="IC11" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="C43" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="SW6" pad="2"/>
<contactref element="SW6" pad="!1"/>
<contactref element="R19" pad="1"/>
<contactref element="R45" pad="CW"/>
<contactref element="C27" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC7" pad="5"/>
<contactref element="C41" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="IC8" pad="3"/>
<contactref element="IC8" pad="5"/>
<contactref element="R17" pad="CCW"/>
<contactref element="IC10" pad="3"/>
<contactref element="C48" pad="2"/>
<contactref element="TR2" pad="S2A"/>
<contactref element="TR2" pad="S1B"/>
<contactref element="D1" pad="-"/>
<contactref element="C3" pad="-"/>
<contactref element="D3" pad="A"/>
<contactref element="C7" pad="-"/>
<contactref element="C45" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="R27" pad="CCW"/>
<contactref element="R40" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="C5" pad="+"/>
<contactref element="C4" pad="-"/>
<contactref element="IC3" pad="2"/>
<contactref element="C6" pad="-"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="D5" pad="1"/>
<contactref element="D6" pad="3"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="J2" pad="LWR-COM"/>
<contactref element="J2" pad="UPR-COM"/>
<contactref element="J3" pad="UPR-COM"/>
<contactref element="C50" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="R39" pad="CCW"/>
<contactref element="SW9" pad="1"/>
<contactref element="J3" pad="LWR-COM"/>
<contactref element="LED-COM" pad="TP"/>
<contactref element="LED-" pad="TP"/>
<contactref element="SHLD-COV" pad="1"/>
<contactref element="SHLD-COV" pad="2"/>
<contactref element="SHLD-COV" pad="3"/>
<contactref element="SHLD-COV" pad="4"/>
<contactref element="SHLD-COV" pad="5"/>
<contactref element="SHLD-COV" pad="6"/>
<contactref element="SHLD-COV" pad="7"/>
<contactref element="SHLD-COV" pad="8"/>
<contactref element="SHLD-COV" pad="9"/>
<contactref element="SHLD-COV" pad="10"/>
<contactref element="SHLD-COV" pad="11"/>
<contactref element="SHLD-COV" pad="12"/>
<contactref element="SHLD-COV" pad="13"/>
<contactref element="SHLD-COV" pad="14"/>
<contactref element="SHLD-COV" pad="15"/>
<contactref element="SHLD-COV" pad="16"/>
<contactref element="SHLD-COV" pad="17"/>
<contactref element="SHLD-COV" pad="18"/>
<contactref element="SHLD-COV" pad="19"/>
<contactref element="SHLD-COV" pad="20"/>
<contactref element="SHLD-COV" pad="21"/>
<contactref element="SHLD-COV" pad="22"/>
<contactref element="SHLD-COV" pad="23"/>
<contactref element="SHLD-COV" pad="24"/>
<contactref element="SHLD-COV" pad="25"/>
<contactref element="SHLD-COV" pad="26"/>
<contactref element="SHLD-COV" pad="27"/>
<contactref element="SHLD-COV" pad="28"/>
<contactref element="SHLD-COV" pad="29"/>
<contactref element="SHLD-COV" pad="30"/>
<contactref element="SHLD-COV" pad="31"/>
<contactref element="SHLD-COV" pad="32"/>
<contactref element="R36" pad="CCW"/>
<contactref element="C52" pad="-"/>
<contactref element="C53" pad="1"/>
<contactref element="SHLD1" pad="1"/>
<contactref element="SHLD1" pad="2"/>
<contactref element="SHLD1" pad="3"/>
<contactref element="SHLD1" pad="4"/>
<contactref element="SHLD1" pad="5"/>
<contactref element="SHLD1" pad="6"/>
<contactref element="SHLD1" pad="7"/>
<contactref element="SHLD1" pad="8"/>
<contactref element="SHLD1" pad="9"/>
<contactref element="SHLD1" pad="10"/>
<contactref element="SHLD1" pad="11"/>
<contactref element="SHLD1" pad="12"/>
<contactref element="SHLD1" pad="13"/>
<contactref element="SHLD1" pad="14"/>
<contactref element="SHLD1" pad="15"/>
<contactref element="SHLD1" pad="16"/>
<contactref element="SHLD1" pad="17"/>
<contactref element="SHLD1" pad="18"/>
<contactref element="SHLD1" pad="19"/>
<contactref element="SHLD1" pad="20"/>
<contactref element="SHLD1" pad="21"/>
<contactref element="SHLD1" pad="22"/>
<contactref element="SHLD1" pad="23"/>
<contactref element="SHLD1" pad="24"/>
<contactref element="SHLD1" pad="25"/>
<contactref element="SHLD1" pad="26"/>
<contactref element="SHLD1" pad="27"/>
<contactref element="SHLD1" pad="28"/>
<contactref element="SHLD1" pad="29"/>
<contactref element="SHLD1" pad="30"/>
<contactref element="SHLD1" pad="31"/>
<contactref element="SHLD1" pad="32"/>
</signal>
<signal name="N$013">
<contactref element="R12" pad="1"/>
<contactref element="J1" pad="CONDUCTOR"/>
</signal>
<signal name="N$017">
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="R11" pad="2"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$019">
<contactref element="R14" pad="2"/>
<contactref element="IC6" pad="3"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="N$022">
<contactref element="C30" pad="1"/>
<contactref element="R26" pad="2"/>
<contactref element="IC9" pad="6"/>
<contactref element="R28" pad="CW"/>
<contactref element="R28" pad="W"/>
</signal>
<signal name="INPUT_BUF1">
<contactref element="C30" pad="2"/>
<contactref element="IC9" pad="7"/>
<contactref element="R28" pad="CCW"/>
<contactref element="SW6" pad="!2"/>
<contactref element="SW6" pad="1"/>
</signal>
<signal name="N$041">
<contactref element="R22" pad="2"/>
<contactref element="IC9" pad="5"/>
<contactref element="C26" pad="2"/>
</signal>
<signal name="N$033">
<contactref element="C40" pad="1"/>
<contactref element="IC9" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R34" pad="CW"/>
<contactref element="R34" pad="W"/>
</signal>
<signal name="INPUT_BUF2">
<contactref element="C40" pad="2"/>
<contactref element="IC9" pad="1"/>
<contactref element="R35" pad="1"/>
<contactref element="R34" pad="CCW"/>
</signal>
<signal name="N$057">
<contactref element="R22" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="C22" pad="2"/>
</signal>
<signal name="N$028">
<contactref element="IC9" pad="3"/>
<contactref element="SW6" pad="!C"/>
</signal>
<signal name="N$034">
<contactref element="R32" pad="1"/>
<contactref element="SW6" pad="C"/>
</signal>
<signal name="N$004">
<contactref element="C18" pad="1"/>
<contactref element="R16" pad="CW"/>
<contactref element="R16" pad="W"/>
<contactref element="R13" pad="2"/>
<contactref element="IC5" pad="6"/>
</signal>
<signal name="N$123">
<contactref element="C18" pad="2"/>
<contactref element="R16" pad="CCW"/>
<contactref element="R20" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="R17" pad="CW"/>
<contactref element="R49" pad="1"/>
<contactref element="IC5" pad="7"/>
</signal>
<signal name="N$031">
<contactref element="C25" pad="1"/>
<contactref element="IC7" pad="6"/>
<contactref element="R25" pad="CW"/>
<contactref element="R25" pad="W"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="INPUT_BUF4">
<contactref element="C25" pad="2"/>
<contactref element="IC7" pad="7"/>
<contactref element="R25" pad="CCW"/>
<contactref element="SW5" pad="2"/>
</signal>
<signal name="N$062">
<contactref element="C24" pad="1"/>
<contactref element="IC7" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R24" pad="CW"/>
<contactref element="R24" pad="W"/>
</signal>
<signal name="INPUT_BUF5">
<contactref element="C24" pad="2"/>
<contactref element="IC7" pad="1"/>
<contactref element="R24" pad="CCW"/>
<contactref element="R27" pad="CW"/>
</signal>
<signal name="N$009">
<contactref element="R21" pad="1"/>
<contactref element="C23" pad="2"/>
</signal>
<signal name="N$014">
<contactref element="SW3" pad="16"/>
<contactref element="C35" pad="1"/>
</signal>
<signal name="N$015">
<contactref element="C31" pad="1"/>
<contactref element="SW3" pad="15"/>
</signal>
<signal name="N$030">
<contactref element="SW3" pad="14"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="N$032">
<contactref element="C32" pad="1"/>
<contactref element="SW3" pad="13"/>
</signal>
<signal name="N$039">
<contactref element="C33" pad="1"/>
<contactref element="SW3" pad="11"/>
</signal>
<signal name="N$040">
<contactref element="C34" pad="1"/>
<contactref element="SW3" pad="9"/>
</signal>
<signal name="N$050">
<contactref element="C38" pad="1"/>
<contactref element="SW3" pad="10"/>
</signal>
<signal name="N$051">
<contactref element="C37" pad="1"/>
<contactref element="SW3" pad="12"/>
</signal>
<signal name="N$060">
<contactref element="SW3" pad="8"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW3" pad="2"/>
<contactref element="SW3" pad="3"/>
<contactref element="SW3" pad="4"/>
<contactref element="SW3" pad="5"/>
<contactref element="SW3" pad="6"/>
<contactref element="SW3" pad="7"/>
<contactref element="C29" pad="1"/>
<contactref element="IC8" pad="6"/>
<contactref element="SW2" pad="COM"/>
</signal>
<signal name="N$012">
<contactref element="R31" pad="2"/>
<contactref element="SW5" pad="COM"/>
</signal>
<signal name="N$063">
<contactref element="C39" pad="1"/>
<contactref element="IC8" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="R29" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="INPUT_BUF6">
<contactref element="C39" pad="2"/>
<contactref element="IC8" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="SW7" pad="DOWN"/>
</signal>
<signal name="N$064">
<contactref element="R18" pad="1"/>
<contactref element="R17" pad="W"/>
</signal>
<signal name="N$020">
<contactref element="R13" pad="1"/>
<contactref element="SW1" pad="C"/>
</signal>
<signal name="N$021">
<contactref element="SW1" pad="!C"/>
<contactref element="IC5" pad="5"/>
</signal>
<signal name="N$016">
<contactref element="R46" pad="1"/>
<contactref element="R41" pad="1"/>
<contactref element="IC10" pad="2"/>
<contactref element="C47" pad="1"/>
<contactref element="R42" pad="2"/>
</signal>
<signal name="N$018">
<contactref element="R46" pad="2"/>
<contactref element="R50" pad="1"/>
<contactref element="IC10" pad="4"/>
<contactref element="C47" pad="2"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="N$023">
<contactref element="R42" pad="1"/>
<contactref element="C45" pad="2"/>
<contactref element="R36" pad="W"/>
</signal>
<signal name="N$026">
<contactref element="R41" pad="2"/>
<contactref element="SW7" pad="COM"/>
</signal>
<signal name="N$038">
<contactref element="TR1" pad="S1B"/>
<contactref element="TR1" pad="S2A"/>
</signal>
<signal name="N$046">
<contactref element="TR1" pad="P2A"/>
<contactref element="AC1" pad="TP"/>
<contactref element="TR1" pad="P1A"/>
<contactref element="TR2" pad="P1A"/>
<contactref element="TR2" pad="P2A"/>
</signal>
<signal name="N$035">
<contactref element="TR1" pad="P1B"/>
<contactref element="AC2" pad="TP"/>
<contactref element="TR1" pad="P2B"/>
<contactref element="TR2" pad="P2B"/>
<contactref element="TR2" pad="P1B"/>
</signal>
<signal name="N$010">
<contactref element="TR1" pad="S2B"/>
<contactref element="D1" pad="AC2"/>
</signal>
<signal name="N$027">
<contactref element="D1" pad="AC1"/>
<contactref element="TR1" pad="S1A"/>
</signal>
<signal name="N$029">
<contactref element="D1" pad="+"/>
<contactref element="C3" pad="+"/>
<contactref element="R1" pad="2"/>
<contactref element="D4" pad="K"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$037">
<contactref element="D2" pad="AC1"/>
<contactref element="TR2" pad="S1A"/>
</signal>
<signal name="N$047">
<contactref element="D2" pad="AC2"/>
<contactref element="TR2" pad="S2B"/>
</signal>
<signal name="N$053">
<contactref element="R1" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="Q1" pad="1"/>
<contactref element="C52" pad="+"/>
</signal>
<signal name="+67V">
<contactref element="C7" pad="+"/>
<contactref element="D4" pad="A"/>
<contactref element="Q1" pad="3"/>
<contactref element="IC10" pad="5"/>
<contactref element="C48" pad="1"/>
</signal>
<signal name="N$006">
<contactref element="R30" pad="2"/>
<contactref element="SW4" pad="COM"/>
</signal>
<signal name="N$056">
<contactref element="SW4" pad="2"/>
<contactref element="R27" pad="W"/>
</signal>
<signal name="N$061">
<contactref element="R37" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="IC10" pad="1"/>
</signal>
<signal name="N$043">
<contactref element="R43" pad="1"/>
<contactref element="R44" pad="1"/>
<contactref element="R39" pad="W"/>
</signal>
<signal name="N$044">
<contactref element="R43" pad="2"/>
<contactref element="R47" pad="1"/>
<contactref element="IC11" pad="4"/>
<contactref element="C49" pad="1"/>
</signal>
<signal name="N$045">
<contactref element="R47" pad="2"/>
<contactref element="R51" pad="1"/>
<contactref element="C49" pad="2"/>
<contactref element="IC11" pad="1"/>
</signal>
<signal name="N$055">
<contactref element="R44" pad="2"/>
<contactref element="IC11" pad="3"/>
<contactref element="SW9" pad="COM"/>
<contactref element="C53" pad="2"/>
</signal>
<signal name="N$002">
<contactref element="D2" pad="+"/>
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$003">
<contactref element="D2" pad="-"/>
<contactref element="IC2" pad="2"/>
<contactref element="C2" pad="-"/>
</signal>
<signal name="N$005">
<contactref element="R35" pad="2"/>
<contactref element="SW8" pad="DOWN"/>
</signal>
<signal name="N$007">
<contactref element="SW8" pad="COM"/>
<contactref element="R45" pad="CCW"/>
</signal>
<signal name="N$001">
<contactref element="R3" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="R6" pad="CCW"/>
</signal>
<signal name="N$011">
<contactref element="R8" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$048">
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="W"/>
</signal>
<signal name="N$049">
<contactref element="R9" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$054">
<contactref element="R9" pad="2"/>
<contactref element="IC4" pad="6"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$059">
<contactref element="IC4" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="SCAN">
<contactref element="SW7" pad="UP"/>
<contactref element="R10" pad="W"/>
</signal>
<signal name="CROSSING">
<contactref element="SW1" pad="!2"/>
<contactref element="SW1" pad="1"/>
<contactref element="IC4" pad="2"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="R10" pad="CCW"/>
</signal>
<signal name="N$008">
<contactref element="J3" pad="UPR-CTR"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="N$036">
<contactref element="J2" pad="LWR-CTR"/>
<contactref element="R50" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="R54" pad="2"/>
</signal>
<signal name="N$058">
<contactref element="R38" pad="1"/>
<contactref element="R39" pad="CW"/>
</signal>
<signal name="N$042">
<contactref element="R45" pad="W"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="N$066">
<contactref element="J2" pad="UPR-CTR"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="N$067">
<contactref element="C13" pad="2"/>
<contactref element="IC4" pad="7"/>
<contactref element="R5" pad="2"/>
<contactref element="R10" pad="CW"/>
</signal>
<signal name="N$025">
<contactref element="R51" pad="2"/>
<contactref element="J3" pad="LWR-CTR"/>
</signal>
<signal name="N$069">
<contactref element="R23" pad="1"/>
<contactref element="SW2" pad="DOWN"/>
</signal>
<signal name="N$070">
<contactref element="R6" pad="CW"/>
<contactref element="C8" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="D5" pad="3"/>
</signal>
<signal name="N$068">
<contactref element="PWR-LED" pad="TP"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="N$071">
<contactref element="LED+" pad="TP"/>
<contactref element="R53" pad="1"/>
</signal>
<signal name="N$024">
</signal>
<signal name="+10VA">
<contactref element="IC3" pad="3"/>
<contactref element="C6" pad="+"/>
<contactref element="R37" pad="1"/>
<contactref element="R36" pad="CW"/>
</signal>
<signal name="N$072">
<contactref element="C29" pad="2"/>
<contactref element="IC8" pad="7"/>
<contactref element="R29" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R53" pad="2"/>
<contactref element="R55" pad="2"/>
</signal>
<signal name="N$052">
<contactref element="C34" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C35" pad="2"/>
<contactref element="R55" pad="1"/>
</signal>
<signal name="N$065">
<contactref element="R18" pad="2"/>
<contactref element="SW2" pad="UP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
