<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="176.9" y2="0" width="0" layer="20"/>
<wire x1="176.9" y1="0" x2="176.9" y2="122" width="0" layer="20"/>
<wire x1="176.9" y1="122" x2="0" y2="122" width="0" layer="20"/>
<text>Tune</text>
<text>ALPS3 - Laser</text>
<text>Power Stabilization</text>
<text>A. Stummer Aug '12</text>
<text>0.18mm (7mil)</text>
<text>0.18mm (7mil)</text>
<text>0.4mm</text>
<text>0.25mm</text>
<text>ALPS3 - Laser Power Stabilization</text>
<text>University of Toronto</text>
<text>J. Thywissen Labs        Rev:C</text>
<wire x1="219" y1="54" x2="179" y2="54" width="0.18" layer="20"/>
<wire x1="179" y1="54" x2="179" y2="28" width="0.18" layer="20"/>
<wire x1="179" y1="28" x2="219" y2="28" width="0.18" layer="20"/>
<wire x1="219" y1="56" x2="219" y2="81" width="0.18" layer="20"/>
<wire x1="219" y1="81" x2="179" y2="81" width="0.18" layer="20"/>
<wire x1="179" y1="81" x2="179" y2="56" width="0.18" layer="20"/>
<wire x1="179" y1="56" x2="219" y2="56" width="0.18" layer="20"/>
<wire x1="219" y1="0" x2="219" y2="26" width="0.18" layer="20"/>
<wire x1="219" y1="26" x2="179" y2="26" width="0.18" layer="20"/>
<wire x1="179" y1="26" x2="179" y2="0" width="0.18" layer="20"/>
<wire x1="179" y1="0" x2="219" y2="0" width="0.18" layer="20"/>
<text>0.5A</text>
<text>RF</text>
<text>Level</text>
<text>Place</text>
<text>VCO</text>
<text>Offset</text>
<text>C</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<hole x="188" y="89" drill="3.86"/>
<hole x="188" y="128" drill="3.86"/>
<text>ALPS3 (C)</text>
<text>PD Log Amp</text>
<text>UofT</text>
<wire x1="219" y1="54" x2="219" y2="28" width="0.18" layer="20"/>
<wire x1="197" y1="134" x2="197" y2="83" width="0.18" layer="20"/>
<wire x1="179" y1="134" x2="179" y2="83" width="0.18" layer="20"/>
<wire x1="179" y1="83" x2="197" y2="83" width="0.18" layer="20"/>
<wire x1="179" y1="134" x2="197" y2="134" width="0.18" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="122" width="0" layer="20"/>
<text>University of Toronto</text>
<text>J. Thywissen Labs</text>
<text>MiniCir A06</text>
<text>VCO Plug-in (C)</text>
<text>University of Toronto</text>
<text>MiniCir A06</text>
<text>VCO Plug-in (C)</text>
<text>J. Thywissen Labs</text>
<wire x1="218" y1="127.2" x2="199.2" y2="127.2" width="0" layer="20"/>
<wire x1="199.2" y1="127.2" x2="199.2" y2="83" width="0" layer="20"/>
<wire x1="199.2" y1="83" x2="218" y2="83" width="0" layer="20"/>
<wire x1="218" y1="83" x2="218" y2="127.2" width="0" layer="20"/>
<hole x="216.23" y="125.43" drill="1.5113"/>
<hole x="200.99" y="125.43" drill="1.5113"/>
<hole x="200.99" y="84.79" drill="1.5113"/>
<hole x="216.23" y="84.79" drill="1.5113"/>
<text>Module</text>
<text>here</text>
<text>J. Thywissen Labs</text>
<text>MiniCir BK377</text>
<text>VCO Plug-in (C)</text>
<text>University of Toronto</text>
<text>D</text>
<text>Q</text>
<text>V</text>
<text>G</text>
<wire x1="0" y1="136" x2="0" y2="124" width="0.05" layer="20"/>
<wire x1="0" y1="124" x2="25" y2="124" width="0.05" layer="20"/>
<wire x1="25" y1="124" x2="25" y2="136" width="0.05" layer="20"/>
<wire x1="25" y1="136" x2="0" y2="136" width="0.05" layer="20"/>
<text>D</text>
<text>Q</text>
<text>V</text>
<text>G</text>
<wire x1="27" y1="136" x2="27" y2="124" width="0.05" layer="20"/>
<wire x1="27" y1="124" x2="52" y2="124" width="0.05" layer="20"/>
<wire x1="52" y1="124" x2="52" y2="136" width="0.05" layer="20"/>
<wire x1="52" y1="136" x2="27" y2="136" width="0.05" layer="20"/>
<text>D</text>
<text>Q</text>
<text>V</text>
<text>G</text>
<wire x1="54" y1="136" x2="54" y2="124" width="0.05" layer="20"/>
<wire x1="54" y1="124" x2="79" y2="124" width="0.05" layer="20"/>
<wire x1="79" y1="124" x2="79" y2="136" width="0.05" layer="20"/>
<wire x1="79" y1="136" x2="54" y2="136" width="0.05" layer="20"/>
<wire x1="25" y1="136" x2="27" y2="136" width="0" layer="20"/>
<wire x1="52" y1="136" x2="54" y2="136" width="0" layer="20"/>
<wire x1="79" y1="136" x2="219" y2="136" width="0" layer="20"/>
</plain>
<libraries>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="MSOP10">
<description>&lt;b&gt;MSOP-10&lt;/b&gt; with 4.8mm row spacing.  Sameas Maxim's µsop-10.</description>
</package>
<package name="QFN16#2">
<description>&lt;b&gt;QFN-16, AKA PVQFN-N16&lt;/b&gt;, from TI's LOG114, package RGV.</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, based on Kemet's description.</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire.  Has fence (bit larger than other TP) around to allow easier soldering.  Drilled 0.0465, plated down to 1.1mm.</description>
</package>
<package name="BOURNS:3296Y">
<description>&lt;b&gt;3296Y (multi, top adj), 3296Z (multi, side adj) or 3386X/H (1-turn, top) Trimpot&lt;/b&gt;, Bourns.  Staggered pins so can insert trimpot one way only.  http://www.bourns.com/pdf/3296.pdf</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;MSOP-8&lt;/b&gt;, A.K.A. RM-8.  Use 0.025" grid.</description>
</package>
<package name="CONN:BNC,DUAL(BOMAR)">
<description>&lt;b&gt;Dual BNC, vertical throughhole, isolated&lt;/b&gt;, Bomar, e.g. 364A2595, H=29.3mm, http://media.digikey.com/pdf/Data%20Sheets/Bomar%20PDFs/BNC_Products_Spec.pdf</description>
</package>
<package name="MINICIRCUITS_CD636">
<description>&lt;b&gt;Minicircuits cases CD541, CD542, CD636,CD637&lt;/b&gt;</description>
</package>
<package name="MINICIRCUITS_DV874">
<description>&lt;b&gt;Minicircuits DV874, SMD 16-pin&lt;/b&gt;, needs 0.02" vias in 4x4 grid.</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, based on TI's version of JEDEC MO-175 Variant AA.</description>
</package>
<package name="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)">
<description>&lt;b&gt;Socket for single pin, Harwin H3182-xx for 1mm pin&lt;/b&gt;</description>
</package>
<package name="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)">
<description>&lt;b&gt;CC1R5-inoutsR-E&lt;/b&gt;, TDK DC-DC isolated, 1.5W, uni- or bipolar&lt;br&gt;
"in": Input 05, 12, 24 or 48V.&lt;br&gt;
"out": Output 3.3, 5, 12, ±12 (or 24), ±15 (or30V).&lt;br&gt;
"s": Polarity single or dual.&lt;br&gt;
Case horiz SMD.&lt;br&gt;
http://www.tdk.co.jp/tefe02/ea335_cc_e.pdf</description>
</package>
<package name="TP-0.042C">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit 1mm pin such as Harwin H2710-xx.</description>
</package>
<package name="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)">
<description>&lt;b&gt;Test Point with 2mm (0.085") hole&lt;/b&gt;, to fit 2mm socket such as Harwin H8505-xx.</description>
</package>
<package name="CAP,PANASONIC_D8,SMT,6.3MMROUND">
<description>&lt;b&gt;Polarized cap, Panasonic D8 case (6.3mm dia)&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, based on Vishay.</description>
</package>
<package name="SWITCH:SPDT-DIP(COPAL)">
<description>&lt;b&gt;DIP (SMT) switch, SPDT&lt;/b&gt;, Copal CJS-1200, fits A1 (J-lead) and B1 (gullwing), http://media.digikey.com/pdf/Data%20Sheets/COPAL%20Electronics%20PDFs/CJS.pdf?cshift_ck=null&amp;client_id=5210&amp;cshift_ck=null&amp;client_id=5210</description>
</package>
<package name="CONN:BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, e.g. 5226990-3,  nut 1-329631-2, shoulder washer 330620.</description>
</package>
<package name="1608(0603)X2Y_DUAL">
<description>&lt;b&gt;X2Y dual cap in 1608 (old 0603)&lt;/b&gt;, for bypassing bipolar parts.&lt;br&gt;
Based on http://www.yageo.com/pdf/X2Y_series_12.pdf.</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="DPAK(CASE369C)">
<description>&lt;b&gt;DPAK, AKA Case 369C&lt;/b&gt;, based on On Semi specs.</description>
</package>
<package name="PAD,0.1X0.065(IN)">
<description>&lt;b&gt;SMT Pad, 0.1" x 0.065"&lt;/b&gt;, for Minircuits SMT packages.  Place one by one on the board as needed.</description>
</package>
<package name="BOURNS_3590">
<description>&lt;b&gt;Pot&lt;/b&gt;, 10-turn, Bourns 3590, mounted on side.  Panel, when mounted, is shown with diagonal lines.&lt;br&gt;
&lt;a href="http://www.bourns.com/pdf/3590.pdf"&gt;http://www.bourns.com/pdf/3590.pdf&lt;/a&gt;&lt;br&gt;
Also remember turns counting dial H-22-6a.</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="SWITCH,DP4T">
<description>&lt;b&gt;Electroswitch C2P0204N-A&lt;/b&gt;, DP4T RA PCB</description>
</package>
<package name="MINICIRCUITS_WW107">
<description>&lt;b&gt;Minicircuits WW107&lt;/b&gt;, for SMT hybrid darlington amps such as ERA-6SM.</description>
</package>
<package name="PANASONIC_EXB-V8V(QUAD-R-PACK)">
<description>&lt;b&gt;EXB-V8V-vvvJV&lt;/b&gt;, Panasonic quad resistor pack, each R is 0603, 5%,&lt;br&gt;
where value "vvv" is two significant digits and decade multiplier.&lt;br&gt;
http://www.panasonic.com/industrial/components/pdf/aoc0000ce1.pdf</description>
</package>
<package name="PHOTODIODE:3TERM">
<description>&lt;b&gt;Photodiode FDS010, Thorlabs&lt;/b&gt;</description>
</package>
<package name="CONN:SMA2">
<description>&lt;b&gt;SMA PCB, straight&lt;/b&gt;,e.g. jack Tyco 5-1814832-1, or plug 901-9895-RFX.</description>
</package>
<package name="SOIC-16">
<description>&lt;b&gt; SOIC-16&lt;/B&gt;, 0.05" pad spacing with 0.15" wide case.</description>
</package>
<package name="LIGHTPIPE,BIVAR_SMFLP">
<description>&lt;b&gt;Lightpipe for SMT LEDs&lt;/b&gt;, Bivar SMFLPx.x</description>
</package>
<package name="PLCC4">
<description>&lt;b&gt;PLCC-4&lt;/b&gt;, for LEDs, based on Optek OVSA1xBLCR8 series.</description>
</package>
<package name="MALLORY_MSR">
<description>&lt;b&gt;Audio Warning Device&lt;/b&gt;, Mallory MSR series, through hole, various sounds.&lt;br&gt;
Based on http://www.mallory-sonalert.com/Specifications/MSR516WR.pdf</description>
</package>
<package name="CASE:HAMMOND_1402DV">
<description>&lt;b&gt;Case, Hammond 1402DV&lt;/b&gt;, aluminum all around (Faraday cage).</description>
</package>
</packages>
</library>
<library name="MySMD">
<packages>
<package name="QFP032">
</package>
<package name="CAP0805-NP">
</package>
<package name="TAN-A">
</package>
<package name="SOT223">
</package>
<package name="LED0805">
</package>
<package name="SOD-123">
</package>
<package name="157SW">
</package>
<package name="RES4NT">
</package>
</packages>
</library>
<library name="MySMD2">
<packages>
<package name="SSOP28">
</package>
<package name="RESONATOR">
</package>
</packages>
</library>
<library name="MyCON2">
<packages>
<package name="USB-MINI-B_2">
</package>
<package name="HEAD15-NOSS">
</package>
<package name="HEAD15-NOSS-1">
</package>
<package name="HEAD3X2">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC6" library="QuantumOptics" package="MSOP10" value="VCA821IDGS">
<attribute name="NAME"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="453">
<attribute name="NAME"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R13" library="QuantumOptics" package="2012(0805)" value="453">
<attribute name="NAME"/>
</element>
<element name="GAIN" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="20">
<attribute name="NAME"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="IC5" library="QuantumOptics" package="MSOP8" value="ADG719BRM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J13" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value="364A2595"/>
<attribute name="NAME"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="RF1" library="QuantumOptics" package="MINICIRCUITS_CD636" value="ADP-2-1W+">
<attribute name="NAME"/>
</element>
<element name="RF2" library="QuantumOptics" package="MINICIRCUITS_DV874" value="RVA-2000V35">
<attribute name="MFG" value="Minicircuits"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R4" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="DESC" value="&quot;RF Level&quot;"/>
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J14" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value="364A2595"/>
<attribute name="NAME"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R35" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="C26" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R36" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="DESC" value="&quot;Offset&quot;"/>
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="J6" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J5" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J9" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="56pF">
<attribute name="NAME"/>
</element>
<element name="PA_+5V" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PA_+12V" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PA_NC" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PA_FM" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PA_RF" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PA_COM1" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="A_VDD" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="A_RF" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="A_COM1" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="A_COM2" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="A_COM3" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="A-COM4" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="A_TUNE" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="AGND" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="PA_COM2" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PA_COM3" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="C29" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C28" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J8" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J7" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="NAME"/>
</element>
<element name="FB2" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="FB4" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="FB3" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C17" library="QuantumOptics" package="1608(0603)X2Y_DUAL" value="0.1uF">
<attribute name="PN" value="CX0805MRX7R7BB104"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="PWR1" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1205SR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C36" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C35" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C37" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="12V_IN" library="QuantumOptics" package="TP-0.042B" value="5002"/>
<element name="12V_RETURN" library="QuantumOptics" package="TP-0.042B" value="5002"/>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.5A">
<attribute name="FUSE" value="fuse:???"/>
<attribute name="PN" value="2 x 100056"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C41" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC12" library="QuantumOptics" package="DPAK(CASE369C)" value="NCP1117DT50">
<attribute name="NAME"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="L1" library="QuantumOptics" package="2012(0805)" value="BLM21PG221SN1D">
<attribute name="DESC" value="220 Ohms @ 100MHz"/>
<attribute name="NAME"/>
</element>
<element name="L3" library="QuantumOptics" package="2012(0805)" value="BLM21PG221SN1D">
<attribute name="DESC" value="220 Ohms @ 100MHz"/>
<attribute name="NAME"/>
</element>
<element name="PB_+5V" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB+12V" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_-15V" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_RF" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_COM1" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_COM2" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_COM3" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="B_VDD" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_RF" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM1" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM3" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM5" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM7" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM9" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM11" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM2" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM4" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM6" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM8" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_COM10" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="B_TUNE" library="QuantumOptics" package="PAD,0.1X0.065(IN)" value="PAD-0.1X0.65IN"/>
<element name="R22" library="QuantumOptics" package="BOURNS_3590" value="10K">
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3590P-1-103L"/>
<attribute name="DESC" value="&quot;Manual&quot;"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC9" library="QuantumOptics" package="SOT23-5" value="AD8065ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R28" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
</element>
<element name="R37" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="R33" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="4.02K">
<attribute name="NAME"/>
</element>
<element name="OSC" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="U$82" library="QuantumOptics" package="TITLEBLOCK_PCB" value="">
<attribute name="LAST_DATE_TIME"/>
<attribute name="DRAWING_NAME"/>
</element>
<element name="PC_+5V" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PC_+12V" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PC_NC" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PC_FM" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PC_RF" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PC_COM1" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="C_VDD" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="C_RF" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="C_COM2" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="C_COM3" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="C_COM4" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="C-COM5" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="C_TUNE" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="C_COM1" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01"/>
<element name="PC_COM2" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PC_COM3" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="C21" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOIC-8" value="ADuM3210BRZ">
<attribute name="NAME"/>
</element>
<element name="C20" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="IC13" library="QuantumOptics" package="QFN16#2" value="LOG114AIRGV">
<attribute name="NAME"/>
</element>
<element name="R48" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="C47" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="NAME"/>
</element>
<element name="C38" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="NAME"/>
</element>
<element name="R47" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="DESC" value="&quot;Iref&quot;"/>
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="I-REF1" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R46" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R45" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="C43" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SW3" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="DESC" value="&quot;0dB Cal&quot;"/>
<attribute name="NAME"/>
</element>
<element name="C48" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="C39" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="C46" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C42" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="29.4K">
<attribute name="NAME"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="D6" library="QuantumOptics" package="SOT23" value="BAS70-04-V">
<attribute name="NAME"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="PD1" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD2" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD3" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD5" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD6" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD4" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PDEXT" library="QuantumOptics" package="MISC" value="HR10-7R-6S(73)">
<attribute name="MFG" value="Hirose"/>
<attribute name="PN" value=""/>
<attribute name="DESC" value="&quot;Remote PD&quot;"/>
<attribute name="NAME"/>
</element>
<element name="PX2" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PX3" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PX1" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PX5" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PX6" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PX4" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PDCON" library="QuantumOptics" package="MISC" value="HR10-7R-6S(73)">
<attribute name="DESC" value="&quot;Remote PD&quot;"/>
<attribute name="MFG" value="Hirose"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH,DP4T" value="C2P0204N-A">
<attribute name="MFG" value="Electroswitch"/>
<attribute name="NAME"/>
<attribute name="NOTE" value="Read notes on how to modify the switch for 4 position."/>
</element>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R27" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="IC1" library="QuantumOptics" package="SOIC-8" value="AD8274AR">
<attribute name="NAME"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="IC10" library="QuantumOptics" package="SOIC-8" value="AD8274AR">
<attribute name="NAME"/>
</element>
<element name="R31" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="R34" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C25" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="IC11" library="QuantumOptics" package="SOIC-8" value="AD8066ARZ">
<attribute name="NAME"/>
</element>
<element name="C24" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C27" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R30" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R29" library="QuantumOptics" package="2012(0805)" value="15K">
<attribute name="NAME"/>
</element>
<element name="R38" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="IC7" library="QuantumOptics" package="MINICIRCUITS_WW107" value="ERA-6SM">
<attribute name="NAME"/>
</element>
<element name="C15" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="NAME"/>
</element>
<element name="L2" library="QuantumOptics" package="2012(0805)" value="BLM21PG221SN1D">
<attribute name="DESC" value="220 Ohms @ 100MHz"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="Q3" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="Q2" library="QuantumOptics" package="SOT23" value="DMG2307L-7">
<attribute name="SECONDSOURCE" value="or similar"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="NAME"/>
</element>
<element name="R7" library="QuantumOptics" package="PANASONIC_EXB-V8V(QUAD-R-PACK)" value="10K">
<attribute name="NAME"/>
</element>
<element name="Q4" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="PD7" library="QuantumOptics" package="PHOTODIODE:3TERM" value="FDS100">
<attribute name="NAME"/>
</element>
<element name="PWR2" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1205SR-E">
<attribute name="NAME"/>
</element>
<element name="C44" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C45" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SPCR1" library="QuantumOptics" package="MISC" value="9908-312">
<attribute name="DESC" value="&quot;Remote PD&quot;"/>
<attribute name="MFG" value="Bivar Inc."/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SPCR2" library="QuantumOptics" package="MISC" value="9908-312">
<attribute name="DESC" value="&quot;Remote PD&quot;"/>
<attribute name="MFG" value="Bivar Inc."/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="Q1" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="D1" library="QuantumOptics" package="SOT23" value="BAS70-04-V">
<attribute name="NAME"/>
</element>
<element name="J10" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="J11" library="QuantumOptics" package="CONN:SMA2" value="5-1814832-1">
<attribute name="NAME"/>
</element>
<element name="COAX" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Crystek Corp."/>
<attribute name="PN" value="CCSMA-MM-086-8"/>
<attribute name="ALT" value="...or similar"/>
</element>
<element name="BLKHD" library="QuantumOptics" package="MISC" value="">
<attribute name="ALT" value="...or similar"/>
<attribute name="MFG" value="TE Connectivity"/>
<attribute name="PN" value="1054868-1"/>
</element>
<element name="J12" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="D2" library="QuantumOptics" package="SOT23" value="BAS70-04-V">
<attribute name="NAME"/>
</element>
<element name="IC3" library="QuantumOptics" package="MSOP8" value="ADG719BRM">
<attribute name="NAME"/>
</element>
<element name="FB1" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC15" library="QuantumOptics" package="SOT23-5" value="out">
<attribute name="ALT" value="NCP4623HSN120T1G"/>
<attribute name="NAME"/>
</element>
<element name="C49" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R14" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="DESC" value="&quot;RF Level&quot;"/>
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="IC14" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
</element>
<element name="C51" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R39" library="QuantumOptics" package="2012(0805)" value="15K">
<attribute name="NAME"/>
</element>
<element name="R41" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R49" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
</element>
<element name="R50" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R51" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C50" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R52" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="R53" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="C30" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C31" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC16" library="QuantumOptics" package="SOT23-5" value="out">
<attribute name="ALT" value="NCP4623HSN120T1G"/>
<attribute name="NAME"/>
</element>
<element name="C52" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R40" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="DESC" value="&quot;RF Level&quot;"/>
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="IC17" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
</element>
<element name="C53" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R42" library="QuantumOptics" package="2012(0805)" value="15K">
<attribute name="NAME"/>
</element>
<element name="R54" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R55" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
</element>
<element name="R56" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R57" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C54" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R58" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="R59" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="C32" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C33" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC18" library="QuantumOptics" package="SOT23-5" value="out">
<attribute name="ALT" value="NCP4623HSN120T1G"/>
<attribute name="NAME"/>
</element>
<element name="C55" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R43" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="DESC" value="&quot;RF Level&quot;"/>
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="IC19" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
</element>
<element name="C56" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R44" library="QuantumOptics" package="2012(0805)" value="15K">
<attribute name="NAME"/>
</element>
<element name="R60" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R61" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
</element>
<element name="R62" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R63" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C57" library="QuantumOptics" package="2012(0805)" value="1nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R64" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="R65" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="IC20" library="QuantumOptics" package="SOIC-16" value="MC74HC4538ADG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R66" library="QuantumOptics" package="2012(0805)" value="10k">
<attribute name="NAME"/>
</element>
<element name="Q5" library="QuantumOptics" package="SOT23" value="MMBT3906">
<attribute name="NAME"/>
</element>
<element name="C59" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R67" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R69" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C58" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="R70" library="QuantumOptics" package="2012(0805)" value="2.21M">
<attribute name="NAME"/>
</element>
<element name="C60" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="R71" library="QuantumOptics" package="2012(0805)" value="200K">
<attribute name="NAME"/>
</element>
<element name="LP1" library="QuantumOptics" package="LIGHTPIPE,BIVAR_SMFLP" value="SMFLP12.0">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="Q7" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="Q8" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="R72" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="LED1" library="QuantumOptics" package="PLCC4" value="OVSA1SBLCR8">
<attribute name="NAME"/>
</element>
<element name="AUD1" library="QuantumOptics" package="MALLORY_MSR" value="MSR516XR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="R68" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="CASE" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Hammond"/>
<attribute name="PN" value="1402DV"/>
<attribute name="NAME"/>
</element>
<element name="U$73" library="QuantumOptics" package="CASE:HAMMOND_1402DV" value=""/>
<element name="U1" library="MySMD" package="QFP032" value="ATMEGA168-20AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C61" library="MySMD" package="CAP0805-NP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="MySMD" package="CAP0805-NP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C63" library="MySMD" package="CAP0805-NP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C64" library="MySMD" package="TAN-A" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C65" library="MySMD" package="TAN-A" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C66" library="MySMD" package="CAP0805-NP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C67" library="MySMD" package="CAP0805-NP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="MySMD" package="SOT223" value="UA78M05">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="MySMD" package="LED0805" value="RED_RX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="MySMD" package="LED0805" value="GREEN_TX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="MySMD" package="LED0805" value="L_AMBER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="MySMD" package="LED0805" value="BLUE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="MySMD" package="SOD-123" value="MBR0520">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW4" library="MySMD" package="157SW" value="RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP1" library="MySMD" package="RES4NT" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP2" library="MySMD" package="RES4NT" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="MySMD2" package="SSOP28" value="FT232RL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J15" library="MyCON2" package="USB-MINI-B_2" value="USB-MINI-B%C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="MySMD2" package="RESONATOR" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J16" library="MyCON2" package="HEAD15-NOSS" value="HEAD15-NOSS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J17" library="MyCON2" package="HEAD15-NOSS-1" value="HEAD15-NOSS-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J18" library="MyCON2" package="HEAD3X2" value="HEAD3X2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$37" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$53" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="U$54" library="SparkFun" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="PB_FM1" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM2" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM3" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM4" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM5" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM6" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM7" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM8" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM9" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM10" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM11" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
<element name="PB_FM12" library="QuantumOptics" package="TP-0.042C" value="H2174-01"/>
</elements>
<signals>
<signal name="AGND">
<contactref element="R18" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="C16" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="IC5" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="RF1" pad="6"/>
<contactref element="RF2" pad="1"/>
<contactref element="RF2" pad="3"/>
<contactref element="RF2" pad="4"/>
<contactref element="RF2" pad="5"/>
<contactref element="RF2" pad="7"/>
<contactref element="RF2" pad="8"/>
<contactref element="RF2" pad="9"/>
<contactref element="RF2" pad="11"/>
<contactref element="RF2" pad="12"/>
<contactref element="RF2" pad="13"/>
<contactref element="RF2" pad="15"/>
<contactref element="RF2" pad="16"/>
<contactref element="C3" pad="1"/>
<contactref element="R4" pad="CCW"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="J9" pad="P$1"/>
<contactref element="J8" pad="P$1"/>
<contactref element="J7" pad="P$1"/>
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="FB3" pad="P$1"/>
<contactref element="C17" pad="COM2"/>
<contactref element="C17" pad="COM1"/>
<contactref element="C35" pad="1"/>
<contactref element="C37" pad="2"/>
<contactref element="C34" pad="NEG"/>
<contactref element="C36" pad="POS"/>
<contactref element="PWR1" pad="+VOUT"/>
<contactref element="IC12" pad="1"/>
<contactref element="PWR1" pad="-VIN"/>
<contactref element="PWR1" pad="RC"/>
<contactref element="12V_RETURN" pad="TP"/>
<contactref element="C41" pad="1"/>
<contactref element="C40" pad="NEG"/>
<contactref element="C18" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="IC9" pad="2"/>
<contactref element="R33" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="IC8" pad="5"/>
<contactref element="C20" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="PD2" pad="TP"/>
<contactref element="PD5" pad="TP"/>
<contactref element="PD4" pad="TP"/>
<contactref element="SW2" pad="BCOM"/>
<contactref element="IC1" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="IC11" pad="5"/>
<contactref element="R38" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC7" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="R7" pad="1A"/>
<contactref element="R7" pad="4A"/>
<contactref element="Q4" pad="2"/>
<contactref element="PWR2" pad="-VIN"/>
<contactref element="PWR2" pad="RC"/>
<contactref element="C7" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R22" pad="CCW"/>
<contactref element="J10" pad="SHIELD2"/>
<contactref element="J10" pad="SHIELD1"/>
<contactref element="J11" pad="COM4"/>
<contactref element="J11" pad="COM3"/>
<contactref element="J11" pad="COM2"/>
<contactref element="J11" pad="COM1"/>
<contactref element="IC4" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC3" pad="3"/>
<contactref element="C59" pad="1"/>
<contactref element="IC20" pad="1"/>
<contactref element="IC20" pad="15"/>
<contactref element="IC20" pad="8"/>
<contactref element="C58" pad="2"/>
<contactref element="C60" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q8" pad="2"/>
<contactref element="Q6" pad="2"/>
</signal>
<signal name="-5V">
<contactref element="R36" pad="CCW"/>
<contactref element="L3" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C36" pad="NEG"/>
<contactref element="PWR1" pad="COM"/>
<contactref element="PD6" pad="TP"/>
<contactref element="C25" pad="2"/>
<contactref element="IC10" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C27" pad="2"/>
<contactref element="IC11" pad="4"/>
</signal>
<signal name="+5V">
<contactref element="L1" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="IC5" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="RF2" pad="14"/>
<contactref element="R4" pad="CW"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="J3" pad="P$1"/>
<contactref element="R36" pad="CW"/>
<contactref element="C35" pad="2"/>
<contactref element="C34" pad="POS"/>
<contactref element="IC12" pad="2"/>
<contactref element="R22" pad="CW"/>
<contactref element="C22" pad="2"/>
<contactref element="IC9" pad="5"/>
<contactref element="R32" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="IC8" pad="8"/>
<contactref element="PD3" pad="TP"/>
<contactref element="C23" pad="2"/>
<contactref element="IC10" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="C24" pad="2"/>
<contactref element="IC11" pad="8"/>
<contactref element="R7" pad="2B"/>
<contactref element="R7" pad="3B"/>
<contactref element="C9" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC3" pad="4"/>
<contactref element="Q5" pad="2"/>
<contactref element="C59" pad="2"/>
<contactref element="IC20" pad="16"/>
<contactref element="IC20" pad="11"/>
<contactref element="R70" pad="2"/>
<contactref element="R71" pad="2"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED1" pad="1"/>
<contactref element="LED1" pad="3"/>
<contactref element="AUD1" pad="+"/>
<contactref element="R69" pad="2"/>
<contactref element="R68" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC6" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC7" pad="1"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC6" pad="7"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC6" pad="5"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC6" pad="6"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R17" pad="2"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="N$24">
<contactref element="IC6" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="GAIN" pad="TP"/>
</signal>
<signal name="N$27">
<contactref element="IC5" pad="1"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="J13" pad="UPR-CTR"/>
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="MANUAL">
<contactref element="IC8" pad="7"/>
<contactref element="IC3" pad="6"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R25" pad="1"/>
<contactref element="J13" pad="LWR-CTR"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="RF_OFF">
<contactref element="IC5" pad="6"/>
<contactref element="IC8" pad="6"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC6" pad="4"/>
<contactref element="RF2" pad="10"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R4" pad="W"/>
<contactref element="C5" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="J4" pad="P$1"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="COM-A">
<contactref element="IC8" pad="4"/>
<contactref element="J13" pad="LWR-COM"/>
<contactref element="J13" pad="UPR-COM"/>
<contactref element="C19" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C44" pad="NEG"/>
<contactref element="PWR2" pad="COM"/>
</signal>
<signal name="N$49">
<contactref element="R19" pad="1"/>
<contactref element="IC10" pad="5"/>
<contactref element="IC10" pad="6"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R35" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="IC11" pad="3"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="R35" pad="1"/>
<contactref element="R36" pad="W"/>
</signal>
<signal name="N$53">
<contactref element="R5" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="RF1" pad="4"/>
<contactref element="J10" pad="CONDUCTOR"/>
</signal>
<signal name="N$10">
<contactref element="RF2" pad="2"/>
<contactref element="RF1" pad="3"/>
</signal>
<signal name="N$57">
<contactref element="SW1" pad="COM"/>
<contactref element="RF1" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="J1" pad="CONDUCTOR"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="R15" pad="1"/>
<contactref element="J12" pad="CONDUCTOR"/>
</signal>
<signal name="N$11">
<contactref element="IC6" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="N$123">
<contactref element="IC6" pad="8"/>
<contactref element="C17" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="L3" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="A_RF" pad="TP"/>
<contactref element="PA_RF" pad="TP"/>
</signal>
<signal name="N$54">
<contactref element="A_VDD" pad="TP"/>
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="POS"/>
<contactref element="IC15" pad="1"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="VCOCOMA">
<contactref element="PA_COM1" pad="TP"/>
<contactref element="PA_COM2" pad="TP"/>
<contactref element="PA_COM3" pad="TP"/>
<contactref element="C29" pad="NEG"/>
<contactref element="C28" pad="1"/>
<contactref element="A_COM3" pad="TP"/>
<contactref element="A_COM1" pad="TP"/>
<contactref element="A_COM2" pad="TP"/>
<contactref element="A-COM4" pad="TP"/>
<contactref element="AGND" pad="TP"/>
<contactref element="C49" pad="1"/>
<contactref element="IC15" pad="2"/>
<contactref element="IC14" pad="2"/>
<contactref element="R50" pad="1"/>
<contactref element="R14" pad="CCW"/>
<contactref element="C50" pad="1"/>
<contactref element="R53" pad="1"/>
<contactref element="C51" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="Q2" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="PWR2" pad="+VIN"/>
<contactref element="PWR1" pad="+VIN"/>
<contactref element="F1" pad="2A"/>
<contactref element="C40" pad="POS"/>
<contactref element="C41" pad="2"/>
<contactref element="IC12" pad="3"/>
<contactref element="J2" pad="P$1"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="12V_IN" pad="TP"/>
<contactref element="F1" pad="1A"/>
</signal>
<signal name="VCOCOMB">
<contactref element="B_COM2" pad="1"/>
<contactref element="B_COM4" pad="1"/>
<contactref element="B_COM6" pad="1"/>
<contactref element="B_COM8" pad="1"/>
<contactref element="B_COM10" pad="1"/>
<contactref element="C32" pad="NEG"/>
<contactref element="C33" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="IC18" pad="2"/>
<contactref element="IC19" pad="2"/>
<contactref element="R62" pad="1"/>
<contactref element="R43" pad="CCW"/>
<contactref element="C57" pad="1"/>
<contactref element="R65" pad="1"/>
<contactref element="B_COM1" pad="1"/>
<contactref element="B_COM3" pad="1"/>
<contactref element="B_COM5" pad="1"/>
<contactref element="B_COM7" pad="1"/>
<contactref element="B_COM9" pad="1"/>
<contactref element="B_COM11" pad="1"/>
<contactref element="PB_COM1" pad="TP"/>
<contactref element="PB_COM2" pad="TP"/>
<contactref element="PB_COM3" pad="TP"/>
<contactref element="C56" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="R10" pad="1"/>
<contactref element="SW2" pad="ACOM"/>
</signal>
<signal name="N$56">
<contactref element="SW2" pad="A1"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="R22" pad="W"/>
<contactref element="C18" pad="2"/>
<contactref element="SW2" pad="A2"/>
</signal>
<signal name="N$73">
<contactref element="IC9" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="OSC" pad="TP"/>
<contactref element="SW2" pad="A4"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="SW1" pad="2"/>
<contactref element="J5" pad="P$1"/>
</signal>
<signal name="N$75">
<contactref element="IC9" pad="3"/>
<contactref element="R33" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="IC9" pad="4"/>
<contactref element="R28" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="SW2" pad="B3"/>
<contactref element="SW2" pad="B2"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="VCOCOMC">
<contactref element="C30" pad="NEG"/>
<contactref element="C31" pad="1"/>
<contactref element="C52" pad="1"/>
<contactref element="IC16" pad="2"/>
<contactref element="IC17" pad="2"/>
<contactref element="R56" pad="1"/>
<contactref element="R40" pad="CCW"/>
<contactref element="C54" pad="1"/>
<contactref element="R59" pad="1"/>
<contactref element="PC_COM1" pad="TP"/>
<contactref element="PC_COM2" pad="TP"/>
<contactref element="PC_COM3" pad="TP"/>
<contactref element="C_COM2" pad="TP"/>
<contactref element="C_COM3" pad="TP"/>
<contactref element="C_COM4" pad="TP"/>
<contactref element="C-COM5" pad="TP"/>
<contactref element="C_COM1" pad="TP"/>
<contactref element="C53" pad="1"/>
</signal>
<signal name="N$82">
<contactref element="IC5" pad="8"/>
<contactref element="R7" pad="1B"/>
<contactref element="R7" pad="2A"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$83">
</signal>
<signal name="N$23">
<contactref element="IC8" pad="2"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="IC8" pad="3"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC13" pad="3"/>
<contactref element="R48" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="R48" pad="1"/>
<contactref element="R47" pad="W"/>
<contactref element="I-REF1" pad="TP"/>
<contactref element="R46" pad="1"/>
<contactref element="C46" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="IC13" pad="16"/>
<contactref element="R47" pad="CW"/>
<contactref element="C43" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="IC13" pad="4"/>
<contactref element="SW3" pad="COM"/>
</signal>
<signal name="N$44">
<contactref element="IC13" pad="9"/>
<contactref element="PX2" pad="TP"/>
</signal>
<signal name="N$63">
<contactref element="IC13" pad="11"/>
<contactref element="IC13" pad="12"/>
</signal>
<signal name="N$91">
<contactref element="SW3" pad="1"/>
<contactref element="R46" pad="2"/>
</signal>
<signal name="N$92">
<contactref element="SW3" pad="2"/>
<contactref element="PD7" pad="ANODE"/>
</signal>
<signal name="N$93">
<contactref element="IC13" pad="14"/>
<contactref element="IC13" pad="15"/>
</signal>
<signal name="+5V-A">
<contactref element="IC8" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C45" pad="2"/>
<contactref element="C44" pad="POS"/>
<contactref element="PWR2" pad="+VOUT"/>
</signal>
<signal name="GND">
<contactref element="R47" pad="CCW"/>
<contactref element="IC13" pad="1"/>
<contactref element="IC13" pad="13"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="2"/>
<contactref element="C38" pad="1"/>
<contactref element="C39" pad="2"/>
<contactref element="IC13" pad="10"/>
<contactref element="C43" pad="1"/>
<contactref element="IC13" pad="5"/>
<contactref element="C46" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="D6" pad="3"/>
<contactref element="PX5" pad="TP"/>
<contactref element="PX4" pad="TP"/>
<contactref element="PD7" pad="CASE"/>
</signal>
<signal name="N$46">
<contactref element="R45" pad="1"/>
<contactref element="C42" pad="2"/>
<contactref element="PD7" pad="CATHODE"/>
</signal>
<signal name="N$95">
<contactref element="R45" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="IC13" pad="8"/>
<contactref element="C39" pad="1"/>
<contactref element="D6" pad="2"/>
<contactref element="PX1" pad="TP"/>
</signal>
<signal name="PID">
<contactref element="R5" pad="2"/>
<contactref element="FB4" pad="P$1"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="R66" pad="1"/>
</signal>
<signal name="N$96">
<contactref element="PD1" pad="TP"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="FB1" pad="P$1"/>
</signal>
<signal name="N$52">
<contactref element="IC13" pad="7"/>
<contactref element="PX3" pad="TP"/>
</signal>
<signal name="N$97">
<contactref element="R20" pad="2"/>
<contactref element="J12" pad="SHIELD2"/>
</signal>
<signal name="N$98">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$99">
<contactref element="IC1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$103">
<contactref element="IC10" pad="3"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="N$104">
<contactref element="IC10" pad="2"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$102">
<contactref element="R31" pad="1"/>
<contactref element="J14" pad="LWR-CTR"/>
</signal>
<signal name="N$105">
<contactref element="R34" pad="1"/>
<contactref element="J14" pad="LWR-COM"/>
</signal>
<signal name="N$100">
<contactref element="J14" pad="UPR-CTR"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$101">
<contactref element="R1" pad="1"/>
<contactref element="J14" pad="UPR-COM"/>
</signal>
<signal name="N$107">
<contactref element="IC11" pad="1"/>
<contactref element="IC11" pad="2"/>
<contactref element="IC10" pad="1"/>
</signal>
<signal name="N$106">
<contactref element="R30" pad="2"/>
<contactref element="IC11" pad="6"/>
<contactref element="R29" pad="1"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="IC6" pad="9"/>
<contactref element="R11" pad="2"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$110">
<contactref element="IC7" pad="3"/>
<contactref element="L2" pad="1"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="L2" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C12" pad="1"/>
<contactref element="J11" pad="CONDUCTOR"/>
</signal>
<signal name="N$29">
<contactref element="R8" pad="2"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$48">
<contactref element="Q2" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="C14" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="R7" pad="4B"/>
<contactref element="R7" pad="3A"/>
</signal>
<signal name="N$61">
<contactref element="Q3" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="D6" pad="1"/>
<contactref element="PX6" pad="TP"/>
<contactref element="C48" pad="1"/>
<contactref element="IC13" pad="PAD"/>
<contactref element="C47" pad="2"/>
<contactref element="IC13" pad="6"/>
<contactref element="IC13" pad="PADHOLE"/>
</signal>
<signal name="N$90">
</signal>
<signal name="N/C">
<contactref element="J6" pad="P$1"/>
</signal>
<signal name="N$112">
<contactref element="RF2" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R19" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="FB2" pad="P$1"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="IC11" pad="7"/>
<contactref element="D2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R29" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="SW2" pad="A3"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="IC14" pad="3"/>
<contactref element="R39" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="R53" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R14" pad="W"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="IC14" pad="4"/>
<contactref element="R50" pad="2"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="R49" pad="2"/>
<contactref element="IC14" pad="1"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="PA_+5V" pad="TP"/>
<contactref element="R14" pad="CW"/>
</signal>
<signal name="N$16">
<contactref element="R41" pad="1"/>
<contactref element="PA_FM" pad="TP"/>
</signal>
<signal name="N$22">
<contactref element="R51" pad="2"/>
<contactref element="A_TUNE" pad="TP"/>
<contactref element="C50" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="C51" pad="2"/>
<contactref element="IC14" pad="5"/>
<contactref element="IC15" pad="3"/>
<contactref element="IC15" pad="5"/>
<contactref element="C49" pad="2"/>
<contactref element="PA_+12V" pad="TP"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="C31" pad="2"/>
<contactref element="C30" pad="POS"/>
<contactref element="IC16" pad="1"/>
<contactref element="R58" pad="2"/>
<contactref element="C_VDD" pad="TP"/>
</signal>
<signal name="N$42">
<contactref element="IC17" pad="3"/>
<contactref element="R42" pad="2"/>
<contactref element="R54" pad="2"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="R40" pad="W"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="IC17" pad="4"/>
<contactref element="R56" pad="2"/>
<contactref element="R55" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="R55" pad="2"/>
<contactref element="IC17" pad="1"/>
<contactref element="R57" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="R40" pad="CW"/>
<contactref element="PC_+5V" pad="TP"/>
</signal>
<signal name="N$76">
<contactref element="R54" pad="1"/>
<contactref element="PC_FM" pad="TP"/>
</signal>
<signal name="N$77">
<contactref element="R57" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C_TUNE" pad="TP"/>
</signal>
<signal name="N$78">
<contactref element="C53" pad="2"/>
<contactref element="IC17" pad="5"/>
<contactref element="IC16" pad="3"/>
<contactref element="IC16" pad="5"/>
<contactref element="C52" pad="2"/>
<contactref element="R58" pad="1"/>
<contactref element="PC_+12V" pad="TP"/>
</signal>
<signal name="N$80">
<contactref element="PC_RF" pad="TP"/>
<contactref element="C_RF" pad="TP"/>
</signal>
<signal name="N$66">
<contactref element="C33" pad="2"/>
<contactref element="C32" pad="POS"/>
<contactref element="IC18" pad="1"/>
<contactref element="R64" pad="2"/>
<contactref element="B_VDD" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="IC19" pad="3"/>
<contactref element="R44" pad="2"/>
<contactref element="R60" pad="2"/>
<contactref element="R65" pad="2"/>
</signal>
<signal name="N$68">
<contactref element="R43" pad="W"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="IC19" pad="4"/>
<contactref element="R62" pad="2"/>
<contactref element="R61" pad="1"/>
</signal>
<signal name="N$72">
<contactref element="R61" pad="2"/>
<contactref element="IC19" pad="1"/>
<contactref element="R63" pad="1"/>
</signal>
<signal name="N$81">
<contactref element="R43" pad="CW"/>
<contactref element="PB_+5V" pad="TP"/>
</signal>
<signal name="N$113">
<contactref element="R60" pad="1"/>
<contactref element="PB_FM" pad="TP"/>
</signal>
<signal name="N$114">
<contactref element="R63" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="B_TUNE" pad="1"/>
</signal>
<signal name="N$115">
<contactref element="C56" pad="2"/>
<contactref element="IC19" pad="5"/>
<contactref element="IC18" pad="3"/>
<contactref element="IC18" pad="5"/>
<contactref element="C55" pad="2"/>
<contactref element="R64" pad="1"/>
<contactref element="PB+12V" pad="TP"/>
</signal>
<signal name="N$116">
<contactref element="PB_RF" pad="TP"/>
<contactref element="B_RF" pad="1"/>
</signal>
<signal name="N$94">
<contactref element="Q5" pad="1"/>
<contactref element="R66" pad="2"/>
</signal>
<signal name="N$117">
<contactref element="R67" pad="2"/>
<contactref element="Q5" pad="3"/>
<contactref element="IC20" pad="5"/>
</signal>
<signal name="N$33">
<contactref element="R26" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="!AUTO">
<contactref element="D1" pad="2"/>
<contactref element="SW2" pad="B1"/>
<contactref element="Q6" pad="1"/>
<contactref element="R68" pad="1"/>
</signal>
<signal name="N$119">
<contactref element="IC20" pad="4"/>
<contactref element="IC20" pad="12"/>
<contactref element="IC20" pad="6"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="N$120">
<contactref element="IC20" pad="10"/>
<contactref element="Q8" pad="1"/>
</signal>
<signal name="N$124">
<contactref element="C58" pad="1"/>
<contactref element="IC20" pad="2"/>
<contactref element="R70" pad="1"/>
</signal>
<signal name="N$121">
<contactref element="C60" pad="1"/>
<contactref element="R71" pad="1"/>
<contactref element="IC20" pad="14"/>
</signal>
<signal name="N$122">
<contactref element="Q7" pad="3"/>
<contactref element="R72" pad="1"/>
</signal>
<signal name="N$126">
<contactref element="R72" pad="2"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$125">
<contactref element="Q8" pad="3"/>
<contactref element="AUD1" pad="-"/>
</signal>
<signal name="N$37">
<contactref element="Q6" pad="3"/>
<contactref element="IC20" pad="3"/>
<contactref element="IC20" pad="13"/>
<contactref element="R69" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="J16" pad="8"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="J16" pad="7"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="J16" pad="6"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="J16" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="C63" pad="1"/>
<contactref element="SW4" pad="2"/>
<contactref element="U1" pad="29"/>
<contactref element="J17" pad="3"/>
<contactref element="J16" pad="3"/>
<contactref element="J18" pad="5"/>
<contactref element="RP1" pad="4"/>
</signal>
<signal name="D1/TX">
<contactref element="U1" pad="31"/>
<contactref element="J16" pad="1"/>
<contactref element="RP1" pad="3"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
<contactref element="J16" pad="9"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="J16" pad="10"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="12"/>
<contactref element="J16" pad="11"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
<contactref element="J16" pad="12"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="14"/>
<contactref element="J16" pad="13"/>
</signal>
<signal name="D11/MOSI">
<contactref element="U1" pad="15"/>
<contactref element="J16" pad="14"/>
<contactref element="J18" pad="4"/>
</signal>
<signal name="D12/MISO">
<contactref element="U1" pad="16"/>
<contactref element="J16" pad="15"/>
<contactref element="J18" pad="1"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="26"/>
<contactref element="J17" pad="9"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
<contactref element="J17" pad="10"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="24"/>
<contactref element="J17" pad="11"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="23"/>
<contactref element="J17" pad="12"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
<contactref element="J17" pad="8"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
<contactref element="J17" pad="7"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
<contactref element="J17" pad="6"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
<contactref element="J17" pad="5"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="20"/>
<contactref element="C61" pad="1"/>
<contactref element="J17" pad="13"/>
</signal>
<signal name="D13/SCK">
<contactref element="U1" pad="17"/>
<contactref element="J17" pad="15"/>
<contactref element="J18" pad="3"/>
<contactref element="RP2" pad="1"/>
</signal>
<signal name="COM">
<contactref element="C61" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C62" pad="2"/>
<contactref element="C64" pad="2"/>
<contactref element="C65" pad="2"/>
<contactref element="C67" pad="2"/>
<contactref element="C66" pad="2"/>
<contactref element="SW4" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="LED5" pad="1"/>
<contactref element="LED4" pad="1"/>
<contactref element="U2" pad="25"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="18"/>
<contactref element="U2" pad="21"/>
<contactref element="J15" pad="1"/>
<contactref element="Y1" pad="2"/>
<contactref element="J17" pad="2"/>
<contactref element="J16" pad="4"/>
<contactref element="J18" pad="6"/>
<contactref element="J15" pad="7"/>
<contactref element="J15" pad="9"/>
<contactref element="J15" pad="8"/>
<contactref element="J15" pad="6"/>
</signal>
<signal name="+5V1">
<contactref element="U3" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="C62" pad="1"/>
<contactref element="C64" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="J17" pad="4"/>
<contactref element="J18" pad="2"/>
<contactref element="RP1" pad="5"/>
<contactref element="U2" pad="20"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED3" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="RP2" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U3" pad="1"/>
<contactref element="J17" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="C66" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="J17" pad="14"/>
</signal>
<signal name="D0/RX">
<contactref element="U1" pad="30"/>
<contactref element="J16" pad="2"/>
<contactref element="RP1" pad="2"/>
</signal>
<signal name="VUSB">
<contactref element="D3" pad="2"/>
<contactref element="C65" pad="1"/>
<contactref element="C67" pad="1"/>
<contactref element="J15" pad="5"/>
</signal>
<signal name="N$69">
<contactref element="C63" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U2" pad="1"/>
<contactref element="RP1" pad="7"/>
</signal>
<signal name="TX">
<contactref element="U2" pad="5"/>
<contactref element="RP1" pad="6"/>
</signal>
<signal name="N$79">
<contactref element="U2" pad="15"/>
<contactref element="J15" pad="3"/>
</signal>
<signal name="N$111">
<contactref element="U2" pad="16"/>
<contactref element="J15" pad="4"/>
</signal>
<signal name="N$118">
<contactref element="LED5" pad="2"/>
<contactref element="RP2" pad="7"/>
</signal>
<signal name="N$127">
<contactref element="U2" pad="23"/>
<contactref element="RP2" pad="3"/>
</signal>
<signal name="N$128">
<contactref element="U2" pad="22"/>
<contactref element="RP2" pad="4"/>
</signal>
<signal name="N$129">
<contactref element="U2" pad="11"/>
</signal>
<signal name="N$130">
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$131">
<contactref element="U2" pad="8"/>
</signal>
<signal name="N$132">
<contactref element="U2" pad="9"/>
</signal>
<signal name="N$133">
<contactref element="U2" pad="10"/>
</signal>
<signal name="N$134">
<contactref element="U2" pad="28"/>
</signal>
<signal name="N$135">
<contactref element="U2" pad="27"/>
</signal>
<signal name="N$136">
<contactref element="U2" pad="24"/>
</signal>
<signal name="N$137">
<contactref element="U2" pad="13"/>
</signal>
<signal name="N$138">
<contactref element="U2" pad="14"/>
</signal>
<signal name="N$139">
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$140">
<contactref element="U2" pad="19"/>
</signal>
<signal name="N$141">
<contactref element="U2" pad="26"/>
</signal>
<signal name="N$142">
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$143">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$144">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="N$145">
<contactref element="RP1" pad="1"/>
</signal>
<signal name="N$146">
<contactref element="RP1" pad="8"/>
</signal>
<signal name="N$147">
<contactref element="RP2" pad="8"/>
<contactref element="LED4" pad="2"/>
</signal>
<signal name="N$148">
<contactref element="RP2" pad="6"/>
<contactref element="LED2" pad="1"/>
</signal>
<signal name="N$149">
<contactref element="RP2" pad="5"/>
<contactref element="LED3" pad="1"/>
</signal>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="S$3">
</signal>
<signal name="S$4">
</signal>
<signal name="S$5">
</signal>
<signal name="S$6">
</signal>
<signal name="S$8">
</signal>
<signal name="S$9">
</signal>
<signal name="S$10">
</signal>
<signal name="S$11">
</signal>
<signal name="S$12">
</signal>
<signal name="S$13">
</signal>
<signal name="S$14">
</signal>
<signal name="S$15">
</signal>
<signal name="S$16">
</signal>
<signal name="S$17">
</signal>
<signal name="S$18">
</signal>
<signal name="S$19">
</signal>
<signal name="S$20">
</signal>
<signal name="S$21">
</signal>
<signal name="S$22">
</signal>
<signal name="S$23">
</signal>
<signal name="S$24">
</signal>
<signal name="S$25">
</signal>
<signal name="S$26">
</signal>
<signal name="S$27">
</signal>
<signal name="S$28">
</signal>
<signal name="S$29">
</signal>
<signal name="S$30">
</signal>
<signal name="S$31">
</signal>
<signal name="S$32">
</signal>
<signal name="S$33">
</signal>
<signal name="S$34">
</signal>
<signal name="S$35">
</signal>
<signal name="S$36">
</signal>
<signal name="S$37">
</signal>
<signal name="S$38">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$41">
</signal>
<signal name="S$42">
</signal>
<signal name="S$43">
</signal>
<signal name="S$44">
</signal>
<signal name="S$45">
</signal>
<signal name="S$46">
</signal>
<signal name="S$47">
</signal>
<signal name="S$48">
</signal>
<signal name="S$49">
</signal>
<signal name="S$7">
</signal>
<signal name="S$50">
</signal>
<signal name="S$51">
</signal>
<signal name="S$52">
</signal>
<signal name="S$53">
</signal>
<signal name="S$54">
</signal>
<signal name="S$55">
</signal>
<signal name="S$57">
</signal>
<signal name="S$56">
</signal>
<signal name="S$58">
</signal>
<signal name="S$59">
</signal>
<signal name="S$60">
</signal>
<signal name="S$61">
</signal>
<signal name="S$62">
</signal>
<signal name="S$63">
</signal>
<signal name="S$83">
</signal>
<signal name="S$84">
</signal>
<signal name="S$88">
</signal>
<signal name="S$90">
</signal>
<signal name="S$64">
</signal>
<signal name="S$65">
</signal>
<signal name="S$66">
</signal>
<signal name="S$67">
</signal>
<signal name="S$68">
</signal>
<signal name="S$69">
</signal>
<signal name="S$70">
</signal>
<signal name="S$71">
</signal>
<signal name="S$72">
</signal>
<signal name="S$73">
</signal>
<signal name="S$74">
</signal>
<signal name="S$75">
</signal>
<signal name="S$76">
</signal>
<signal name="S$77">
</signal>
<signal name="S$78">
</signal>
<signal name="S$79">
</signal>
<signal name="S$80">
</signal>
<signal name="S$81">
</signal>
<signal name="S$82">
</signal>
<signal name="S$85">
</signal>
<signal name="S$86">
</signal>
<signal name="S$87">
</signal>
<signal name="S$89">
</signal>
<signal name="S$91">
</signal>
<signal name="S$92">
</signal>
<signal name="S$93">
</signal>
<signal name="S$94">
</signal>
<signal name="S$95">
</signal>
<signal name="S$96">
</signal>
<signal name="S$97">
</signal>
<signal name="S$98">
</signal>
<signal name="S$99">
</signal>
<signal name="S$100">
</signal>
<signal name="S$101">
</signal>
</signals>
</board>
</drawing>
</eagle>
