<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="176.9" y2="0" width="0" layer="20"/>
<wire x1="176.9" y1="0" x2="176.9" y2="122" width="0" layer="20"/>
<text>ALPS3 - Laser</text>
<text>Power Stabilization</text>
<text>A. Stummer Aug '12</text>
<text>0.18mm (7mil)</text>
<text>0.18mm (7mil)</text>
<text>0.4mm</text>
<text>0.25mm</text>
<text>ALPS3 - Laser Power Stabilization
J. Thywissen Labs        Rev:E
University of Toronto</text>
<text>0.5A</text>
<text>RF
Level</text>
<text>E</text>
<wire x1="0" y1="122" x2="176.9" y2="122" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="122" width="0" layer="20"/>
<wire x1="0" y1="135.6388" x2="0" y2="122" width="0" layer="20"/>
<text>Panelized with 0.3" (7.62mm) spaces between
boards for Alberta Printed Circuits APC.
</text>
</plain>
<libraries>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="MSOP10">
<description>&lt;b&gt;MSOP-10&lt;/b&gt;, JEDEC MO-187AB.  Sameas Maxim's µsop-10 and TI's VSSOP DGA (S-PDSO-G10).</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT.</description>
</package>
<package name="TP-0.060">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.060" (1.5mm) hole, to fit slightly larger test points. Has continious fence so will generate lots of DRCs which can be ignored.</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire. Has continious fence so will generate lots of DRCs which can be ignored.</description>
</package>
<package name="BOURNS:3296Y">
<description>&lt;b&gt;3296Y (multi, top adj), 3296Z (multi, side adj) or 3386X/H (1-turn, top) Trimpot&lt;/b&gt;, Bourns.  Staggered pins so can insert trimpot one way only.  http://www.bourns.com/pdf/3296.pdf</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;MSOP-8&lt;/b&gt;, A.K.A. RM-8.  Use 0.025" grid.</description>
</package>
<package name="CONN:BNC,DUAL(BOMAR)">
<description>&lt;b&gt;Dual BNC, vertical throughhole, isolated&lt;/b&gt;, Bomar, e.g. 364A2595, H=29.3mm, http://media.digikey.com/pdf/Data%20Sheets/Bomar%20PDFs/BNC_Products_Spec.pdf</description>
</package>
<package name="MINICIRCUITS_CD636">
<description>&lt;b&gt;Minicircuits cases CD541, CD542, CD636,CD637&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, based on TI's version of JEDEC MO-175 Variant AA.</description>
</package>
<package name="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)">
<description>&lt;b&gt;Socket for single pin, Harwin H3182-xx for 1mm pin&lt;/b&gt;</description>
</package>
<package name="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)">
<description>&lt;b&gt;CC1R5-inoutsR-E&lt;/b&gt;, TDK DC-DC isolated, 1.5W, uni- or bipolar&lt;br&gt;
"in": Input 05, 12, 24 or 48V.&lt;br&gt;
"out": Output 3.3, 5, 12, ±12 (or 24), ±15 (or30V).&lt;br&gt;
"s": Polarity single or dual.&lt;br&gt;
Case horiz SMD.&lt;br&gt;
http://www.tdk.co.jp/tefe02/ea335_cc_e.pdf</description>
</package>
<package name="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)">
<description>&lt;b&gt;Test Point with 2mm (0.085") hole&lt;/b&gt;, to fit 2mm socket such as Harwin H8505-xx.</description>
</package>
<package name="CAP,PANASONIC_D8,SMT,6.3MMROUND">
<description>&lt;b&gt;Polarized cap, Panasonic D8 case (6.3mm dia) and Cornell-Dubllier D and X (6.3mm dia)&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, based on Vishay.</description>
</package>
<package name="SWITCH:SPDT-DIP(COPAL)">
<description>&lt;b&gt;DIP (SMT) switch, SPDT&lt;/b&gt;, Copal CJS-1200, fits A1 (J-lead) and B1 (gullwing), or just solder pads.</description>
</package>
<package name="CONN:BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, e.g. 5226990-3,  nut 1-329631-2, shoulder washer 330620.</description>
</package>
<package name="1608(0603)X2Y_DUAL">
<description>&lt;b&gt;X2Y dual cap in 1608 (old 0603)&lt;/b&gt;, for bypassing bipolar parts.&lt;br&gt;
Based on http://www.yageo.com/pdf/X2Y_series_12.pdf.</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056 or lower profile 01110005MR.</description>
</package>
<package name="DPAK(CASE369C)">
<description>&lt;b&gt;DPAK, AKA Case 369C&lt;/b&gt;, based on On Semi specs.</description>
</package>
<package name="BOURNS_3590">
<description>&lt;b&gt;Pot&lt;/b&gt;, 10-turn, Bourns 3590, mounted on side.  Panel, when mounted, is shown with diagonal lines.&lt;br&gt;
&lt;a href="http://www.bourns.com/pdf/3590.pdf"&gt;http://www.bourns.com/pdf/3590.pdf&lt;/a&gt;&lt;br&gt;
Also remember turns counting dial H-22-6a.</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="SWITCH,DP4T">
<description>&lt;b&gt;Electroswitch C2P0204N-A&lt;/b&gt;, DP4T RA PCB</description>
</package>
<package name="MINICIRCUITS_WW107">
<description>&lt;b&gt;Minicircuits WW107&lt;/b&gt;, for SMT hybrid darlington amps such as ERA-6SM.</description>
</package>
<package name="PANASONIC_EXB-V8V(QUAD-R-PACK)">
<description>&lt;b&gt;EXB-V8V-vvvJV&lt;/b&gt;, Panasonic quad resistor pack, each R is 0603, 5%,&lt;br&gt;
where value "vvv" is two significant digits and decade multiplier.&lt;br&gt;
http://www.panasonic.com/industrial/components/pdf/aoc0000ce1.pdf</description>
</package>
<package name="SOIC-16">
<description>&lt;b&gt; SOIC-16&lt;/B&gt;, 0.05" pad spacing with 0.15" wide case.</description>
</package>
<package name="LIGHTPIPE,BIVAR_SMFLP">
<description>&lt;b&gt;Lightpipe for SMT LEDs&lt;/b&gt;, Bivar SMFLPx.x</description>
</package>
<package name="PLCC4">
<description>&lt;b&gt;PLCC-4&lt;/b&gt;, for LEDs, based on Optek OVSA1xBLCR8 series.</description>
</package>
<package name="MALLORY_MSR">
<description>&lt;b&gt;Audio Warning Device&lt;/b&gt;, Mallory MSR series, through hole, various sounds.&lt;br&gt;
Based on http://www.mallory-sonalert.com/Specifications/MSR516WR.pdf</description>
</package>
<package name="CASE:HAMMOND_1402DV">
<description>&lt;b&gt;Case, Hammond 1402DV&lt;/b&gt;, aluminum all around (Faraday cage).</description>
</package>
<package name="TRANSFORMER,PULSE_CX2___">
<description>&lt;b&gt;Transformer, Pulse CX2074/2147&lt;/b&gt;, centre tapped secondary.</description>
</package>
<package name="CONN,SMA2">
<description>&lt;b&gt;SMA PCB, straight&lt;/b&gt;,e.g. jack Tyco 5-1814832-1, or plug 901-9895-RFX.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC9" library="QuantumOptics" package="MSOP10" value="VCA82?IDGS">
<attribute name="NAME"/>
</element>
<element name="R36" library="QuantumOptics" package="2012(0805)" value="453">
<attribute name="NAME"/>
</element>
<element name="R33" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R34" library="QuantumOptics" package="2012(0805)" value="453">
<attribute name="NAME"/>
</element>
<element name="GAIN" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R35" library="QuantumOptics" package="2012(0805)" value="20">
<attribute name="NAME"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="IC11" library="QuantumOptics" package="MSOP8" value="ADG719BRM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Amphenol"/>
<attribute name="PN" value="112705"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="RF1" library="QuantumOptics" package="MINICIRCUITS_CD636" value="ADP-2-1W+">
<attribute name="NAME"/>
</element>
<element name="R27" library="QuantumOptics" package="BOURNS:3296Y" value="50">
<attribute name="DESC" value="&quot;RF Level&quot;"/>
<attribute name="PN" value="3296Y-1-500"/>
<attribute name="NAME"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Amphenol"/>
<attribute name="PN" value="112705"/>
<attribute name="NAME"/>
</element>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="10K/6.65K">
<attribute name="NAME"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="10K/4.99K">
<attribute name="NAME"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="VCO_VDD" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="VCO_RF" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="A_COM2" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="A_COM1" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="A_COM3" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="A-COM1" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="VCO_TUNE" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="AGND" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR0.8MM(HARWIN_H8505-XX)" value="H8505-01">
<attribute name="SPACER" value="9913-062"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="C25" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="NAME"/>
</element>
<element name="FB2" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="FB4" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C20" library="QuantumOptics" package="1608(0603)X2Y_DUAL" value="0.1uF">
<attribute name="PN" value="CX0805MRX7R7BB104"/>
<attribute name="NAME"/>
</element>
<element name="C19" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="PWR1" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1205SR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C29" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C31" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C32" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="12V_IN" library="QuantumOptics" package="TP-0.060" value="5002"/>
<element name="12V_RETURN" library="QuantumOptics" package="TP-0.060" value="5002"/>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.5A">
<attribute name="FUSE" value="fuse:???"/>
<attribute name="PN" value="2 x 01110005MR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C27" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC12" library="QuantumOptics" package="DPAK(CASE369C)" value="NCP1117DT50">
<attribute name="NAME"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="L1" library="QuantumOptics" package="2012(0805)" value="BLM21PG221SN1D">
<attribute name="DESC" value="220 Ohms @ 100MHz"/>
<attribute name="NAME"/>
</element>
<element name="L2" library="QuantumOptics" package="2012(0805)" value="BLM21PG221SN1D">
<attribute name="DESC" value="220 Ohms @ 100MHz"/>
<attribute name="NAME"/>
</element>
<element name="R26" library="QuantumOptics" package="BOURNS_3590" value="10K">
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="3590P-1-103L"/>
<attribute name="DESC" value="&quot;Manual&quot;"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R28" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R30" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
</element>
<element name="R29" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="4.02K">
<attribute name="NAME"/>
</element>
<element name="OSC" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="U$82" library="QuantumOptics" package="TITLEBLOCK_PCB" value="">
<attribute name="LAST_DATE_TIME"/>
<attribute name="DRAWING_NAME"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="IC3" library="QuantumOptics" package="SOIC-8" value="ADuM3210BRZ">
<attribute name="NAME"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="20K/3.32K">
<attribute name="NAME"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="PD1" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD2" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD3" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD5" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD6" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PD4" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PDEXT" library="QuantumOptics" package="MISC" value="HR10-7R-6S(73)">
<attribute name="MFG" value="Hirose"/>
<attribute name="PN" value=""/>
<attribute name="DESC" value="&quot;Remote PD&quot;"/>
<attribute name="NAME"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH,DP4T" value="C2P0204N-A">
<attribute name="MFG" value="Electroswitch"/>
<attribute name="NAME"/>
<attribute name="NOTE" value="Read notes on how to modify the switch for 4 position."/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="IC1" library="QuantumOptics" package="SOIC-8" value="AD8274AR">
<attribute name="NAME"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-8" value="AD8274AR">
<attribute name="NAME"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="6.04K">
<attribute name="NAME"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="15K">
<attribute name="NAME"/>
</element>
<element name="IC10" library="QuantumOptics" package="MINICIRCUITS_WW107" value="ERA-6SM">
<attribute name="NAME"/>
</element>
<element name="C21" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="NAME"/>
</element>
<element name="L3" library="QuantumOptics" package="2012(0805)" value="BLM21PG221SN1D">
<attribute name="DESC" value="220 Ohms @ 100MHz"/>
<attribute name="NAME"/>
</element>
<element name="R37" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="Q3" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="Q1" library="QuantumOptics" package="SOT23" value="DMG2307L-7">
<attribute name="SECONDSOURCE" value="or similar"/>
<attribute name="NAME"/>
</element>
<element name="R38" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C22" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="NAME"/>
</element>
<element name="R40" library="QuantumOptics" package="PANASONIC_EXB-V8V(QUAD-R-PACK)" value="10K">
<attribute name="NAME"/>
</element>
<element name="Q2" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="R39" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="PWR2" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1205SR-E">
<attribute name="NAME"/>
</element>
<element name="C30" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
<attribute name="NAME"/>
</element>
<element name="C33" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="200pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="D2" library="QuantumOptics" package="SOT23" value="BAS70-04-V">
<attribute name="NAME"/>
</element>
<element name="J5" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="COAX" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value=""/>
<attribute name="PN" value="CBA-SMAMR-SMAF"/>
<attribute name="ALT" value="...or similar"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="IC5" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="D1" library="QuantumOptics" package="SOT23" value="BAS70-04-V">
<attribute name="NAME"/>
</element>
<element name="IC7" library="QuantumOptics" package="MSOP8" value="ADG719BRM">
<attribute name="NAME"/>
</element>
<element name="FB1" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R13" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="DESC" value="&quot;RF Level&quot;"/>
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOT23-5" value="AD8065ART">
<attribute name="NAME"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="41.2K">
<attribute name="NAME"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="30.1K">
<attribute name="NAME"/>
</element>
<element name="IC14" library="QuantumOptics" package="SOIC-16" value="MC74HC4538ADG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="QuantumOptics" package="2012(0805)" value="10k">
<attribute name="NAME"/>
</element>
<element name="Q4" library="QuantumOptics" package="SOT23" value="MMBT3906">
<attribute name="NAME"/>
</element>
<element name="C43" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R45" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R48" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C38" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="R49" library="QuantumOptics" package="2012(0805)" value="2.21M">
<attribute name="NAME"/>
</element>
<element name="C42" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value="08053C225KAT2A"/>
<attribute name="NAME"/>
</element>
<element name="R50" library="QuantumOptics" package="2012(0805)" value="200K">
<attribute name="NAME"/>
</element>
<element name="LP1" library="QuantumOptics" package="LIGHTPIPE,BIVAR_SMFLP" value="SMFLP12.0">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="Q6" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="Q7" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="R51" library="QuantumOptics" package="2012(0805)" value="453">
<attribute name="NAME"/>
</element>
<element name="LED1" library="QuantumOptics" package="PLCC4" value="OVSA1SBLCR8">
<attribute name="NAME"/>
</element>
<element name="AUD1" library="QuantumOptics" package="MALLORY_MSR" value="MSR516XR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="QuantumOptics" package="SOT23" value="2N7002L">
<attribute name="NAME"/>
</element>
<element name="R46" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="U$73" library="QuantumOptics" package="CASE:HAMMOND_1402DV" value=""/>
<element name="D3" library="QuantumOptics" package="SOT23" value="BAS70-04-V">
<attribute name="NAME"/>
</element>
<element name="R31" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="TR1" library="QuantumOptics" package="TRANSFORMER,PULSE_CX2___" value="CX2147NL">
<attribute name="NAME"/>
</element>
<element name="J6" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="FB3" library="QuantumOptics" package="CONN,RECEPTCLE,SINGLE,FOR1MM(HARWIN_H3182-XX)" value="H3182-xx">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Harwin"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="out/10K">
<attribute name="NAME"/>
</element>
<element name="CASE" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Hammond"/>
<attribute name="PN" value="1402DV"/>
<attribute name="NAME"/>
</element>
<element name="WWART" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="CUI"/>
<attribute name="PN" value="EPSA120100U-P6P-EJ"/>
<attribute name="NAME"/>
</element>
<element name="KNOB2" library="QuantumOptics" package="MISC" value="PKG50B1/8">
<attribute name="MFG" value="Tyco"/>
<attribute name="PN" value="???"/>
<attribute name="NAME"/>
</element>
<element name="SW4" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="???"/>
<attribute name="PN" value="???"/>
<attribute name="NAME"/>
</element>
<element name="KNOB1" library="QuantumOptics" package="MISC" value="PKE60B1/4">
<attribute name="MFG" value="Tyco"/>
<attribute name="PN" value="???"/>
<attribute name="NAME"/>
</element>
<element name="J7" library="QuantumOptics" package="CONN,SMA2" value="5-1814832-1">
<attribute name="NAME"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="15K">
<attribute name="NAME"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="16.2K">
<attribute name="NAME"/>
</element>
<element name="IC6" library="QuantumOptics" package="SOT23-5" value="AD8065ART">
<attribute name="NAME"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="GROM" library="QuantumOptics" package="MISC" value="">
<attribute name="MFG" value="Keystone"/>
<attribute name="PN" value="733"/>
</element>
<element name="SPCRS" library="QuantumOptics" package="MISC" value="4 of 9913-062">
<attribute name="ALT" value="...or similar"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value="CBA-SMAMR-SMAF"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="R33" pad="1"/>
<contactref element="R35" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="IC11" pad="3"/>
<contactref element="C24" pad="1"/>
<contactref element="RF1" pad="6"/>
<contactref element="R27" pad="CCW"/>
<contactref element="R25" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="J4" pad="SHIELD2"/>
<contactref element="J4" pad="SHIELD1"/>
<contactref element="C20" pad="COM2"/>
<contactref element="C20" pad="COM1"/>
<contactref element="C31" pad="1"/>
<contactref element="C32" pad="2"/>
<contactref element="C28" pad="NEG"/>
<contactref element="C29" pad="POS"/>
<contactref element="PWR1" pad="+VOUT"/>
<contactref element="IC12" pad="1"/>
<contactref element="PWR1" pad="-VIN"/>
<contactref element="PWR1" pad="RC"/>
<contactref element="12V_RETURN" pad="TP"/>
<contactref element="C27" pad="1"/>
<contactref element="C26" pad="NEG"/>
<contactref element="C15" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="IC8" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="IC3" pad="5"/>
<contactref element="C7" pad="1"/>
<contactref element="PD2" pad="TP"/>
<contactref element="PD5" pad="TP"/>
<contactref element="PD4" pad="TP"/>
<contactref element="SW2" pad="BCOM"/>
<contactref element="IC1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC10" pad="4"/>
<contactref element="IC10" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="R40" pad="1A"/>
<contactref element="R40" pad="4A"/>
<contactref element="Q2" pad="2"/>
<contactref element="PWR2" pad="-VIN"/>
<contactref element="PWR2" pad="RC"/>
<contactref element="C23" pad="1"/>
<contactref element="R26" pad="CCW"/>
<contactref element="J5" pad="SHIELD2"/>
<contactref element="J5" pad="SHIELD1"/>
<contactref element="IC5" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC7" pad="3"/>
<contactref element="C43" pad="1"/>
<contactref element="IC14" pad="1"/>
<contactref element="IC14" pad="15"/>
<contactref element="IC14" pad="8"/>
<contactref element="C38" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="FB3" pad="P$1"/>
<contactref element="J7" pad="COM4"/>
<contactref element="J7" pad="COM1"/>
<contactref element="J7" pad="COM3"/>
<contactref element="J7" pad="COM2"/>
<contactref element="AGND" pad="TP"/>
<contactref element="A_COM1" pad="TP"/>
<contactref element="A_COM3" pad="TP"/>
<contactref element="A_COM2" pad="TP"/>
<contactref element="A-COM1" pad="TP"/>
<contactref element="IC4" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="IC6" pad="3"/>
</signal>
<signal name="-5V">
<contactref element="L2" pad="1"/>
<contactref element="C32" pad="1"/>
<contactref element="C29" pad="NEG"/>
<contactref element="PWR1" pad="COM"/>
<contactref element="PD6" pad="TP"/>
<contactref element="C5" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="R32" pad="1"/>
<contactref element="R13" pad="CCW"/>
<contactref element="C11" pad="2"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="L1" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="IC11" pad="4"/>
<contactref element="C31" pad="2"/>
<contactref element="C28" pad="POS"/>
<contactref element="IC12" pad="2"/>
<contactref element="R26" pad="CW"/>
<contactref element="C17" pad="2"/>
<contactref element="IC8" pad="5"/>
<contactref element="R23" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC3" pad="8"/>
<contactref element="PD3" pad="TP"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="R40" pad="2B"/>
<contactref element="R40" pad="3B"/>
<contactref element="C9" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC7" pad="4"/>
<contactref element="C43" pad="2"/>
<contactref element="IC14" pad="16"/>
<contactref element="IC14" pad="11"/>
<contactref element="R49" pad="2"/>
<contactref element="R50" pad="2"/>
<contactref element="LED1" pad="2"/>
<contactref element="LED1" pad="1"/>
<contactref element="LED1" pad="3"/>
<contactref element="AUD1" pad="+"/>
<contactref element="R48" pad="2"/>
<contactref element="R46" pad="2"/>
<contactref element="Q4" pad="3"/>
<contactref element="R13" pad="CW"/>
<contactref element="R8" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="IC9" pad="1"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC10" pad="1"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC9" pad="7"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC9" pad="5"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="IC9" pad="6"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R35" pad="2"/>
<contactref element="IC9" pad="10"/>
</signal>
<signal name="N$24">
<contactref element="R22" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="GAIN" pad="TP"/>
<contactref element="R31" pad="1"/>
<contactref element="TR1" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="IC11" pad="1"/>
<contactref element="C25" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="J2" pad="UPR-CTR"/>
<contactref element="R7" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="MANUAL">
<contactref element="IC3" pad="7"/>
<contactref element="IC7" pad="6"/>
<contactref element="R45" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R12" pad="1"/>
<contactref element="J2" pad="LWR-CTR"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="RF_OFF">
<contactref element="IC11" pad="6"/>
<contactref element="IC3" pad="6"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC9" pad="4"/>
<contactref element="R27" pad="W"/>
</signal>
<signal name="N$43">
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="6"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="COM-A">
<contactref element="IC3" pad="4"/>
<contactref element="J2" pad="LWR-COM"/>
<contactref element="J2" pad="UPR-COM"/>
<contactref element="C3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C30" pad="NEG"/>
<contactref element="PWR2" pad="COM"/>
</signal>
<signal name="N$49">
<contactref element="R19" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="6"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="R21" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="RF1" pad="4"/>
<contactref element="J5" pad="CONDUCTOR"/>
</signal>
<signal name="N$10">
<contactref element="RF1" pad="3"/>
<contactref element="R27" pad="CW"/>
</signal>
<signal name="N$57">
<contactref element="SW1" pad="COM"/>
<contactref element="RF1" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="J4" pad="CONDUCTOR"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="CONDUCTOR"/>
</signal>
<signal name="N$11">
<contactref element="IC9" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="N$123">
<contactref element="IC9" pad="8"/>
<contactref element="C20" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="Q1" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="PWR2" pad="+VIN"/>
<contactref element="PWR1" pad="+VIN"/>
<contactref element="F1" pad="2A"/>
<contactref element="C26" pad="POS"/>
<contactref element="C27" pad="2"/>
<contactref element="IC12" pad="3"/>
<contactref element="R39" pad="2"/>
<contactref element="F1" pad="2B"/>
<contactref element="C6" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="VCO_VDD" pad="TP"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="12V_IN" pad="TP"/>
<contactref element="F1" pad="1A"/>
<contactref element="F1" pad="1B"/>
</signal>
<signal name="N$47">
<contactref element="R22" pad="1"/>
<contactref element="SW2" pad="ACOM"/>
</signal>
<signal name="N$56">
<contactref element="SW2" pad="A1"/>
<contactref element="IC7" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="R26" pad="W"/>
<contactref element="C15" pad="2"/>
<contactref element="SW2" pad="A2"/>
</signal>
<signal name="N$73">
<contactref element="IC8" pad="1"/>
<contactref element="R29" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="OSC" pad="TP"/>
<contactref element="SW2" pad="A4"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="SW1" pad="2"/>
<contactref element="VCO_RF" pad="TP"/>
</signal>
<signal name="N$75">
<contactref element="IC8" pad="3"/>
<contactref element="R24" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$74">
<contactref element="IC8" pad="4"/>
<contactref element="R28" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="SW2" pad="B3"/>
<contactref element="SW2" pad="B2"/>
<contactref element="D2" pad="3"/>
</signal>
<signal name="N$82">
<contactref element="IC11" pad="8"/>
<contactref element="R40" pad="1B"/>
<contactref element="R40" pad="2A"/>
<contactref element="C23" pad="2"/>
</signal>
<signal name="N$83">
</signal>
<signal name="N$23">
<contactref element="IC3" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="IC3" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="+5V-A">
<contactref element="IC3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="C30" pad="POS"/>
<contactref element="PWR2" pad="+VOUT"/>
</signal>
<signal name="PID">
<contactref element="R21" pad="2"/>
<contactref element="FB4" pad="P$1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC7" pad="2"/>
<contactref element="R43" pad="1"/>
</signal>
<signal name="N$96">
<contactref element="PD1" pad="TP"/>
<contactref element="R17" pad="2"/>
<contactref element="FB1" pad="P$1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$98">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$99">
<contactref element="IC1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$103">
<contactref element="IC2" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$104">
<contactref element="IC2" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$102">
<contactref element="R9" pad="1"/>
<contactref element="J3" pad="LWR-CTR"/>
</signal>
<signal name="N$105">
<contactref element="R11" pad="1"/>
<contactref element="J3" pad="LWR-COM"/>
</signal>
<signal name="N$100">
<contactref element="J3" pad="UPR-CTR"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$101">
<contactref element="R1" pad="1"/>
<contactref element="J3" pad="UPR-COM"/>
</signal>
<signal name="N$106">
<contactref element="R18" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="IC6" pad="4"/>
</signal>
<signal name="N$108">
<contactref element="IC9" pad="9"/>
<contactref element="R36" pad="2"/>
<contactref element="C21" pad="2"/>
</signal>
<signal name="N$110">
<contactref element="IC10" pad="3"/>
<contactref element="L3" pad="1"/>
<contactref element="C22" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="L3" pad="2"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C25" pad="1"/>
<contactref element="J7" pad="CONDUCTOR"/>
</signal>
<signal name="N$29">
<contactref element="R37" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$48">
<contactref element="Q1" pad="1"/>
<contactref element="R38" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="C22" pad="1"/>
<contactref element="IC11" pad="2"/>
<contactref element="R40" pad="4B"/>
<contactref element="R40" pad="3A"/>
</signal>
<signal name="N$61">
<contactref element="Q3" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="N$90">
</signal>
<signal name="N$1">
<contactref element="R19" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="FB2" pad="P$1"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="3"/>
<contactref element="IC6" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R20" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="SW2" pad="A3"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="N$38">
<contactref element="IC4" pad="4"/>
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$94">
<contactref element="Q4" pad="1"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$117">
<contactref element="R45" pad="2"/>
<contactref element="IC14" pad="5"/>
<contactref element="Q4" pad="2"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="R30" pad="1"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="!AUTO">
<contactref element="D2" pad="2"/>
<contactref element="SW2" pad="B1"/>
<contactref element="Q5" pad="1"/>
<contactref element="R46" pad="1"/>
</signal>
<signal name="N$119">
<contactref element="IC14" pad="4"/>
<contactref element="IC14" pad="12"/>
<contactref element="IC14" pad="6"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="N$120">
<contactref element="IC14" pad="10"/>
<contactref element="Q7" pad="1"/>
</signal>
<signal name="N$124">
<contactref element="C38" pad="1"/>
<contactref element="IC14" pad="2"/>
<contactref element="R49" pad="1"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="N$121">
<contactref element="C42" pad="1"/>
<contactref element="R50" pad="1"/>
<contactref element="IC14" pad="14"/>
</signal>
<signal name="N$122">
<contactref element="Q6" pad="3"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$126">
<contactref element="R51" pad="2"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$125">
<contactref element="Q7" pad="3"/>
<contactref element="AUD1" pad="-"/>
</signal>
<signal name="N$37">
<contactref element="Q5" pad="3"/>
<contactref element="IC14" pad="3"/>
<contactref element="IC14" pad="13"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="S$30">
</signal>
<signal name="S$32">
</signal>
<signal name="S$33">
</signal>
<signal name="S$34">
</signal>
<signal name="S$36">
</signal>
<signal name="S$37">
</signal>
<signal name="S$46">
</signal>
<signal name="S$47">
</signal>
<signal name="S$48">
</signal>
<signal name="S$49">
</signal>
<signal name="S$83">
</signal>
<signal name="S$84">
</signal>
<signal name="S$88">
</signal>
<signal name="S$90">
</signal>
<signal name="N$69">
<contactref element="R31" pad="2"/>
<contactref element="IC9" pad="3"/>
<contactref element="TR1" pad="1"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="N$79">
<contactref element="J6" pad="SHIELD2"/>
<contactref element="J6" pad="SHIELD1"/>
<contactref element="TR1" pad="4"/>
</signal>
<signal name="N$84">
<contactref element="J6" pad="CONDUCTOR"/>
<contactref element="TR1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="R15" pad="2"/>
<contactref element="IC4" pad="1"/>
<contactref element="VCO_TUNE" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R13" pad="W"/>
<contactref element="R16" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
