<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="167" y2="0" width="0" layer="20"/>
<wire x1="167" y1="0" x2="167" y2="140.6" width="0" layer="20"/>
<wire x1="167" y1="140.6" x2="0" y2="140.6" width="0" layer="20"/>
<wire x1="0" y1="140.6" x2="0" y2="0" width="0" layer="20"/>
<text>12V+</text>
<text>12V-</text>
<text>0.5A</text>
<text>Quad Analog Isolator 2</text>
<text>J. Thywissen Labs</text>
<text>University of Toronto</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>Rev:A</text>
<text>Quad Analog Isolator 2</text>
<text>A</text>
<text>A. Stummer Oct '12</text>
<text>0.18mm</text>
<text>0.5mm</text>
<text>0.18mm</text>
<text>0.25mm</text>
</plain>
<libraries>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="SOIC28B">
<description>&lt;b&gt; SOIC-28, isolation version&lt;/B&gt;, missing centre pins, for Avago ISO12x isolation amps.  http://focus.ti.com/lit/ds/symlink/iso124.pdf</description>
</package>
<package name="2917(7343)">
<description>&lt;b&gt;2917 (7343) SMT package&lt;/b&gt;, using medium density (nominal footprint) from Kemet.</description>
</package>
<package name="CAP,POL,8MM,PLASTIC_BASE">
<description>&lt;b&gt;Capacitor, polarized, 8mm SMT on plastic base&lt;/b&gt;, e.g. Nippon Chemi-con Corp, H70, H80 and HA0 packages, and, Nichicon 8mm.</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, 0.075" c-c pad spacing.  Preferred grid is 0.025".</description>
</package>
<package name="BOURNS_3214">
<description>&lt;b&gt;Trimpot, Bourns 3214W&lt;/b&gt;, 5-turn, top adjust, SMT.&lt;br&gt;
http://www.bourns.com/PDFs/3214.pdf</description>
</package>
<package name="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)">
<description>&lt;b&gt;CC1R5-inoutsR-E&lt;/b&gt;, TDK DC-DC isolated, 1.5W, uni- or bipolar&lt;br&gt;
"in": Input 05, 12, 24 or 48V.&lt;br&gt;
"out": Output 3.3, 5, 12, ±12 (or 24), ±15 (or30V).&lt;br&gt;
"s": Polarity single or dual.&lt;br&gt;
Case horiz SMD.&lt;br&gt;
http://www.tdk.co.jp/tefe02/ea335_cc_e.pdf</description>
</package>
<package name="CONN:BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, e.g. 5226990-3,  nut 1-329631-2, shoulder washer 330620.</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="CASE:HAMMOND_1598C">
<description>&lt;b&gt;PCB to fit case, Hammond 1598C&lt;/b&gt;.  Plastic clamshell case.  Four PCB short mounting posts.&lt;br&gt;
Vertical clearance PCB to inside of lid = 40.5mm.&lt;br&gt;
http://www.hammondmfg.com/pdf/1598C.pdf (nice graphics!)</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire.  Has fence (bit larger than other TP) around to allow easier soldering.</description>
</package>
<package name="SWITCH:SPDT-DIP(COPAL)">
<description>&lt;b&gt;DIP (SMT) switch, SPDT&lt;/b&gt;, Copal CJS-1200, fits A1 (J-lead) and B1 (gullwing), http://media.digikey.com/pdf/Data%20Sheets/COPAL%20Electronics%20PDFs/CJS.pdf?cshift_ck=null&amp;client_id=5210&amp;cshift_ck=null&amp;client_id=5210</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="QuantumOptics" package="SOIC28B" value="ISO124U">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QuantumOptics" package="2917(7343)" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="QuantumOptics" package="2917(7343)" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="QuantumOptics" package="2917(7343)" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="QuantumOptics" package="2917(7343)" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="QuantumOptics" package="BOURNS_3214" value="50K">
<attribute name="MFG" value=""/>
<attribute name="PN" value="3214W-1-503E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
</element>
<element name="PWR1" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;In 1&quot;"/>
<attribute name="NAME"/>
</element>
<element name="PWR2" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="4.99K">
<attribute name="NAME"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="680pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="270pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;Out 1&quot;"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="U$1" library="QuantumOptics" package="CASE:HAMMOND_1598C" value=""/>
<element name="IC3" library="QuantumOptics" package="SOIC28B" value="ISO124U">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C17" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C18" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C21" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C22" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="QuantumOptics" package="BOURNS_3214" value="50K">
<attribute name="MFG" value=""/>
<attribute name="PN" value="3214W-1-503E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
</element>
<element name="PWR3" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;In 2&quot;"/>
<attribute name="NAME"/>
</element>
<element name="PWR4" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="4.99K">
<attribute name="NAME"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C25" library="QuantumOptics" package="2012(0805)" value="680pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C26" library="QuantumOptics" package="2012(0805)" value="270pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C27" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C28" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;Out 2&quot;"/>
<attribute name="NAME"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="IC5" library="QuantumOptics" package="SOIC28B" value="ISO124U">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C31" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C32" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C35" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C36" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="QuantumOptics" package="BOURNS_3214" value="50K">
<attribute name="MFG" value=""/>
<attribute name="PN" value="3214W-1-503E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
</element>
<element name="PWR5" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J5" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;In 3&quot;"/>
<attribute name="NAME"/>
</element>
<element name="PWR6" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="4.99K">
<attribute name="NAME"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C39" library="QuantumOptics" package="2012(0805)" value="680pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C40" library="QuantumOptics" package="2012(0805)" value="270pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC6" library="QuantumOptics" package="SOIC-8" value="AD8671ARZ">
<attribute name="NAME"/>
</element>
<element name="C41" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C42" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J6" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;Out 3&quot;"/>
<attribute name="NAME"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="IC7" library="QuantumOptics" package="SOIC28B" value="ISO124U">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C45" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C46" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C49" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C50" library="QuantumOptics" package="CAP,POL,8MM,PLASTIC_BASE" value="22uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="A700D226M016ATE018"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="QuantumOptics" package="BOURNS_3214" value="50K">
<attribute name="MFG" value=""/>
<attribute name="PN" value="3214W-1-503E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
</element>
<element name="PWR7" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J7" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;In 4&quot;"/>
<attribute name="NAME"/>
</element>
<element name="PWR8" library="QuantumOptics" package="DC-DC:CC1R5-XXXXX-R-E(TDK/LAMBDA)" value="CC1R5-1212DR-E">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="4.99K">
<attribute name="NAME"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C53" library="QuantumOptics" package="2012(0805)" value="680pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C54" library="QuantumOptics" package="2012(0805)" value="270pF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOIC-8" value="AD8671ARZ">
<attribute name="NAME"/>
</element>
<element name="C55" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C56" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="J8" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="227161-1">
<attribute name="DESC" value="&quot;Out 4&quot;"/>
<attribute name="NAME"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.5A">
<attribute name="PN" value="2 x 100056"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="12V+" library="QuantumOptics" package="TP-0.042B" value="5002K"/>
<element name="12V-" library="QuantumOptics" package="TP-0.042B" value="5002K"/>
<element name="IC9" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
</element>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C57" library="QuantumOptics" package="2012(0805)" value="100pF">
<attribute name="NAME"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH:SPDT-DIP(COPAL)" value="CJS-1200TA">
<attribute name="NAME"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-8" value="AD8672ARZ">
<attribute name="NAME"/>
</element>
<element name="R27" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R28" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C58" library="QuantumOptics" package="2012(0805)" value="100pF">
<attribute name="NAME"/>
</element>
<element name="CASE" library="QuantumOptics" package="MISC" value="1598CGY">
<attribute name="MFG" value="Hammond"/>
<attribute name="PN" value=""/>
</element>
<element name="POWER" library="QuantumOptics" package="MISC" value="EPS120050-P7P">
<attribute name="MFG" value="CUI"/>
<attribute name="PN" value=""/>
</element>
<element name="FILTR" library="QuantumOptics" package="MISC" value="LFB143064-000">
<attribute name="MFG" value="Laird Tech"/>
<attribute name="PN" value=""/>
</element>
<element name="U$3" library="QuantumOptics" package="TITLEBLOCK_PCB" value=""/>
<element name="GRMMT" library="QuantumOptics" package="MISC" value="731 or 736">
<attribute name="MFG" value="Keystone"/>
<attribute name="PN" value=""/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="+"/>
<contactref element="C4" pad="2"/>
<contactref element="PWR1" pad="+VOUT"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="-"/>
<contactref element="PWR1" pad="-VOUT"/>
<contactref element="PWR1" pad="TRM"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="27"/>
<contactref element="J1" pad="CONDUCTOR"/>
</signal>
<signal name="N$4">
<contactref element="C7" pad="+"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="15"/>
<contactref element="PWR2" pad="+VOUT"/>
<contactref element="C13" pad="2"/>
<contactref element="R3" pad="CCW"/>
<contactref element="IC9" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="13"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="14"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="W"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="-12VIN">
<contactref element="PWR1" pad="RC"/>
<contactref element="PWR1" pad="-VIN"/>
<contactref element="C1" pad="1"/>
<contactref element="PWR2" pad="RC"/>
<contactref element="PWR2" pad="-VIN"/>
<contactref element="C2" pad="1"/>
<contactref element="PWR3" pad="RC"/>
<contactref element="PWR3" pad="-VIN"/>
<contactref element="C23" pad="1"/>
<contactref element="PWR4" pad="RC"/>
<contactref element="PWR4" pad="-VIN"/>
<contactref element="C24" pad="1"/>
<contactref element="PWR5" pad="RC"/>
<contactref element="PWR5" pad="-VIN"/>
<contactref element="C37" pad="1"/>
<contactref element="PWR6" pad="RC"/>
<contactref element="PWR6" pad="-VIN"/>
<contactref element="C38" pad="1"/>
<contactref element="PWR7" pad="RC"/>
<contactref element="PWR7" pad="-VIN"/>
<contactref element="C51" pad="1"/>
<contactref element="PWR8" pad="RC"/>
<contactref element="PWR8" pad="-VIN"/>
<contactref element="C52" pad="1"/>
<contactref element="12V-" pad="TP"/>
</signal>
<signal name="COM-IN1">
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="C3" pad="-"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="28"/>
<contactref element="C6" pad="+"/>
<contactref element="PWR1" pad="COM"/>
</signal>
<signal name="N$16">
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C12" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="IC9" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="C11" pad="2"/>
<contactref element="IC9" pad="2"/>
<contactref element="IC9" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="PWR2" pad="-VOUT"/>
<contactref element="PWR2" pad="TRM"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="-"/>
<contactref element="IC1" pad="16"/>
<contactref element="C14" pad="2"/>
<contactref element="R3" pad="CW"/>
<contactref element="IC9" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="J2" pad="CONDUCTOR"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="COM-OUT1">
<contactref element="C7" pad="-"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C10" pad="+"/>
<contactref element="PWR2" pad="COM"/>
<contactref element="C12" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="J2" pad="SHIELD2"/>
<contactref element="J2" pad="SHIELD1"/>
<contactref element="R1" pad="1"/>
<contactref element="IC9" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="IC3" pad="1"/>
<contactref element="C15" pad="POS"/>
<contactref element="C16" pad="2"/>
<contactref element="PWR3" pad="+VOUT"/>
</signal>
<signal name="N$6">
<contactref element="IC3" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="NEG"/>
<contactref element="PWR3" pad="-VOUT"/>
<contactref element="PWR3" pad="TRM"/>
</signal>
<signal name="N$7">
<contactref element="IC3" pad="27"/>
<contactref element="J3" pad="CONDUCTOR"/>
</signal>
<signal name="N$13">
<contactref element="C19" pad="POS"/>
<contactref element="C20" pad="2"/>
<contactref element="IC3" pad="15"/>
<contactref element="PWR4" pad="+VOUT"/>
<contactref element="C27" pad="2"/>
<contactref element="R7" pad="CCW"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="IC3" pad="13"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="IC3" pad="14"/>
<contactref element="R8" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R7" pad="W"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="COM-IN2">
<contactref element="J3" pad="SHIELD2"/>
<contactref element="J3" pad="SHIELD1"/>
<contactref element="C15" pad="NEG"/>
<contactref element="C17" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="IC3" pad="28"/>
<contactref element="C18" pad="POS"/>
<contactref element="PWR3" pad="COM"/>
</signal>
<signal name="N$24">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="C26" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="C25" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="SW2" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="PWR4" pad="-VOUT"/>
<contactref element="PWR4" pad="TRM"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="NEG"/>
<contactref element="IC3" pad="16"/>
<contactref element="C28" pad="2"/>
<contactref element="R7" pad="CW"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$28">
<contactref element="J4" pad="CONDUCTOR"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="COM-OUT2">
<contactref element="C19" pad="NEG"/>
<contactref element="C21" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C22" pad="POS"/>
<contactref element="PWR4" pad="COM"/>
<contactref element="C26" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="J4" pad="SHIELD2"/>
<contactref element="J4" pad="SHIELD1"/>
<contactref element="R12" pad="1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$29">
<contactref element="IC5" pad="1"/>
<contactref element="C29" pad="POS"/>
<contactref element="C30" pad="2"/>
<contactref element="PWR5" pad="+VOUT"/>
</signal>
<signal name="N$30">
<contactref element="IC5" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="NEG"/>
<contactref element="PWR5" pad="-VOUT"/>
<contactref element="PWR5" pad="TRM"/>
</signal>
<signal name="N$31">
<contactref element="IC5" pad="27"/>
<contactref element="J5" pad="CONDUCTOR"/>
</signal>
<signal name="N$32">
<contactref element="C33" pad="POS"/>
<contactref element="C34" pad="2"/>
<contactref element="IC5" pad="15"/>
<contactref element="PWR6" pad="+VOUT"/>
<contactref element="IC6" pad="7"/>
<contactref element="C41" pad="2"/>
<contactref element="R13" pad="CCW"/>
</signal>
<signal name="N$33">
<contactref element="IC5" pad="13"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="IC5" pad="14"/>
<contactref element="R14" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="R13" pad="W"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="+12VIN">
<contactref element="PWR5" pad="+VIN"/>
<contactref element="C37" pad="2"/>
<contactref element="PWR6" pad="+VIN"/>
<contactref element="C38" pad="2"/>
<contactref element="PWR7" pad="+VIN"/>
<contactref element="C51" pad="2"/>
<contactref element="PWR8" pad="+VIN"/>
<contactref element="C52" pad="2"/>
<contactref element="PWR1" pad="+VIN"/>
<contactref element="C1" pad="2"/>
<contactref element="PWR2" pad="+VIN"/>
<contactref element="C2" pad="2"/>
<contactref element="PWR3" pad="+VIN"/>
<contactref element="C23" pad="2"/>
<contactref element="PWR4" pad="+VIN"/>
<contactref element="C24" pad="2"/>
<contactref element="F1" pad="2A"/>
</signal>
<signal name="COM-IN3">
<contactref element="J5" pad="SHIELD2"/>
<contactref element="J5" pad="SHIELD1"/>
<contactref element="C29" pad="NEG"/>
<contactref element="C31" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="IC5" pad="28"/>
<contactref element="C32" pad="POS"/>
<contactref element="PWR5" pad="COM"/>
</signal>
<signal name="N$38">
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="C39" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="C40" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="IC6" pad="3"/>
</signal>
<signal name="N$40">
<contactref element="IC6" pad="6"/>
<contactref element="IC6" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="PWR6" pad="-VOUT"/>
<contactref element="PWR6" pad="TRM"/>
<contactref element="C35" pad="2"/>
<contactref element="C36" pad="NEG"/>
<contactref element="IC5" pad="16"/>
<contactref element="IC6" pad="4"/>
<contactref element="C42" pad="2"/>
<contactref element="R13" pad="CW"/>
</signal>
<signal name="N$42">
<contactref element="J6" pad="CONDUCTOR"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="COM-OUT3">
<contactref element="C33" pad="NEG"/>
<contactref element="C35" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C36" pad="POS"/>
<contactref element="PWR6" pad="COM"/>
<contactref element="C40" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="J6" pad="SHIELD2"/>
<contactref element="J6" pad="SHIELD1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="IC7" pad="1"/>
<contactref element="C43" pad="POS"/>
<contactref element="C44" pad="2"/>
<contactref element="PWR7" pad="+VOUT"/>
</signal>
<signal name="N$44">
<contactref element="IC7" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="C46" pad="NEG"/>
<contactref element="PWR7" pad="-VOUT"/>
<contactref element="PWR7" pad="TRM"/>
</signal>
<signal name="N$45">
<contactref element="IC7" pad="27"/>
<contactref element="J7" pad="CONDUCTOR"/>
</signal>
<signal name="N$46">
<contactref element="C47" pad="POS"/>
<contactref element="C48" pad="2"/>
<contactref element="IC7" pad="15"/>
<contactref element="PWR8" pad="+VOUT"/>
<contactref element="IC8" pad="7"/>
<contactref element="C55" pad="2"/>
<contactref element="R19" pad="CCW"/>
</signal>
<signal name="N$47">
<contactref element="IC7" pad="13"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="IC7" pad="14"/>
<contactref element="R20" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$49">
<contactref element="R19" pad="W"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="COM-IN4">
<contactref element="J7" pad="SHIELD2"/>
<contactref element="J7" pad="SHIELD1"/>
<contactref element="C43" pad="NEG"/>
<contactref element="C45" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="IC7" pad="28"/>
<contactref element="C46" pad="POS"/>
<contactref element="PWR7" pad="COM"/>
</signal>
<signal name="N$52">
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="C53" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="C54" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="IC8" pad="3"/>
</signal>
<signal name="N$54">
<contactref element="IC8" pad="6"/>
<contactref element="IC8" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="PWR8" pad="-VOUT"/>
<contactref element="PWR8" pad="TRM"/>
<contactref element="C49" pad="2"/>
<contactref element="C50" pad="NEG"/>
<contactref element="IC7" pad="16"/>
<contactref element="IC8" pad="4"/>
<contactref element="C56" pad="2"/>
<contactref element="R19" pad="CW"/>
</signal>
<signal name="N$56">
<contactref element="J8" pad="CONDUCTOR"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="COM-OUT4">
<contactref element="C47" pad="NEG"/>
<contactref element="C49" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C50" pad="POS"/>
<contactref element="PWR8" pad="COM"/>
<contactref element="C54" pad="1"/>
<contactref element="C56" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="J8" pad="SHIELD2"/>
<contactref element="J8" pad="SHIELD1"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="12V+" pad="TP"/>
<contactref element="F1" pad="1A"/>
</signal>
<signal name="N$23">
<contactref element="R27" pad="1"/>
<contactref element="R28" pad="1"/>
<contactref element="C58" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$36">
<contactref element="R28" pad="2"/>
<contactref element="C58" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="N$37">
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
</signal>
<signal name="N$60">
</signal>
<signal name="N$59">
<contactref element="R25" pad="1"/>
<contactref element="IC9" pad="6"/>
<contactref element="R26" pad="1"/>
<contactref element="C57" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="R26" pad="2"/>
<contactref element="IC9" pad="7"/>
<contactref element="C57" pad="2"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="R6" pad="1"/>
<contactref element="SW1" pad="COM"/>
</signal>
<signal name="N$63">
<contactref element="R11" pad="1"/>
<contactref element="SW2" pad="COM"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$22">
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
</signals>
</board>
</drawing>
</eagle>
