<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="22-23-2021">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
<package name="22-23-2031">
<description>.100" (2.54mm) Center Header - 3 Pin</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="0805">
</package>
<package name="TH1">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="HEADER2ROW2POS">
</package>
<package name="22-23-2051">
<description>.100" (2.54mm) Center Header - 5 Pin</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="HEADER2ROW3POS">
</package>
<package name="HEADER2ROW4POS">
</package>
<package name="HEADER2ROW5POS">
</package>
<package name="ELECCAPTH1">
<description>Radial lead electrolytic cap with 2.5mm (~0.1") lead spacing. &lt;br&gt; Modeled after the Panasonic ECG series of Aluminum Caps (100uF).</description>
</package>
<package name="5227161">
</package>
<package name="POT1">
<description>Murata P37W Series &lt;br&gt;
Bourns 3266W</description>
</package>
<package name="5227222">
</package>
<package name="SSA-LXB101W">
</package>
<package name="PVA1">
</package>
<package name="5103308-2">
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="TESTPT4952">
</package>
<package name="TO-92">
<description>&lt;b&gt;TP 92&lt;/b&gt;</description>
</package>
<package name="TO92-">
<description>&lt;b&gt;TO 92 pad in line&lt;/b&gt;</description>
</package>
<package name="CTS206-124">
</package>
<package name="BOURNS3314">
</package>
<package name="BOURNS3214W">
</package>
<package name="DO-214AC">
</package>
<package name="SOD-323F">
</package>
<package name="HEADER2ROW1POS">
</package>
<package name="CJS-1200A">
</package>
<package name="SOT-23">
</package>
<package name="1210">
</package>
<package name="TO-220">
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="BITECH23B">
</package>
</packages>
<symbols>
<symbol name="MV">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="BU-BNC-NOPIN">
</symbol>
<symbol name="LEDNOPIN">
</symbol>
<symbol name="PANELPOTNOPIN">
</symbol>
<symbol name="SPDT-SWITCH-NOPIN">
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="OPAMP">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OPAMP2">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="HEADER2ROW2POS">
<pin name="1"/>
<pin name="3"/>
<pin name="2"/>
<pin name="4"/>
</symbol>
<symbol name="PDNOPIN">
</symbol>
<symbol name="REF01">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="TRIM"/>
<pin name="VO"/>
</symbol>
<symbol name="HEADER2ROW">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="CAPPOL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="BNC">
<pin name="INCOND" direction="pas"/>
<pin name="OUTCOND" direction="pas"/>
</symbol>
<symbol name="POT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="BUFFERWINVERT">
<pin name="IN" direction="in"/>
<pin name="ENABLE" direction="in" function="dot"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="BUFFERWINVERT2">
<pin name="IN" direction="in"/>
<pin name="ENABLE" direction="in" function="dot"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LED">
<pin name="ANODE"/>
<pin name="CATHODE"/>
</symbol>
<symbol name="DPSTSWITCH">
<pin name="1A" direction="pas"/>
<pin name="1B" direction="pas"/>
<pin name="2A" direction="pas"/>
<pin name="2B" direction="pas"/>
</symbol>
<symbol name="INVERTER">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
</symbol>
<symbol name="INVERTER2">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="510338-2">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
<pin name="P$3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="OPAMP3">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NULL2"/>
<pin name="NULL1"/>
</symbol>
<symbol name="DIODE">
<pin name="ANODE"/>
<pin name="CATHODE"/>
</symbol>
<symbol name="TESTPT">
<pin name="P$1"/>
</symbol>
<symbol name="JFET">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="MOSFET">
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="NPN">
<pin name="B"/>
<pin name="C"/>
<pin name="E"/>
</symbol>
<symbol name="SPDTANALOGSWITCH">
<pin name="D"/>
<pin name="S1"/>
<pin name="S2"/>
<pin name="IN"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VL" direction="in"/>
</symbol>
<symbol name="SPSTSWITCH">
<pin name="1B" direction="pas"/>
<pin name="2B" direction="pas"/>
</symbol>
<symbol name="SPDTSWITCH">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="SPDTSWITCH2">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$4"/>
<pin name="P$3"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B"/>
<pin name="C"/>
<pin name="E"/>
</symbol>
<symbol name="MAX62">
<pin name="VIN"/>
<pin name="GND"/>
<pin name="TRIM"/>
<pin name="VO"/>
<pin name="NR"/>
</symbol>
<symbol name="SPSTSWITCH2">
<pin name="P$1"/>
<pin name="P$3"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="22-23-2021" prefix="X">
<description>.100" (2.54mm) Center Header - 2 Pin</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
</gates>
<devices>
<device name="" package="22-23-2021">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22-23-2031" prefix="X">
<description>.100" (2.54mm) Center Header - 3 Pin</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
</gates>
<devices>
<device name="" package="22-23-2031">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PANELBNC" prefix="X">
<description>BNC Panel Mount, Solder, 50 Ohm</description>
<gates>
<gate name="G$1" symbol="BU-BNC-NOPIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="DISTRIBUTOR" value="L-COM"/>
<attribute name="PARTNUM" value="BAC1503"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PANELLED">
<gates>
<gate name="G$1" symbol="LEDNOPIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PANELPOT" uservalue="yes">
<description>Panel Mount Potentiometer</description>
<gates>
<gate name="G$1" symbol="PANELPOTNOPIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="COMPANY" value="Bourns Inc"/>
<attribute name="DIGIKEY" value="3590S Series"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PANELSPDTSWITCH">
<description>Panel Mount, Single Pole Double Throw Switch</description>
<gates>
<gate name="G$1" symbol="SPDT-SWITCH-NOPIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name="">
<attribute name="DIGIKEY" value="450-1523-ND"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR?" prefix="R" uservalue="yes">
<description>Standard resistor. Packages starting in "TH" are through hole.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH1" package="TH1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP?" prefix="C" uservalue="yes">
<description>Standard Cap</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TH1" package="TH1">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF356?" prefix="IC">
<description>LF356 Op Amp, National Semiconductor</description>
<gates>
<gate name="G$1" symbol="OPAMP2"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SO08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2ROW2POS" prefix="X">
<description>Standard 0.1" 2x2 header</description>
<gates>
<gate name="-1" symbol="HEADER2ROW"/>
<gate name="-2" symbol="HEADER2ROW"/>
</gates>
<devices>
<device name="" package="HEADER2ROW2POS">
<connects>
<connect gate="-1" pin="P$1" pad="1A"/>
<connect gate="-1" pin="P$2" pad="1B"/>
<connect gate="-2" pin="P$1" pad="2A"/>
<connect gate="-2" pin="P$2" pad="2B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PANELPD" prefix="PD">
<description>Photodiode, Mounted Externally</description>
<gates>
<gate name="G$1" symbol="PDNOPIN"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22-23-2051" prefix="X">
<description>.100" (2.54mm) Center Header - 5 Pin</description>
<gates>
<gate name="-1" symbol="MV"/>
<gate name="-2" symbol="M"/>
<gate name="-3" symbol="M"/>
<gate name="-4" symbol="M"/>
<gate name="-5" symbol="M"/>
</gates>
<devices>
<device name="" package="22-23-2051">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
<connect gate="-5" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF347?" prefix="IC">
<description>Quad FET Op-Amp with 4MHz Bandwidth &lt;br&gt;
Low input bias current &lt;br&gt;
Moderate voltage noise and input voltage offset</description>
<gates>
<gate name="-A" symbol="OPAMP"/>
<gate name="-B" symbol="OPAMP"/>
<gate name="-C" symbol="OPAMP"/>
<gate name="-D" symbol="OPAMP2"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="-A" pin="IN+" pad="3"/>
<connect gate="-A" pin="IN-" pad="2"/>
<connect gate="-A" pin="OUT" pad="1"/>
<connect gate="-B" pin="IN+" pad="5"/>
<connect gate="-B" pin="IN-" pad="6"/>
<connect gate="-B" pin="OUT" pad="7"/>
<connect gate="-C" pin="IN+" pad="10"/>
<connect gate="-C" pin="IN-" pad="9"/>
<connect gate="-C" pin="OUT" pad="8"/>
<connect gate="-D" pin="IN+" pad="12"/>
<connect gate="-D" pin="IN-" pad="13"/>
<connect gate="-D" pin="OUT" pad="14"/>
<connect gate="-D" pin="V+" pad="4"/>
<connect gate="-D" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="-A" pin="IN+" pad="3"/>
<connect gate="-A" pin="IN-" pad="2"/>
<connect gate="-A" pin="OUT" pad="1"/>
<connect gate="-B" pin="IN+" pad="5"/>
<connect gate="-B" pin="IN-" pad="6"/>
<connect gate="-B" pin="OUT" pad="7"/>
<connect gate="-C" pin="IN+" pad="10"/>
<connect gate="-C" pin="IN-" pad="9"/>
<connect gate="-C" pin="OUT" pad="8"/>
<connect gate="-D" pin="IN+" pad="12"/>
<connect gate="-D" pin="IN-" pad="13"/>
<connect gate="-D" pin="OUT" pad="14"/>
<connect gate="-D" pin="V+" pad="4"/>
<connect gate="-D" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF01?" prefix="IC">
<description>10V Reference &lt;br&gt;
12V to 40V Input &lt;br&gt;
10mA drive</description>
<gates>
<gate name="G$1" symbol="REF01"/>
</gates>
<devices>
<device name="Z" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2ROW3POS" prefix="X">
<gates>
<gate name="-1" symbol="HEADER2ROW"/>
<gate name="-2" symbol="HEADER2ROW"/>
<gate name="-3" symbol="HEADER2ROW"/>
</gates>
<devices>
<device name="" package="HEADER2ROW3POS">
<connects>
<connect gate="-1" pin="P$1" pad="1A"/>
<connect gate="-1" pin="P$2" pad="1B"/>
<connect gate="-2" pin="P$1" pad="2A"/>
<connect gate="-2" pin="P$2" pad="2B"/>
<connect gate="-3" pin="P$1" pad="3A"/>
<connect gate="-3" pin="P$2" pad="3B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2ROW4POS" prefix="X">
<gates>
<gate name="-1" symbol="HEADER2ROW"/>
<gate name="-2" symbol="HEADER2ROW"/>
<gate name="-3" symbol="HEADER2ROW"/>
<gate name="-4" symbol="HEADER2ROW"/>
</gates>
<devices>
<device name="" package="HEADER2ROW4POS">
<connects>
<connect gate="-1" pin="P$1" pad="1A"/>
<connect gate="-1" pin="P$2" pad="1B"/>
<connect gate="-2" pin="P$1" pad="2A"/>
<connect gate="-2" pin="P$2" pad="2B"/>
<connect gate="-3" pin="P$1" pad="3A"/>
<connect gate="-3" pin="P$2" pad="3B"/>
<connect gate="-4" pin="P$1" pad="4A"/>
<connect gate="-4" pin="P$2" pad="4B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2ROW5POS" prefix="X">
<description>2x5 0.1" header</description>
<gates>
<gate name="-1" symbol="HEADER2ROW"/>
<gate name="-2" symbol="HEADER2ROW"/>
<gate name="-3" symbol="HEADER2ROW"/>
<gate name="-4" symbol="HEADER2ROW"/>
<gate name="-5" symbol="HEADER2ROW"/>
</gates>
<devices>
<device name="" package="HEADER2ROW5POS">
<connects>
<connect gate="-1" pin="P$1" pad="1A"/>
<connect gate="-1" pin="P$2" pad="1B"/>
<connect gate="-2" pin="P$1" pad="2A"/>
<connect gate="-2" pin="P$2" pad="2B"/>
<connect gate="-3" pin="P$1" pad="3A"/>
<connect gate="-3" pin="P$2" pad="3B"/>
<connect gate="-4" pin="P$1" pad="4A"/>
<connect gate="-4" pin="P$2" pad="4B"/>
<connect gate="-5" pin="P$1" pad="5A"/>
<connect gate="-5" pin="P$2" pad="5B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPPOL?" prefix="C" uservalue="yes">
<description>Polarized Capacitor. Can be either aluminum or tantalum electrolytic. Use appropriate package depending on the type (and capacitance)</description>
<gates>
<gate name="G$1" symbol="CAPPOL"/>
</gates>
<devices>
<device name="RADIAL-0.1SPACING" package="ELECCAPTH1">
<connects>
<connect gate="G$1" pin="1" pad="PLUS"/>
<connect gate="G$1" pin="2" pad="MINUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5227161" prefix="X">
<description>Right Angle 50Ohm PCB BNC Connector. DigiKey Part #A32258-ND.</description>
<gates>
<gate name="G$1" symbol="BNC"/>
</gates>
<devices>
<device name="" package="5227161">
<connects>
<connect gate="G$1" pin="INCOND" pad="INCOND"/>
<connect gate="G$1" pin="OUTCOND" pad="OUTCOND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT-?" prefix="R" uservalue="yes">
<description>Potentiometer &lt;br&gt;
Package Variant A is for Murata P37W or Bourns 3266W Series, which is top adjust screw with one offset pin.</description>
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="A" package="POT1">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339?" prefix="U">
<description>Quad Comparator. Same as LM239/2901.</description>
<gates>
<gate name="G$1" symbol="OPAMP"/>
<gate name="G$2" symbol="OPAMP"/>
<gate name="G$3" symbol="OPAMP"/>
<gate name="G$4" symbol="OPAMP2"/>
</gates>
<devices>
<device name="D" package="SO14">
<connects>
<connect gate="G$1" pin="IN+" pad="5"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$2" pin="IN+" pad="7"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="1"/>
<connect gate="G$3" pin="IN+" pad="9"/>
<connect gate="G$3" pin="IN-" pad="8"/>
<connect gate="G$3" pin="OUT" pad="14"/>
<connect gate="G$4" pin="IN+" pad="11"/>
<connect gate="G$4" pin="IN-" pad="10"/>
<connect gate="G$4" pin="OUT" pad="13"/>
<connect gate="G$4" pin="V+" pad="3"/>
<connect gate="G$4" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="DIL14">
<connects>
<connect gate="G$1" pin="IN+" pad="5"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$2" pin="IN+" pad="7"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="1"/>
<connect gate="G$3" pin="IN+" pad="9"/>
<connect gate="G$3" pin="IN-" pad="8"/>
<connect gate="G$3" pin="OUT" pad="14"/>
<connect gate="G$4" pin="IN+" pad="11"/>
<connect gate="G$4" pin="IN-" pad="10"/>
<connect gate="G$4" pin="OUT" pad="13"/>
<connect gate="G$4" pin="V+" pad="3"/>
<connect gate="G$4" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC125?" prefix="U">
<description>Quad 3-State Buffer</description>
<gates>
<gate name="G$1" symbol="BUFFERWINVERT2"/>
<gate name="G$2" symbol="BUFFERWINVERT"/>
<gate name="G$3" symbol="BUFFERWINVERT"/>
<gate name="G$4" symbol="BUFFERWINVERT"/>
</gates>
<devices>
<device name="M" package="SO14">
<connects>
<connect gate="G$1" pin="ENABLE" pad="1"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$2" pin="ENABLE" pad="4"/>
<connect gate="G$2" pin="IN" pad="5"/>
<connect gate="G$2" pin="OUT" pad="6"/>
<connect gate="G$3" pin="ENABLE" pad="10"/>
<connect gate="G$3" pin="IN" pad="9"/>
<connect gate="G$3" pin="OUT" pad="8"/>
<connect gate="G$4" pin="ENABLE" pad="13"/>
<connect gate="G$4" pin="IN" pad="12"/>
<connect gate="G$4" pin="OUT" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5227222">
<description>Vertical BNC Connector
Tyco - Digi-Key Part #A32262</description>
<gates>
<gate name="G$1" symbol="BNC"/>
</gates>
<devices>
<device name="" package="5227222">
<connects>
<connect gate="G$1" pin="INCOND" pad="CENTERPIN"/>
<connect gate="G$1" pin="OUTCOND" pad="SHIELDPIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSA-LXB101W" prefix="LED">
<description>10 Segment RED LED &lt;br&gt;
Lumex</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="G$2" symbol="LED"/>
<gate name="G$3" symbol="LED"/>
<gate name="G$4" symbol="LED"/>
<gate name="G$5" symbol="LED"/>
<gate name="G$6" symbol="LED"/>
<gate name="G$7" symbol="LED"/>
<gate name="G$8" symbol="LED"/>
<gate name="G$9" symbol="LED"/>
<gate name="G$10" symbol="LED"/>
</gates>
<devices>
<device name="" package="SSA-LXB101W">
<connects>
<connect gate="G$1" pin="ANODE" pad="1"/>
<connect gate="G$1" pin="CATHODE" pad="20"/>
<connect gate="G$10" pin="ANODE" pad="10"/>
<connect gate="G$10" pin="CATHODE" pad="11"/>
<connect gate="G$2" pin="ANODE" pad="2"/>
<connect gate="G$2" pin="CATHODE" pad="19"/>
<connect gate="G$3" pin="ANODE" pad="3"/>
<connect gate="G$3" pin="CATHODE" pad="18"/>
<connect gate="G$4" pin="ANODE" pad="4"/>
<connect gate="G$4" pin="CATHODE" pad="17"/>
<connect gate="G$5" pin="ANODE" pad="5"/>
<connect gate="G$5" pin="CATHODE" pad="16"/>
<connect gate="G$6" pin="ANODE" pad="6"/>
<connect gate="G$6" pin="CATHODE" pad="15"/>
<connect gate="G$7" pin="ANODE" pad="7"/>
<connect gate="G$7" pin="CATHODE" pad="14"/>
<connect gate="G$8" pin="ANODE" pad="8"/>
<connect gate="G$8" pin="CATHODE" pad="13"/>
<connect gate="G$9" pin="ANODE" pad="9"/>
<connect gate="G$9" pin="CATHODE" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PVA?*" prefix="S">
<description>DPST Push Button Switch &lt;br&gt;
PVA Series from C+K Components</description>
<gates>
<gate name="G$1" symbol="DPSTSWITCH"/>
</gates>
<devices>
<device name="1" package="PVA1">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="1B"/>
<connect gate="G$1" pin="2A" pad="2"/>
<connect gate="G$1" pin="2B" pad="2B"/>
</connects>
<technologies>
<technology name="EE"/>
<technology name="OA"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC04?">
<description>Inverter</description>
<gates>
<gate name="G$1" symbol="INVERTER2"/>
<gate name="G$2" symbol="INVERTER"/>
<gate name="G$3" symbol="INVERTER"/>
<gate name="G$4" symbol="INVERTER"/>
<gate name="G$5" symbol="INVERTER"/>
<gate name="G$6" symbol="INVERTER"/>
</gates>
<devices>
<device name="SC" package="SO14">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$2" pin="IN" pad="3"/>
<connect gate="G$2" pin="OUT" pad="4"/>
<connect gate="G$3" pin="IN" pad="5"/>
<connect gate="G$3" pin="OUT" pad="6"/>
<connect gate="G$4" pin="IN" pad="9"/>
<connect gate="G$4" pin="OUT" pad="8"/>
<connect gate="G$5" pin="IN" pad="11"/>
<connect gate="G$5" pin="OUT" pad="10"/>
<connect gate="G$6" pin="IN" pad="13"/>
<connect gate="G$6" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PC" package="DIL14">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$2" pin="IN" pad="3"/>
<connect gate="G$2" pin="OUT" pad="4"/>
<connect gate="G$3" pin="IN" pad="5"/>
<connect gate="G$3" pin="OUT" pad="6"/>
<connect gate="G$4" pin="IN" pad="9"/>
<connect gate="G$4" pin="OUT" pad="8"/>
<connect gate="G$5" pin="IN" pad="11"/>
<connect gate="G$5" pin="OUT" pad="10"/>
<connect gate="G$6" pin="IN" pad="13"/>
<connect gate="G$6" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5103308-2" prefix="X">
<description>0.1" Header with polarizing key &lt;br&gt;
Mates with Ribbon Cable connector 1658621-2</description>
<gates>
<gate name="G$1" symbol="510338-2"/>
</gates>
<devices>
<device name="" package="5103308-2">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78XXL" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="78XX"/>
</gates>
<devices>
<device name="" package="78XXL">
<connects>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="IN" pad="IN"/>
<connect gate="A" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4227?" prefix="U">
<description>Low-noise quad op amp &lt;br&gt;
8MHz bandwidth &lt;br&gt;
3nv/Hz^0.5 voltage noise &lt;br&gt;
0.4pA/Hz^(0.5) current noise</description>
<gates>
<gate name="G$1" symbol="OPAMP2"/>
<gate name="G$2" symbol="OPAMP"/>
<gate name="G$3" symbol="OPAMP"/>
<gate name="G$4" symbol="OPAMP"/>
</gates>
<devices>
<device name="PA" package="DIL14">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="11"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="IN+" pad="10"/>
<connect gate="G$3" pin="IN-" pad="9"/>
<connect gate="G$3" pin="OUT" pad="8"/>
<connect gate="G$4" pin="IN+" pad="12"/>
<connect gate="G$4" pin="IN-" pad="13"/>
<connect gate="G$4" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UA" package="SO14">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="11"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="IN+" pad="10"/>
<connect gate="G$3" pin="IN-" pad="9"/>
<connect gate="G$3" pin="OUT" pad="8"/>
<connect gate="G$4" pin="IN+" pad="12"/>
<connect gate="G$4" pin="IN-" pad="13"/>
<connect gate="G$4" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP470?" prefix="U">
<description>Low-noise quad op-amp &lt;br&gt;
5nV/Hz^(0.5) voltage noise &lt;br&gt;
6MHz bandwidth &lt;br&gt;
Low Offset voltage drift 2uV/C &lt;br&gt;
1.7pA/Hz^(0.5) @ 10Hz, 0.4pA/Hz^(0.4) @1kHz current noise</description>
<gates>
<gate name="G$1" symbol="OPAMP2"/>
<gate name="G$2" symbol="OPAMP"/>
<gate name="G$3" symbol="OPAMP"/>
<gate name="G$4" symbol="OPAMP"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="11"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="IN+" pad="10"/>
<connect gate="G$3" pin="IN-" pad="9"/>
<connect gate="G$3" pin="OUT" pad="8"/>
<connect gate="G$4" pin="IN+" pad="12"/>
<connect gate="G$4" pin="IN-" pad="13"/>
<connect gate="G$4" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO16">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="13"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
<connect gate="G$3" pin="IN+" pad="12"/>
<connect gate="G$3" pin="IN-" pad="11"/>
<connect gate="G$3" pin="OUT" pad="10"/>
<connect gate="G$4" pin="IN+" pad="14"/>
<connect gate="G$4" pin="IN-" pad="15"/>
<connect gate="G$4" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1357?" prefix="U">
<description>High-speed (25MHz), high slew rate (600V/us) &lt;br&gt;
High bias current, 8nV/Hz^(0.5) voltage noise</description>
<gates>
<gate name="G$1" symbol="OPAMP3"/>
</gates>
<devices>
<device name="CN8" package="DIL08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="NULL1" pad="1"/>
<connect gate="G$1" pin="NULL2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C38" package="SO08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="NULL1" pad="1"/>
<connect gate="G$1" pin="NULL2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD826?" prefix="U">
<description>High speed (50MHz) dual op-amp &lt;br&gt;
15nV/Hz^(0.5) voltage noise, 1.5pA/Hz^(0.5) current noise&lt;br&gt;
15nA offset current (10uA bias)</description>
<gates>
<gate name="G$1" symbol="OPAMP2"/>
<gate name="G$2" symbol="OPAMP"/>
</gates>
<devices>
<device name="AN" package="DIL08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AR" package="SO08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE?" prefix="D" uservalue="yes">
<description>Generic diode</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="TH" package="TH1">
<connects>
<connect gate="G$1" pin="ANODE" pad="P$1"/>
<connect gate="G$1" pin="CATHODE" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA227?" prefix="U">
<gates>
<gate name="G$1" symbol="OPAMP3"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="NULL1" pad="1"/>
<connect gate="G$1" pin="NULL2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="NULL1" pad="1"/>
<connect gate="G$1" pin="NULL2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TESTPT?" prefix="X">
<gates>
<gate name="G$1" symbol="TESTPT"/>
</gates>
<devices>
<device name="4952" package="TESTPT4952">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NJFET?">
<gates>
<gate name="G$1" symbol="JFET"/>
</gates>
<devices>
<device name="-BF245" package="TO92-">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG419?">
<gates>
<gate name="G$1" symbol="SPDTANALOGSWITCH"/>
</gates>
<devices>
<device name="BR" package="SO08">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="8"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8676" prefix="U">
<gates>
<gate name="G$1" symbol="OPAMP2"/>
<gate name="G$2" symbol="OPAMP"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CTS206-124" prefix="S">
<description>DIP Switch &lt;br&gt;
4 Position SPDT &lt;br&gt;
CTS</description>
<gates>
<gate name="G$1" symbol="SPDTSWITCH2"/>
<gate name="G$2" symbol="SPDTSWITCH2"/>
<gate name="G$3" symbol="SPDTSWITCH2"/>
<gate name="G$4" symbol="SPDTSWITCH2"/>
</gates>
<devices>
<device name="" package="CTS206-124">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$2" pin="P$1" pad="5"/>
<connect gate="G$2" pin="P$2" pad="6"/>
<connect gate="G$2" pin="P$3" pad="7"/>
<connect gate="G$2" pin="P$4" pad="8"/>
<connect gate="G$3" pin="P$1" pad="9"/>
<connect gate="G$3" pin="P$2" pad="10"/>
<connect gate="G$3" pin="P$3" pad="11"/>
<connect gate="G$3" pin="P$4" pad="12"/>
<connect gate="G$4" pin="P$1" pad="13"/>
<connect gate="G$4" pin="P$2" pad="14"/>
<connect gate="G$4" pin="P$3" pad="15"/>
<connect gate="G$4" pin="P$4" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT3314?" prefix="R" uservalue="yes">
<description>Bourns Surface Mount Potentiometer &lt;br&gt;
1 Turn &lt;br&gt;
100ppm/C</description>
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="J" package="BOURNS3314">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT3214?" prefix="R" uservalue="yes">
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="W" package="BOURNS3214W">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="S1A" prefix="D">
<description>1A Rectifier Diode</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="DO-214AC">
<connects>
<connect gate="G$1" pin="ANODE" pad="2"/>
<connect gate="G$1" pin="CATHODE" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1N4148?" prefix="D">
<description>Small signal diode</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="TH" package="TH1">
<connects>
<connect gate="G$1" pin="ANODE" pad="P$1"/>
<connect gate="G$1" pin="CATHODE" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W" package="SOD-323F">
<connects>
<connect gate="G$1" pin="ANODE" pad="1"/>
<connect gate="G$1" pin="CATHODE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR?" prefix="L" uservalue="yes">
<description>Inductor &lt;br&gt;
Good surf mount is Murata LQM21F series</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEADER2ROW1POS">
<gates>
<gate name="G$1" symbol="HEADER2ROW"/>
</gates>
<devices>
<device name="" package="HEADER2ROW1POS">
<connects>
<connect gate="G$1" pin="P$1" pad="1A"/>
<connect gate="G$1" pin="P$2" pad="1B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CJS-1200?" prefix="S">
<description>Single SPDT Surface Mount Switch &lt;br&gt;
Copal Electronics</description>
<gates>
<gate name="G$1" symbol="SPDTSWITCH"/>
</gates>
<devices>
<device name="A" package="CJS-1200A">
<connects>
<connect gate="G$1" pin="P$1" pad="2"/>
<connect gate="G$1" pin="P$2" pad="1"/>
<connect gate="G$1" pin="P$3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC846">
<description>Surface Mount NPN &lt;br&gt;
100mA max &lt;br&gt;
45V C-E</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="" package="SOT-23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC856">
<description>PNP &lt;br&gt;
100mA &lt;br&gt;
~100 gain</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="" package="SOT-23">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78XX?" prefix="U">
<description>Voltage Regulator</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="C" package="TO-220">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX62*?" prefix="U">
<description>Precision Voltage Reference</description>
<gates>
<gate name="G$1" symbol="MAX62"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NR" pad="3"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDA04">
<description>DIP Switch (SPST) &lt;br&gt;
x 4</description>
<gates>
<gate name="G$1" symbol="SPSTSWITCH2"/>
<gate name="G$2" symbol="SPSTSWITCH2"/>
<gate name="G$3" symbol="SPSTSWITCH2"/>
<gate name="G$4" symbol="SPSTSWITCH2"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$3" pad="8"/>
<connect gate="G$2" pin="P$1" pad="2"/>
<connect gate="G$2" pin="P$3" pad="7"/>
<connect gate="G$3" pin="P$1" pad="3"/>
<connect gate="G$3" pin="P$3" pad="6"/>
<connect gate="G$4" pin="P$1" pad="4"/>
<connect gate="G$4" pin="P$3" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358?">
<description>Cheap dual op-amp</description>
<gates>
<gate name="G$1" symbol="OPAMP2"/>
<gate name="G$2" symbol="OPAMP"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="G$2" pin="IN+" pad="5"/>
<connect gate="G$2" pin="IN-" pad="6"/>
<connect gate="G$2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDA08">
<gates>
<gate name="G$1" symbol="SPSTSWITCH2"/>
<gate name="G$2" symbol="SPSTSWITCH2"/>
<gate name="G$3" symbol="SPSTSWITCH2"/>
<gate name="G$4" symbol="SPSTSWITCH2"/>
<gate name="G$5" symbol="SPSTSWITCH2"/>
<gate name="G$6" symbol="SPSTSWITCH2"/>
<gate name="G$7" symbol="SPSTSWITCH2"/>
<gate name="G$8" symbol="SPSTSWITCH2"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$3" pad="16"/>
<connect gate="G$2" pin="P$1" pad="2"/>
<connect gate="G$2" pin="P$3" pad="15"/>
<connect gate="G$3" pin="P$1" pad="3"/>
<connect gate="G$3" pin="P$3" pad="14"/>
<connect gate="G$4" pin="P$1" pad="4"/>
<connect gate="G$4" pin="P$3" pad="13"/>
<connect gate="G$5" pin="P$1" pad="5"/>
<connect gate="G$5" pin="P$3" pad="12"/>
<connect gate="G$6" pin="P$1" pad="6"/>
<connect gate="G$6" pin="P$3" pad="11"/>
<connect gate="G$7" pin="P$1" pad="7"/>
<connect gate="G$7" pin="P$3" pad="10"/>
<connect gate="G$8" pin="P$1" pad="8"/>
<connect gate="G$8" pin="P$3" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BITECH23?" prefix="R" uservalue="yes">
<description>Trim POT from BITECH &lt;br&gt;
Newark Part # 63M1857 (20k), 63M1861 (50k)</description>
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="B" package="BITECH23B">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
