<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="73.4" y1="77.036" x2="73.4" y2="100" width="0" layer="20"/>
<wire x1="73.4" y1="100" x2="63.9" y2="100" width="0" layer="20"/>
<wire x1="63.9" y1="100" x2="63.9" y2="77.036" width="0" layer="20"/>
<wire x1="63.9" y1="77.036" x2="73.4" y2="77.036" width="0" layer="20"/>
<wire x1="73.4" y1="46" x2="73.4" y2="8.5" width="0" layer="20"/>
<wire x1="0" y1="46" x2="0" y2="8.5" width="0" layer="20"/>
<wire x1="0" y1="8.5" x2="4.9" y2="8.5" width="0" layer="20"/>
<wire x1="7.9" y1="5.5" x2="7.9" y2="1" width="0" layer="20"/>
<wire x1="7.9" y1="1" x2="65.4" y2="1" width="0" layer="20"/>
<wire x1="65.4" y1="1" x2="65.4" y2="5.5" width="0" layer="20"/>
<wire x1="68.4" y1="8.5" x2="73.4" y2="8.5" width="0" layer="20"/>
<wire x1="0" y1="46" x2="4.9" y2="46" width="0" layer="20"/>
<wire x1="7.9" y1="49" x2="7.9" y2="54" width="0" layer="20"/>
<wire x1="7.9" y1="54" x2="65.4" y2="54" width="0" layer="20"/>
<wire x1="65.4" y1="54" x2="65.4" y2="49" width="0" layer="20"/>
<wire x1="68.4" y1="46" x2="73.4" y2="46" width="0" layer="20"/>
<wire x1="81.02" y1="100" x2="81.02" y2="0" width="0" layer="20"/>
<wire x1="140.02" y1="100" x2="81.02" y2="100" width="0" layer="20"/>
<wire x1="140.02" y1="0" x2="81.02" y2="0" width="0" layer="20"/>
<wire x1="140.02" y1="100" x2="140.02" y2="0" width="0" layer="20"/>
<hole x="68.54" y="12.36" drill="3.175"/>
<hole x="68.54" y="42.36" drill="3.175"/>
<hole x="4.54" y="12.36" drill="3.175"/>
<hole x="4.54" y="42.36" drill="3.175"/>
<wire x1="65.4" y1="5.5" x2="68.4" y2="8.5" width="0" layer="20" curve="-90"/>
<wire x1="68.4" y1="46" x2="65.4" y2="49" width="0" layer="20" curve="-90"/>
<wire x1="4.9" y1="8.5" x2="7.9" y2="5.5" width="0" layer="20" curve="-90"/>
<wire x1="7.9" y1="49" x2="4.9" y2="46" width="0" layer="20" curve="-90"/>
<text>0.25A Medium-blow
Littlefuse 20102500021P</text>
<text>3D Mini Magnetometer  Rev:A
University of Toronto - Physics
J.Thywissen Labs</text>
<text>3D Mini Magnetometer
UofT - Physics
J. Thywissen Labs
Rev:A</text>
<text>Mini
Mag
:A</text>
<wire x1="0" y1="61.62" x2="56.28" y2="61.62" width="0" layer="20"/>
<wire x1="56.28" y1="61.62" x2="56.28" y2="92" width="0" layer="20"/>
<wire x1="50.14" y1="100" x2="8" y2="100" width="0" layer="20"/>
<hole x="16" y="89.56" drill="1.5113"/>
<hole x="44" y="89.56" drill="1.5113"/>
<wire x1="0" y1="92" x2="0" y2="61.62" width="0" layer="20"/>
<wire x1="8" y1="95.26" x2="4.72" y2="92" width="0" layer="20" curve="-90"/>
<wire x1="4.72" y1="92" x2="0" y2="92" width="0" layer="20"/>
<wire x1="8" y1="95.28" x2="8" y2="100" width="0" layer="20"/>
<wire x1="50.14" y1="95.26" x2="53.42" y2="92" width="0" layer="20" curve="90"/>
<wire x1="53.42" y1="92" x2="56.28" y2="92" width="0" layer="20"/>
<wire x1="50.14" y1="95.28" x2="50.14" y2="100" width="0" layer="20"/>
<text>Audio Amp
Rev:A
UofT Physics</text>
<text>+9V</text>
<text>Warning for Rev:A - Labels for R6 and R12 are reversed on all 3 channels</text>
<text>Y</text>
<text>X</text>
<text>Z</text>
<text>Up: Z-Off</text>
<text>Up: Temperature</text>
<text>Dn: Set/Reset</text>
<text>Dn: XY-Off</text>
<text>Warning for Rev:A - On audio amps (page 2), LDO pinouts are wrong!</text>
</plain>
<libraries>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="LPCC-16">
<description>&lt;b&gt;LPCC-16&lt;/b&gt;, taken from Honeywell HMC1043 3D magnetometer. Wider footprint is for wide package such as HMC1043L.</description>
</package>
<package name="TP,1MM_PAD,LONG">
<description>&lt;b&gt;1mm c-c pad for 1mm FPC/FFC connections&lt;/b&gt;</description>
</package>
<package name="1608(0603)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0603 SMT, based on Kemet's description.</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, based on Kemet's description.</description>
</package>
<package name="MSOP10">
<description>&lt;b&gt;MSOP-10&lt;/b&gt; with 4.8mm row spacing.  Sameas Maxim's µsop-10.</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, based on TI's version of JEDEC MO-175 Variant AA.</description>
</package>
<package name="CAP,PANASONIC_D8,SMT,6.3MMROUND">
<description>&lt;b&gt;Polarized cap, Panasonic D8 case (6.3mm dia) and Cornell-Dubllier D and X (6.3mm dia)&lt;/b&gt;</description>
</package>
<package name="CONN:BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, e.g. 5226990-3,  nut 1-329631-2, shoulder washer 330620.</description>
</package>
<package name="CONN:BNC,DUAL(BOMAR)">
<description>&lt;b&gt;Dual BNC, vertical throughhole, isolated&lt;/b&gt;, Bomar, e.g. 364A2595, H=29.3mm, http://media.digikey.com/pdf/Data%20Sheets/Bomar%20PDFs/BNC_Products_Spec.pdf</description>
</package>
<package name="BOURNS_3009P">
<description>&lt;b&gt;3005P or 3009P Trimpot&lt;/b&gt;, Bourns, 15-turn, through-hole, end adjust. 3005 is ±50ppm, 3009 is ±100ppm.</description>
</package>
<package name="NEC_PS2501L-1">
<description>&lt;b&gt;PS2501L-1 Optocoupler&lt;/b&gt;, NEC, single channel, transistor output, CTR 80%min 300%typ, 5uS&lt;br&gt;
http://www.cel.com/pdf/datasheets/ps2501.pdf</description>
</package>
<package name="PANASONIC_ELLATV(COIL)">
<description>&lt;b&gt;ELLATV Inductor&lt;/b&gt;, Panasonic, SMT high current chokes, small, low resistance.&lt;br&gt;
&lt;a href="http://www.panasonic.com/industrial/components/pdf/agb0000ce14.pdf"&gt;
http://www.panasonic.com/industrial/components/pdf/agb0000ce14.pdf&lt;/a&gt;</description>
</package>
<package name="DC-DC:CC3-XXXXX-R-E(TDK/LAMBDA)">
<description>&lt;b&gt;CC3-inoutsR-E&lt;/b&gt;, TDK DC-DC isolated, 3W, uni- or bipolar&lt;br&gt;
"in": Input 05, 12, 24 or 48V.&lt;br&gt;
"out": Output 3.3, 5, 12, ±12 (or 24), ±15 (or30V).&lt;br&gt;
"s": Polarity single or dual.&lt;br&gt;
Case horiz SMD.&lt;br&gt;
http://www.tdk.co.jp/tefe02/ea335_cc_e.pdf</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire. Has continious fence so will generate lots of DRCs which can be ignored.</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="MSOP8GND">
<description>&lt;b&gt;MSOP-8 with exposed ground&lt;/b&gt;, e.g. Jedec MO-187-AA-T, Hittite HMC346 or Analog Devices Mini-SO-EP package.</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, based on Vishay.</description>
</package>
<package name="CASE,HAMMOND_RL6105_RL6115">
<description>&lt;b&gt;Hammond plastic case, 80 x 60mm, 30/40mmH, rounded corners.</description>
</package>
<package name="CONN,RIBBON,2X10,SULLINS_SBH41-NBPB-D10-ST-__">
<description>&lt;b&gt;Ribbon cable connector, 2 rows of 10, 0.05" grid&lt;/b&gt;, Sullins SBH41-NBPB-D10-SP-BK (SMT), can sub -SM- for no PCB guides, mates with SFH41-PPPB-D10-ID-BK (insulation displacement).</description>
</package>
<package name="CONN,FPC-FFC,1MM,16-POS">
<description>&lt;b&gt;Connector for FFC/FPC cables, 1mm, 16-position, SMT&lt;/b&gt;, such as Hirose FH12-16S-1SV(55).</description>
</package>
<package name="SWITCH:E-SWITCH_1??AV2?">
<description>&lt;b&gt;Toggle SPDT, right angle PCB, vertical actuation&lt;/b&gt;, C&amp;K E-Switch series, such as E101MD1AV2BE (on-on) or E103MD1AV2BE (on-off-on).</description>
</package>
<package name="BOURNS_3310">
<description>&lt;b&gt;Pot, Bourns 3310C&lt;/a&gt;, single turn, cheap: tempco ±1,000PPM, 50,000 cycle life.&lt;br&gt;
&lt;a href = "http://www.bourns.com/PDFs/3310.pdf"&gt;
http://www.bourns.com/PDFs/3310.pdf&lt;/a&gt;</description>
</package>
<package name="SOD323">
<description>&lt;b&gt;SOD-323, Diode&lt;/b&gt;Taken from http://www.nxp.com/documents/data_sheet/BZX384_SERIES.pdf</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOIC-20W">
<description>&lt;b&gt;SOIC-20&lt;/b&gt;, AKA Case 751D-05. This is the wide version, which is the more common.&lt;br&gt;
Based on  http://www.onsemi.com/pub/Collateral/MC100LVEL14-D.PDF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="QuantumOptics" package="LPCC-16" value="HMC1043"/>
<element name="4" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="11" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="2" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="5" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="13" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="12" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="3" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="14" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="1" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="15" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="16" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="9" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="6" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="R1" library="QuantumOptics" package="1608(0603)" value="10K@25°">
<attribute name="MFG" value="Cantherm"/>
<attribute name="PN" value="CMFA3970103JNT"/>
</element>
<element name="IC2" library="QuantumOptics" package="SOIC-8" value="ADR445BR">
<attribute name="NAME"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOIC-8" value="OPA2209AIDR">
<attribute name="NAME"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="C17" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="7" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="8" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="C1" library="QuantumOptics" package="1608(0603)" value="200nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C2" library="QuantumOptics" package="1608(0603)" value="1uF">
<attribute name="PN" value="C0603C105K4RACTU"/>
</element>
<element name="IC5" library="QuantumOptics" package="MSOP10" value="AD8253ARM">
<attribute name="NAME"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC9" library="QuantumOptics" package="SOT23-5" value="OPA209AIDB">
<attribute name="NAME"/>
</element>
<element name="C19" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C20" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="40.2K">
<attribute name="NAME"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="39pF">
<attribute name="NAME"/>
</element>
<element name="IC6" library="QuantumOptics" package="MSOP10" value="AD8253ARM">
<attribute name="NAME"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC10" library="QuantumOptics" package="SOT23-5" value="OPA209AIDB">
<attribute name="NAME"/>
</element>
<element name="C22" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="40.2K">
<attribute name="NAME"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C21" library="QuantumOptics" package="2012(0805)" value="39pF">
<attribute name="NAME"/>
</element>
<element name="IC7" library="QuantumOptics" package="MSOP10" value="AD8253ARM">
<attribute name="NAME"/>
</element>
<element name="C15" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC11" library="QuantumOptics" package="SOT23-5" value="OPA209AIDB">
<attribute name="NAME"/>
</element>
<element name="C25" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C26" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="40.2K">
<attribute name="NAME"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="C24" library="QuantumOptics" package="2012(0805)" value="39pF">
<attribute name="NAME"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="200">
<attribute name="NAME"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOT23-5" value="NC7S14M5X">
<attribute name="NAME"/>
</element>
<element name="10" library="QuantumOptics" package="TP,1MM_PAD,LONG" value="">
<attribute name="NAME"/>
</element>
<element name="C29" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="NAME"/>
</element>
<element name="C30" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="NAME"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="DESC" value="&quot;X&quot;"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="DESC" value="&quot;Y&quot;"/>
<attribute name="NAME"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="DESC" value="&quot;Z&quot;"/>
<attribute name="NAME"/>
</element>
<element name="J4" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="364A2595">
<attribute name="DESC" value=""/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="J5" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="364A2595">
<attribute name="DESC" value=""/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R11" library="QuantumOptics" package="BOURNS_3009P" value="20K">
<attribute name="PN" value="3005P-1-203"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="2.21M">
<attribute name="NAME"/>
</element>
<element name="R13" library="QuantumOptics" package="BOURNS_3009P" value="20K">
<attribute name="PN" value="3005P-1-203"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="2.21M">
<attribute name="NAME"/>
</element>
<element name="R15" library="QuantumOptics" package="BOURNS_3009P" value="20K">
<attribute name="PN" value="3005P-1-203"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="2.21M">
<attribute name="NAME"/>
</element>
<element name="IC12" library="QuantumOptics" package="NEC_PS2501L-1" value="PS2501L-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="200">
<attribute name="NAME"/>
</element>
<element name="L1" library="QuantumOptics" package="PANASONIC_ELLATV(COIL)" value="120uH">
<attribute name="PN" value="ELL-ATV121M"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="QuantumOptics" package="PANASONIC_ELLATV(COIL)" value="120uH">
<attribute name="PN" value="ELL-ATV121M"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="NAME"/>
</element>
<element name="C32" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="NAME"/>
</element>
<element name="PWR1" library="QuantumOptics" package="DC-DC:CC3-XXXXX-R-E(TDK/LAMBDA)" value="CC3-1212DR-E">
<attribute name="NAME"/>
</element>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="0.25A Med-Blo">
<attribute name="FUSE" value="20102500021P"/>
<attribute name="HOLDER" value="2 of 520101"/>
<attribute name="NAME"/>
</element>
<element name="C33" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="NAME"/>
<attribute name="PN" value="EEH-ZA1V680XP"/>
</element>
<element name="+12V" library="QuantumOptics" package="TP-0.042B" value="5001">
<attribute name="NAME"/>
</element>
<element name="RTN" library="QuantumOptics" package="TP-0.042B" value="5001">
<attribute name="NAME"/>
</element>
<element name="CBL1" library="QuantumOptics" package="MISC" value="1mmx16 FPC/FFC">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="PN1" value="Parlex 100R16-??B"/>
<attribute name="PN2" value="Molex 2103903??"/>
<attribute name="PN3" value="Wurth 686716???001"/>
</element>
<element name="CBL2" library="QuantumOptics" package="MISC" value="0.025&quot; ribbon cable">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C27" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="NAME"/>
</element>
<element name="C28" library="QuantumOptics" package="CAP,PANASONIC_D8,SMT,6.3MMROUND" value="68uF">
<attribute name="NAME"/>
</element>
<element name="IC13" library="QuantumOptics" package="MSOP8GND" value="ADP3654ARH">
<attribute name="NAME"/>
</element>
<element name="R28" library="QuantumOptics" package="BOURNS_3009P" value="20K">
<attribute name="PN" value="3005P-1-203"/>
<attribute name="DESC" value="&quot;S/R&quot;"/>
</element>
<element name="R29" library="QuantumOptics" package="2012(0805)" value="14.3K">
<attribute name="NAME"/>
</element>
<element name="Q1" library="QuantumOptics" package="SOT23" value="MMBT6427">
<attribute name="NAME"/>
</element>
<element name="U$39" library="QuantumOptics" package="CASE,HAMMOND_RL6105_RL6115" value=""/>
<element name="J6" library="QuantumOptics" package="CONN,RIBBON,2X10,SULLINS_SBH41-NBPB-D10-ST-__" value="SBH41-NBPB-D10-SP-BK">
<attribute name="NAME"/>
</element>
<element name="J7" library="QuantumOptics" package="CONN,RIBBON,2X10,SULLINS_SBH41-NBPB-D10-ST-__" value="SBH41-NBPB-D10-SP-BK">
<attribute name="NAME"/>
</element>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="R27" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="R30" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="NAME"/>
</element>
<element name="CASE1" library="QuantumOptics" package="MISC" value="Hammond RL6105(F)">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="CASE2" library="QuantumOptics" package="MISC" value="Hammond 1455L1201">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="J8" library="QuantumOptics" package="CONN,FPC-FFC,1MM,16-POS" value="FH12-16S-1SV(55)">
<attribute name="NAME"/>
</element>
<element name="C34" library="QuantumOptics" package="2012(0805)" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C39" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="QuantumOptics" package="2012(0805)" value="1.10M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="10.0M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="+" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="-" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="R36" library="QuantumOptics" package="2012(0805)" value="4.02K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED+" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="IC17" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="QuantumOptics" package="2012(0805)" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
</element>
<element name="J9" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227161-3">
<attribute name="NAME"/>
</element>
<element name="C36" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C37" library="QuantumOptics" package="2012(0805)" value="0 Ohm">
<attribute name="NAME"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="E101MD1AV2BE">
<attribute name="NAME"/>
</element>
<element name="R23" library="QuantumOptics" package="BOURNS_3310" value="10K">
<attribute name="PN" value="3310C-001-104L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="QuantumOptics" package="2012(0805)" value="56.2">
<attribute name="NAME"/>
</element>
<element name="C42" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH:E-SWITCH_1??AV2?" value="E101MD1AV2BE">
<attribute name="NAME"/>
</element>
<element name="D1" library="QuantumOptics" package="SOD323" value="B0540WS-7">
<attribute name="NAME"/>
</element>
<element name="R35" library="QuantumOptics" package="2012(0805)" value="56.2">
<attribute name="NAME"/>
</element>
<element name="L" library="QuantumOptics" package="TP-0.042B" value="5001">
<attribute name="NAME"/>
</element>
<element name="R" library="QuantumOptics" package="TP-0.042B" value="5001">
<attribute name="NAME"/>
</element>
<element name="COM" library="QuantumOptics" package="TP-0.042B" value="5001">
<attribute name="NAME"/>
</element>
<element name="3.5MM" library="QuantumOptics" package="MISC" value="35RAPC2BH3">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC14" library="QuantumOptics" package="SOT223" value="LM1117MPX-5.0">
<attribute name="NAME"/>
</element>
<element name="C40" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C43" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="LED-" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="CASE3" library="QuantumOptics" package="MISC" value="Hammond 1593P">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="CON1" library="QuantumOptics" package="MISC" value="SFH413-PPPB-D10-ID-BK">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="CON2" library="QuantumOptics" package="MISC" value="SFH413-PPPB-D10-ID-BK">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC15" library="QuantumOptics" package="SOT223" value="LM1117MPX-5.0">
<attribute name="NAME"/>
</element>
<element name="C44" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C45" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C47" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC16" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
</element>
<element name="C48" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="IC18" library="QuantumOptics" package="SOIC-20W" value="SA575DG"/>
<element name="PWR" library="QuantumOptics" package="MISC" value="EPS120050-P5P">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="4" pad="PAD"/>
</signal>
<signal name="N$2">
<contactref element="14" pad="PAD"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="6"/>
<contactref element="11" pad="PAD"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="15"/>
<contactref element="2" pad="PAD"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="3"/>
<contactref element="5" pad="PAD"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="1"/>
<contactref element="3" pad="PAD"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="11"/>
<contactref element="13" pad="PAD"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="10"/>
<contactref element="12" pad="PAD"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="4"/>
<contactref element="1" pad="PAD"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="16"/>
<contactref element="15" pad="PAD"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="14"/>
<contactref element="16" pad="PAD"/>
</signal>
<signal name="N$15">
<contactref element="6" pad="PAD"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="IC2" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC4" pad="5"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC5" pad="4"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="IC5" pad="9"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="IC9" pad="3"/>
<contactref element="IC6" pad="2"/>
<contactref element="IC6" pad="4"/>
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="IC6" pad="9"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="IC10" pad="3"/>
<contactref element="IC7" pad="2"/>
<contactref element="IC7" pad="4"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="IC7" pad="9"/>
<contactref element="C25" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="IC11" pad="3"/>
<contactref element="IC8" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="C27" pad="NEG"/>
<contactref element="C28" pad="POS"/>
<contactref element="R29" pad="1"/>
<contactref element="J6" pad="6"/>
<contactref element="J6" pad="5"/>
<contactref element="J6" pad="15"/>
<contactref element="J6" pad="16"/>
<contactref element="R3" pad="2"/>
<contactref element="J8" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="IC2" pad="6"/>
<contactref element="C6" pad="2"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="R4" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="IC4" pad="7"/>
<contactref element="R17" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="-15V">
<contactref element="IC4" pad="4"/>
<contactref element="C8" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="3"/>
<contactref element="C20" pad="2"/>
<contactref element="IC9" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="IC6" pad="6"/>
<contactref element="IC6" pad="3"/>
<contactref element="C23" pad="2"/>
<contactref element="IC10" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="3"/>
<contactref element="C26" pad="2"/>
<contactref element="IC11" pad="2"/>
<contactref element="C28" pad="NEG"/>
<contactref element="J6" pad="3"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="+15V">
<contactref element="IC4" pad="8"/>
<contactref element="C7" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="IC5" pad="8"/>
<contactref element="C19" pad="2"/>
<contactref element="IC9" pad="5"/>
<contactref element="C13" pad="2"/>
<contactref element="IC6" pad="8"/>
<contactref element="C22" pad="2"/>
<contactref element="IC10" pad="5"/>
<contactref element="C15" pad="2"/>
<contactref element="IC7" pad="8"/>
<contactref element="C25" pad="2"/>
<contactref element="IC11" pad="5"/>
<contactref element="C27" pad="POS"/>
<contactref element="R28" pad="CW"/>
<contactref element="Q1" pad="3"/>
<contactref element="J6" pad="1"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="IC4" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC8" pad="5"/>
<contactref element="C10" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="CW"/>
<contactref element="R13" pad="CW"/>
<contactref element="R15" pad="CW"/>
<contactref element="J8" pad="14"/>
<contactref element="J8" pad="10"/>
</signal>
<signal name="-5V">
<contactref element="R10" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R11" pad="CCW"/>
<contactref element="R13" pad="CCW"/>
<contactref element="R15" pad="CCW"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="X-">
<contactref element="IC5" pad="10"/>
<contactref element="J8" pad="5"/>
</signal>
<signal name="Y-">
<contactref element="IC6" pad="10"/>
<contactref element="J8" pad="11"/>
</signal>
<signal name="Z-">
<contactref element="IC7" pad="10"/>
<contactref element="J8" pad="12"/>
</signal>
<signal name="N$11">
<contactref element="7" pad="PAD"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC13" pad="1"/>
<contactref element="IC13" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="9" pad="PAD"/>
<contactref element="C2" pad="2"/>
<contactref element="IC13" pad="6"/>
</signal>
<signal name="N$24">
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$26">
<contactref element="IC5" pad="7"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R6" pad="2"/>
<contactref element="IC9" pad="4"/>
<contactref element="R18" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="IC6" pad="7"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="R7" pad="2"/>
<contactref element="IC10" pad="4"/>
<contactref element="R19" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="IC7" pad="7"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R8" pad="2"/>
<contactref element="IC11" pad="4"/>
<contactref element="R20" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="IC4" pad="6"/>
<contactref element="R10" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC5" pad="1"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="IC6" pad="1"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="IC7" pad="1"/>
<contactref element="J8" pad="13"/>
</signal>
<signal name="N$16">
<contactref element="J6" pad="10"/>
<contactref element="J8" pad="16"/>
</signal>
<signal name="N$42">
<contactref element="J6" pad="11"/>
<contactref element="J8" pad="15"/>
</signal>
<signal name="N$43">
<contactref element="J6" pad="12"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="J6" pad="13"/>
<contactref element="J8" pad="6"/>
</signal>
<signal name="N$44">
<contactref element="IC8" pad="4"/>
<contactref element="J8" pad="8"/>
</signal>
<signal name="N$47">
<contactref element="10" pad="PAD"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="IC8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="J6" pad="14"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="SHIELD2"/>
<contactref element="J2" pad="SHIELD1"/>
<contactref element="J3" pad="SHIELD2"/>
<contactref element="J3" pad="SHIELD1"/>
<contactref element="J5" pad="UPR-COM"/>
<contactref element="IC12" pad="3"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="J1" pad="SHIELD2"/>
<contactref element="C30" pad="POS"/>
<contactref element="C29" pad="NEG"/>
<contactref element="C31" pad="NEG"/>
<contactref element="C32" pad="POS"/>
<contactref element="PWR1" pad="COM"/>
<contactref element="J7" pad="6"/>
<contactref element="J7" pad="5"/>
<contactref element="J7" pad="16"/>
<contactref element="J7" pad="15"/>
</signal>
<signal name="N$49">
<contactref element="R26" pad="1"/>
<contactref element="J7" pad="7"/>
</signal>
<signal name="N$50">
<contactref element="R27" pad="1"/>
<contactref element="J7" pad="8"/>
</signal>
<signal name="N$51">
<contactref element="R30" pad="1"/>
<contactref element="J7" pad="9"/>
</signal>
<signal name="N$52">
<contactref element="J5" pad="UPR-CTR"/>
<contactref element="J7" pad="13"/>
</signal>
<signal name="N$53">
<contactref element="J4" pad="UPR-CTR"/>
<contactref element="J7" pad="10"/>
</signal>
<signal name="N$54">
<contactref element="J4" pad="LWR-CTR"/>
<contactref element="J7" pad="11"/>
</signal>
<signal name="N$55">
<contactref element="J4" pad="LWR-COM"/>
<contactref element="J4" pad="UPR-COM"/>
<contactref element="J7" pad="12"/>
</signal>
<signal name="N$18">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="WIPER"/>
</signal>
<signal name="N$33">
<contactref element="R14" pad="2"/>
<contactref element="R13" pad="WIPER"/>
</signal>
<signal name="N$38">
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="WIPER"/>
</signal>
<signal name="N$56">
<contactref element="J5" pad="LWR-CTR"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="R25" pad="1"/>
<contactref element="IC12" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="J5" pad="LWR-COM"/>
<contactref element="IC12" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="IC12" pad="4"/>
<contactref element="J7" pad="14"/>
</signal>
<signal name="N$59">
<contactref element="L1" pad="1"/>
<contactref element="C29" pad="POS"/>
<contactref element="J7" pad="1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="N$61">
<contactref element="L2" pad="1"/>
<contactref element="C30" pad="NEG"/>
<contactref element="J7" pad="3"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="N$62">
<contactref element="L2" pad="2"/>
<contactref element="C32" pad="NEG"/>
<contactref element="PWR1" pad="-VOUT"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="L1" pad="2"/>
<contactref element="C31" pad="POS"/>
<contactref element="PWR1" pad="+VOUT"/>
</signal>
<signal name="N$64">
<contactref element="PWR1" pad="RC"/>
<contactref element="PWR1" pad="-VIN"/>
<contactref element="C33" pad="NEG"/>
<contactref element="RTN" pad="TP"/>
</signal>
<signal name="N$67">
<contactref element="PWR1" pad="TRM"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="PWR1" pad="+VIN"/>
<contactref element="F1" pad="1A"/>
<contactref element="F1" pad="1B"/>
<contactref element="C33" pad="POS"/>
</signal>
<signal name="N$66">
<contactref element="F1" pad="2A"/>
<contactref element="F1" pad="2B"/>
<contactref element="+12V" pad="TP"/>
</signal>
<signal name="N$68">
<contactref element="IC13" pad="2"/>
<contactref element="IC13" pad="4"/>
<contactref element="8" pad="PAD"/>
</signal>
<signal name="N$14">
<contactref element="IC13" pad="7"/>
<contactref element="IC13" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R29" pad="2"/>
<contactref element="R28" pad="CCW"/>
</signal>
<signal name="N$46">
<contactref element="R28" pad="WIPER"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$71">
<contactref element="J6" pad="7"/>
<contactref element="IC9" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="C18" pad="2"/>
</signal>
<signal name="N$72">
<contactref element="J6" pad="8"/>
<contactref element="IC10" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="C21" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="J6" pad="9"/>
<contactref element="IC11" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="J3" pad="CONDUCTOR"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="J2" pad="CONDUCTOR"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="J1" pad="CONDUCTOR"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="R2" pad="1"/>
<contactref element="J8" pad="9"/>
</signal>
<signal name="N$32">
<contactref element="C5" pad="1"/>
<contactref element="IC18" pad="13"/>
</signal>
<signal name="N$37">
<contactref element="C3" pad="1"/>
<contactref element="IC18" pad="16"/>
</signal>
<signal name="N$45">
<contactref element="C34" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="SW1" pad="DOWN"/>
<contactref element="R23" pad="CW"/>
<contactref element="IC18" pad="14"/>
<contactref element="IC18" pad="11"/>
</signal>
<signal name="N$70">
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="C35" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="C34" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="IC18" pad="12"/>
</signal>
<signal name="N$75">
<contactref element="C36" pad="1"/>
<contactref element="IC18" pad="15"/>
</signal>
<signal name="N$77">
<contactref element="C38" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="R23" pad="CCW"/>
<contactref element="IC18" pad="8"/>
</signal>
<signal name="N$78">
<contactref element="C39" pad="2"/>
<contactref element="IC17" pad="5"/>
<contactref element="C49" pad="1"/>
<contactref element="C42" pad="2"/>
<contactref element="IC14" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="IC18" pad="20"/>
<contactref element="IC14" pad="4"/>
</signal>
<signal name="N$79">
<contactref element="C41" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="J9" pad="CONDUCTOR"/>
</signal>
<signal name="N$80">
<contactref element="R31" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="IC17" pad="3"/>
</signal>
<signal name="N$87">
<contactref element="C46" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="IC14" pad="3"/>
<contactref element="C43" pad="2"/>
<contactref element="IC15" pad="3"/>
<contactref element="C44" pad="2"/>
</signal>
<signal name="N$88">
<contactref element="LED+" pad="TP"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$89">
<contactref element="IC17" pad="4"/>
<contactref element="R37" pad="1"/>
<contactref element="R38" pad="2"/>
<contactref element="C50" pad="1"/>
</signal>
<signal name="N$91">
<contactref element="R38" pad="1"/>
<contactref element="C51" pad="2"/>
</signal>
<signal name="N$92">
<contactref element="R37" pad="2"/>
<contactref element="IC17" pad="1"/>
<contactref element="C50" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="SW1" pad="UP"/>
</signal>
<signal name="GNDX">
<contactref element="C35" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="-" pad="TP"/>
<contactref element="C49" pad="2"/>
<contactref element="IC17" pad="2"/>
<contactref element="C51" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="J9" pad="SHIELD1"/>
<contactref element="J9" pad="SHIELD2"/>
<contactref element="C36" pad="2"/>
<contactref element="C42" pad="1"/>
<contactref element="COM" pad="TP"/>
<contactref element="IC14" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="LED-" pad="TP"/>
<contactref element="IC15" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C47" pad="1"/>
<contactref element="IC16" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="IC18" pad="10"/>
</signal>
<signal name="N$82">
<contactref element="C3" pad="2"/>
<contactref element="SW1" pad="COM"/>
</signal>
<signal name="N$84">
<contactref element="C37" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="N$86">
<contactref element="R33" pad="1"/>
<contactref element="C41" pad="2"/>
</signal>
<signal name="N$90">
<contactref element="+" pad="TP"/>
<contactref element="SW2" pad="COM"/>
</signal>
<signal name="N$93">
<contactref element="SW2" pad="DOWN"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$85">
<contactref element="R23" pad="W"/>
<contactref element="IC16" pad="3"/>
</signal>
<signal name="N$76">
<contactref element="R35" pad="2"/>
<contactref element="L" pad="TP"/>
</signal>
<signal name="N$83">
<contactref element="R34" pad="2"/>
<contactref element="R" pad="TP"/>
</signal>
<signal name="N$94">
<contactref element="IC15" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="IC16" pad="5"/>
<contactref element="C48" pad="1"/>
<contactref element="IC15" pad="4"/>
</signal>
<signal name="N$96">
<contactref element="IC16" pad="4"/>
<contactref element="IC16" pad="1"/>
<contactref element="C37" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
