<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="8" y1="0" x2="65.75" y2="0" width="0" layer="20"/>
<wire x1="65.75" y1="0" x2="65.75" y2="5" width="0" layer="20"/>
<wire x1="73.5" y1="8" x2="73.5" y2="45.75" width="0" layer="20"/>
<wire x1="65.75" y1="53.5" x2="0" y2="53.5" width="0" layer="20"/>
<wire x1="0" y1="53.5" x2="0" y2="45.75" width="0" layer="20"/>
<wire x1="0" y1="45.75" x2="0" y2="8" width="0" layer="20"/>
<wire x1="0" y1="8" x2="5" y2="8" width="0" layer="20"/>
<wire x1="8" y1="5" x2="8" y2="0" width="0" layer="20"/>
<wire x1="5" y1="8" x2="8" y2="5" width="0" layer="20" curve="-90"/>
<wire x1="69" y1="8" x2="73.5" y2="8" width="0" layer="20"/>
<wire x1="69" y1="8" x2="65.75" y2="5" width="0" layer="20" curve="85.601295"/>
<wire x1="65.75" y1="48.75" x2="65.75" y2="53.5" width="0" layer="20"/>
<wire x1="73.5" y1="45.75" x2="68.75" y2="45.75" width="0" layer="20"/>
<wire x1="65.75" y1="48.75" x2="68.75" y2="45.75" width="0" layer="20" curve="90"/>
<wire x1="8" y1="48.75" x2="8" y2="53.5" width="0" layer="20"/>
<wire x1="5" y1="45.75" x2="0" y2="45.75" width="0" layer="20"/>
<wire x1="5" y1="45.75" x2="8" y2="48.75" width="0" layer="20" curve="90"/>
<hole x="4.8514" y="11.8618" drill="3.175"/>
<hole x="4.8514" y="41.8592" drill="3.175"/>
<hole x="68.8594" y="41.8592" drill="3.175"/>
<hole x="68.8594" y="11.8618" drill="3.175"/>
<text>White Flash</text>
<text>Rev: A
R. Marjoribanks Labs
University of Toronto</text>
</plain>
<libraries>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire. Has continious fence so will generate lots of DRCs which can be ignored.</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT.</description>
</package>
<package name="CAP:NICHICON_F91_C">
<description>&lt;b&gt;Capacitor, SMT, Nichicon F91-C&lt;/b&gt;, from http://rocky.digikey.com/weblib/Nichicon/Web%20Data/Tant%20SMT%20F91%20series%20engineering%20data.pdf</description>
</package>
<package name="PASSIVE_10MM">
<description>&lt;b&gt;Passive through-hole 10mm spacing&lt;/b&gt;</description>
</package>
<package name="EIA-A(SMA)">
<description>&lt;b&gt;EIA size A, AKA SMA&lt;/b&gt;, SMT.</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056 or lower profile 01110005MR.</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="CONN:BNC-AMP-TYPE3HORIZ">
<description>&lt;b&gt;BNC PCB &lt;u&gt;Horizontal&lt;/u&gt; mount connector&lt;/b&gt;, Amp, horizontal, e.g. 5226990-3,  nut 1-329631-2, shoulder washer 330620.</description>
</package>
<package name="LED_LUMILED_REBEL">
<description>&lt;b&gt;LED, Lumiled Rebel series&lt;/b&gt;, such as LXML-PM01-0100</description>
</package>
<package name="TO263">
<description>&lt;b&gt;TO-263&lt;/b&gt;, SMT power.</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, based on Vishay.</description>
</package>
<package name="RESISITOR,CURRENTSENSE,CADDOCK_SR10">
<description>&lt;b&gt;Current sense resistor&lt;/b&gt;, Caddock SR10 series, Kelvin.</description>
</package>
<package name="BOURNS:3296Y">
<description>&lt;b&gt;3296Y (multi, top adj), 3296Z (multi, side adj) or 3386X/H (1-turn, top) Trimpot&lt;/b&gt;, Bourns.  Staggered pins so can insert trimpot one way only.  http://www.bourns.com/pdf/3296.pdf</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="DC-DC,AG-SERIES(TO2KV)">
<description>&lt;b&gt;DC-DC converter, HV #1&lt;/b&gt;, based on XP-Emco AG series, 100V-2KV only, 1-1.5W</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, based on TI's version of JEDEC MO-175 Variant AA.</description>
</package>
<package name="CASE,HAMMOND_RL6105_RL6115">
<description>&lt;b&gt;Hammond plastic case, 80 x 60mm, 30/40mmH, rounded corners.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12V+" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="2.2uF">
<attribute name="PN" value=""/>
<attribute name="MFG" value=""/>
<attribute name="NAME"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="PN" value=""/>
<attribute name="MFG" value=""/>
<attribute name="NAME"/>
</element>
<element name="C2" library="QuantumOptics" package="CAP:NICHICON_F91_C" value="33uF">
<attribute name="PN" value="F911C336MCC"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="QuantumOptics" package="PASSIVE_10MM" value="4.7nF">
<attribute name="PN" value="ECW-F6472JL"/>
<attribute name="V" value="600V"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="QuantumOptics" package="CAP:NICHICON_F91_C" value="33uF">
<attribute name="PN" value="F911C336MCC"/>
<attribute name="NAME"/>
</element>
<element name="D2" library="QuantumOptics" package="EIA-A(SMA)" value="UA1MTR">
<attribute name="NAME"/>
</element>
<element name="D1" library="QuantumOptics" package="EIA-A(SMA)" value="UA1MTR">
<attribute name="NAME"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="250mA">
<attribute name="NAME"/>
</element>
<element name="HLDR1" library="QuantumOptics" package="MISC" value="01110005MR">
<attribute name="PN" value=""/>
<attribute name="MFG" value=""/>
<attribute name="NAME"/>
</element>
<element name="HLDR2" library="QuantumOptics" package="MISC" value="01110005MR">
<attribute name="PN" value=""/>
<attribute name="MFG" value=""/>
<attribute name="NAME"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227677-1">
<attribute name="NAME"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN:BNC-AMP-TYPE3HORIZ" value="5227677-1">
<attribute name="NAME"/>
</element>
<element name="LED1B" library="QuantumOptics" package="LED_LUMILED_REBEL" value="LXML-PM01-0100">
<attribute name="NAME"/>
</element>
<element name="Q2" library="QuantumOptics" package="TO263" value="SPB17N80C3">
<attribute name="NAME"/>
</element>
<element name="Q1" library="QuantumOptics" package="SOT23" value="MMBT3906">
<attribute name="NAME"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R14" library="QuantumOptics" package="RESISITOR,CURRENTSENSE,CADDOCK_SR10" value="SR10-0.1-1%">
<attribute name="NAME"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="R13" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R10" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="1.2">
<attribute name="NAME"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="5.6">
<attribute name="NAME"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="24.9K">
<attribute name="NAME"/>
</element>
<element name="R5" library="QuantumOptics" package="BOURNS:3296Y" value="10K">
<attribute name="PN" value="3296Y-1-103"/>
<attribute name="NAME"/>
</element>
<element name="RET" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="U3" library="QuantumOptics" package="SOIC-8" value="NCP81074A">
<attribute name="NAME"/>
</element>
<element name="U2" library="QuantumOptics" package="DC-DC,AG-SERIES(TO2KV)" value="AG05P-12">
<attribute name="NAME"/>
</element>
<element name="U1" library="QuantumOptics" package="SOT23-5" value="AD8065ARTZ">
<attribute name="NAME"/>
</element>
<element name="U$24" library="QuantumOptics" package="CASE,HAMMOND_RL6105_RL6115" value=""/>
<element name="CASE" library="QuantumOptics" package="MISC" value="RL6115">
<attribute name="PN" value=""/>
<attribute name="MFG" value=""/>
<attribute name="NAME"/>
</element>
<element name="HV+" library="QuantumOptics" package="TP-0.042B" value=""/>
<element name="COM" library="QuantumOptics" package="TP-0.042B" value=""/>
<element name="LED1A" library="QuantumOptics" package="LED_LUMILED_REBEL" value="LXML-PM01-0100"/>
<element name="SWITCH" library="QuantumOptics" package="MISC" value="M2112LCW01">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="ACDC" library="QuantumOptics" package="MISC" value="PSM03A-120-R">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="8"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="U2" pad="HV-"/>
<contactref element="U2" pad="IN-"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="CCW"/>
<contactref element="Q1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="R13" pad="1"/>
<contactref element="D2" pad="K"/>
<contactref element="J1" pad="SHIELD2"/>
<contactref element="J1" pad="SHIELD1"/>
<contactref element="R14" pad="CUR2"/>
<contactref element="RET" pad="TP"/>
<contactref element="C9" pad="-"/>
<contactref element="COM" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="R9" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="J1" pad="CONDUCTOR"/>
</signal>
<signal name="+12V">
<contactref element="C9" pad="+"/>
<contactref element="F1" pad="2A"/>
<contactref element="F1" pad="2B"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="7"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="U3" pad="5"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U3" pad="4"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="4"/>
<contactref element="R8" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="CTRL"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="3"/>
<contactref element="R5" pad="W"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="HV+"/>
<contactref element="R4" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="1"/>
<contactref element="R5" pad="CW"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="R1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="N$15">
<contactref element="R13" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="LED1B" pad="K"/>
<contactref element="LED1A" pad="K"/>
</signal>
<signal name="N$16">
<contactref element="R7" pad="2"/>
<contactref element="HV+" pad="TP"/>
</signal>
<signal name="N$18">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="J2" pad="SHIELD1"/>
<contactref element="J2" pad="SHIELD2"/>
<contactref element="R14" pad="SEN2"/>
</signal>
<signal name="N$17">
<contactref element="LED1B" pad="A"/>
<contactref element="R14" pad="CUR1"/>
<contactref element="LED1A" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="J2" pad="CONDUCTOR"/>
<contactref element="R14" pad="SEN1"/>
</signal>
<signal name="N$22">
<contactref element="12V+" pad="TP"/>
<contactref element="F1" pad="1A"/>
<contactref element="F1" pad="1B"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
