<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="166.5" y2="0" width="0" layer="20"/>
<wire x1="166.5" y1="0" x2="166.5" y2="191.5" width="0" layer="20"/>
<wire x1="166.5" y1="191.5" x2="0" y2="191.5" width="0" layer="20"/>
<wire x1="0" y1="191.5" x2="0" y2="0" width="0" layer="20"/>
<hole x="143.55" y="20.69" drill="3.175"/>
<hole x="143.55" y="70.69" drill="3.175"/>
<hole x="143.55" y="120.69" drill="3.175"/>
<hole x="143.55" y="170.69" drill="3.175"/>
<text>Differential
Conductance</text>
<text>A</text>
<text>A. Stummer July'13</text>
<text>0.18mm</text>
<text>1mm</text>
<text>0.18mm</text>
<text>0.1mm</text>
<text>0.25mm</text>
<text>Differential Conductance
University of Toronto
K. Burch Labs
Rev:A</text>
</plain>
<libraries>
<library name="QuantumOptics">
<description>&lt;b&gt;U of T Physics, Quantum Optics Labs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Alan Stummer, Nov '03&lt;/author&gt;&lt;p&gt;
Various devices, symbols and packages used here.</description>
<packages>
<package name="MSOP10">
<description>&lt;b&gt;MSOP-10&lt;/b&gt; with 4.8mm row spacing.  Sameas Maxim's µsop-10.</description>
</package>
<package name="VISHAY_WSC4527">
<description>&lt;b&gt;Vishay/Dale WSC4527 2W SMT power resistor&lt;/b&gt;</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, based on Kemet's description.</description>
</package>
<package name="SOIC-14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;, TO-252, TS-003</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;MSOP-8&lt;/b&gt;, A.K.A. RM-8.  Use 0.025" grid.</description>
</package>
<package name="CSX750(CITIZEN_OSC)">
<description>&lt;b&gt;ASVxxx from Abracon&lt;/b&gt;, formerly CSX750 by Citizen, +3.3V or +5V, 1MHZ to 133MHz.</description>
</package>
<package name="BOURNS_5322(4WIRE)">
<description>&lt;b&gt;Resistor, pseudo-Kelvin&lt;/b&gt;, Bourns PWR5322Wxxx, actually 2 split terminals.</description>
</package>
<package name="CONN:BNC,DUAL(BOMAR)">
<description>&lt;b&gt;Dual BNC, vertical throughhole, isolated&lt;/b&gt;, Bomar, e.g. 364A2595, H=29.3mm, http://media.digikey.com/pdf/Data%20Sheets/Bomar%20PDFs/BNC_Products_Spec.pdf</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, based on TI's version of JEDEC MO-175 Variant AA.</description>
</package>
<package name="DISPLAY:3WIRE">
<description>&lt;b&gt;LCD display module&lt;/b&gt;, serial (RS232, I2C or SPI), actually just the connector.  e.g. Newhaven Display Intl NHD-0216B3Z-FL-GBW&lt;br&gt;
http://www.newhavendisplay.com/pdf/nhd-0216b3z-fl-gbw.pdf</description>
</package>
<package name="HEATSINK:274-2AB(WAKEFIELD,25C/W)">
<description>&lt;b&gt;Heatsink&lt;/b&gt;, Wakefield #274-2AB, through-hole for TO-220 or just on a plane, 0.5"H, 25°/W&lt;br&gt;
Use 0.15" (3.8mm) hole, has 0.52"x0.75" footprint&lt;br&gt;
Can also fit 274-1AB, 0.375"H, 28°/W.&lt;br&gt;
http://www.wakefield.com/pdf/Low%20Power.pdf</description>
</package>
<package name="EIA-7343">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, EIA-7343-xx, SMT, such as Kemet T530 case D, X or Y.&lt;br&gt;
&lt;a href="http://www.kemet.com/kemet/web/homepage/kechome.nsf/weben/33821761A656A8D9CA2570A50016091D/$file/F3102T530.pdff"&gt;
http://www.kemet.com/kemet/web/homepage/kechome.nsf/weben/33821761A656A8D9CA2570A50016091D/$file/F3102T530.pdf&lt;/a&gt;</description>
</package>
<package name="RABBIT_RCM42XX(THRU)">
<description>&lt;b&gt;RCM42xx Rabbit module&lt;/b&gt;, really just a 1x25 1.27mm connector such as Samtec SFM(L)-125-01-S-D (if no -125- use -130 30-position and cut short).</description>
</package>
<package name="MISC">
<description>&lt;b&gt;Misc Part&lt;/b&gt;, part not on board but placeholder so it shows up on the BOM.</description>
</package>
<package name="SWITCH,GRAYHILL_71BDF36">
<description>&lt;b&gt;Rotary Switch, 2 deck, 10 position&lt;/b&gt;, such as Grayhill 71BDF36-02PAJN. Has alternate commons for 2 poles per deck.</description>
</package>
<package name="SOT23-6">
<description>&lt;B&gt;SOT-23 6-pin&lt;/B&gt;, on wonderful 0.95mm (~0.037") pad-pad spacing.</description>
</package>
<package name="FUSE">
<description>&lt;B&gt;Fuse Holder&lt;/B&gt;, 5 x 20 mm, from two of Littlefuse 100056.http://www.littelfuse.com/data/en/Data_Sheets/0105_129_clips.pdf</description>
</package>
<package name="SOIC-8">
<description>&lt;b&gt;SOIC-8 (AKA SO-8)&lt;/b&gt;, pads on 0.050" grid.</description>
</package>
<package name="SWITCH,C&amp;K_7000_4PDT">
<description>&lt;b&gt;Switch, 4PDT, C&amp;K 7000 Series&lt;/b&gt;, RA through-hole, such as 7401MD9AV2BE.</description>
</package>
<package name="DPAK(CASE369C)">
<description>&lt;b&gt;DPAK, AKA Case 369C&lt;/b&gt;, based on On Semi specs.</description>
</package>
<package name="TP-0.042B">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point such as Keystone 5002K, or wire.  Has fence (bit larger than other TP) around to allow easier soldering.  Drilled 0.0465, plated down to 1.1mm.</description>
</package>
<package name="DC-DC:CC3-XXXXX-R-E(TDK/LAMBDA)">
<description>&lt;b&gt;CC3-inoutsR-E&lt;/b&gt;, TDK DC-DC isolated, 3W, uni- or bipolar&lt;br&gt;
"in": Input 05, 12, 24 or 48V.&lt;br&gt;
"out": Output 3.3, 5, 12, ±12 (or 24), ±15 (or30V).&lt;br&gt;
"s": Polarity single or dual.&lt;br&gt;
Case horiz SMD.&lt;br&gt;
http://www.tdk.co.jp/tefe02/ea335_cc_e.pdf</description>
</package>
<package name="TO263">
<description>&lt;b&gt;TO-263&lt;/b&gt;, SMT power.</description>
</package>
<package name="RELAY:DPDT-LATCHING(OMRON_G6SK-2F)">
<description>&lt;b&gt;DPDT, latching, dual coil&lt;/b&gt;, Omron G6SK-2F and Panasonic TX2SA-LT-, drop-in replacements.</description>
</package>
<package name="SOIC-24-0.3">
<description>&lt;b&gt;SOIC-24&lt;/b&gt; with 0.3"c-c rows and 0.05" pin spacing.</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;, based on Vishay.</description>
</package>
<package name="CASE:HAMMOND_1598D">
<description>&lt;b&gt;Case, Hammond 1598D&lt;/b&gt;, case is 206mmW x 180D x 64H, http://www.hammondmfg.com/pdf/1598D.pdf.&lt;br&gt;
Has 0.5mm space between PCB and inside of front and back plates, larger gap at sides.</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="TITLEBLOCK_PCB">
<description>&lt;b&gt;Title block&lt;/b&gt;, for use on board layouts.  Put below and outside the board outline.  
Add Targets.  On layer 100, add who drew it, drawing name and revision letter.</description>
</package>
<package name="PLACEHOLDER">
<description>&lt;b&gt;Non-existant decal, a Placeholder&lt;/b&gt;, used to make a part which does not need a package but Eagle demands something, e.g. if making schematic only and don't care about PCB.&lt;br&gt;
Pins are labeled "1" through "50".</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC3" library="QuantumOptics" package="MSOP10" value="AD9833B">
<attribute name="NAME"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC5" library="QuantumOptics" package="MSOP10" value="AD5162BRM10">
<attribute name="NAME"/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="IC4" library="QuantumOptics" package="SOIC-14" value="AD5552BR">
<attribute name="NAME"/>
</element>
<element name="C7" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="49.9K">
<attribute name="NAME"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="IC1" library="QuantumOptics" package="MSOP8" value="ADR444ARM">
<attribute name="NAME"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
<attribute name="NAME"/>
</element>
<element name="IC2" library="QuantumOptics" package="CSX750(CITIZEN_OSC)" value="CSX750FCC10.000M-UT">
<attribute name="NAME"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R33" library="QuantumOptics" package="BOURNS_5322(4WIRE)" value="1">
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="PWR5322W1R00JE"/>
<attribute name="NAME"/>
</element>
<element name="R34" library="QuantumOptics" package="VISHAY_WSC4527" value="10">
<attribute name="MFG" value="Vishay/Dale"/>
<attribute name="SPEC" value="1% ±20PPM/°"/>
<attribute name="PN" value="WSC452710R00F"/>
<attribute name="NAME"/>
</element>
<element name="R35" library="QuantumOptics" package="VISHAY_WSC4527" value="100">
<attribute name="MFG" value="Vishay/Dale"/>
<attribute name="SPEC" value="1% ±20PPM/°"/>
<attribute name="PN" value="WSC4527100R0FEA"/>
<attribute name="NAME"/>
</element>
<element name="R36" library="QuantumOptics" package="2012(0805)" value="1K">
<attribute name="MFG" value="TE Connectivity"/>
<attribute name="SPEC" value="0.1% ±10PPM/°"/>
<attribute name="PN" value="RN73C2A1K0BTDF"/>
<attribute name="NAME"/>
</element>
<element name="R38" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="MFG" value="TE Connectivity"/>
<attribute name="SPEC" value="0.1% ±10PPM/°"/>
<attribute name="PN" value="RN73C2A100KBTDF"/>
<attribute name="NAME"/>
</element>
<element name="R37" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="MFG" value="TE Connectivity"/>
<attribute name="SPEC" value="0.1% ±10PPM/°"/>
<attribute name="PN" value="RN73C2A10KBTDF"/>
<attribute name="NAME"/>
</element>
<element name="R39" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="J3" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="364A2595">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC17" library="QuantumOptics" package="MSOP8" value="AD7694BRM">
<attribute name="NAME"/>
</element>
<element name="C48" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
<attribute name="NAME"/>
</element>
<element name="C47" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C39" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R48" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="C46" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R55" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="R56" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="IC16" library="QuantumOptics" package="MSOP10" value="AD8253ARM">
<attribute name="NAME"/>
</element>
<element name="C44" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C45" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R49" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="IC18" library="QuantumOptics" package="MSOP8" value="AD7694BRM">
<attribute name="NAME"/>
</element>
<element name="C51" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
<attribute name="NAME"/>
</element>
<element name="C50" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R58" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="R59" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="DIS1" library="QuantumOptics" package="DISPLAY:3WIRE" value="NHD-0220D3Z-FL-GBW-ND">
<attribute name="MFG" value="Newhaven Display Intl."/>
<attribute name="NAME"/>
</element>
<element name="C21" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C30" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEF-UD0J101R"/>
<attribute name="NAME"/>
</element>
<element name="MOD1" library="QuantumOptics" package="RABBIT_RCM42XX(THRU)" value="RCM4210">
<attribute name="NAME"/>
</element>
<element name="CONN1" library="QuantumOptics" package="MISC" value="SFML-125-01-S-D ">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SW2" library="QuantumOptics" package="SWITCH,GRAYHILL_71BDF36" value="71BDF36-02PAJN">
<attribute name="NAME"/>
<attribute name="ALT" value="71ADF36-02PAJN"/>
</element>
<element name="IC7" library="QuantumOptics" package="SOT23-6" value="TLV3501AIDBVR">
<attribute name="NAME"/>
</element>
<element name="R40" library="QuantumOptics" package="BOURNS_5322(4WIRE)" value="dns">
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="PWR5322W1R00JE"/>
<attribute name="NAME"/>
</element>
<element name="R41" library="QuantumOptics" package="BOURNS_5322(4WIRE)" value="dns">
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="PWR5322W1R00JE"/>
<attribute name="NAME"/>
</element>
<element name="R42" library="QuantumOptics" package="BOURNS_5322(4WIRE)" value="dns">
<attribute name="MFG" value="Bourns"/>
<attribute name="PN" value="PWR5322W1R00JE"/>
<attribute name="NAME"/>
</element>
<element name="J2" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="364A2595">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C19" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="499K">
<attribute name="NAME"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
<attribute name="NAME"/>
</element>
<element name="Q2" library="QuantumOptics" package="TO252" value="STD878">
<attribute name="NAME"/>
</element>
<element name="Q3" library="QuantumOptics" package="TO252" value="STD888">
<attribute name="NAME"/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="C15" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="SW1" library="QuantumOptics" package="SWITCH,GRAYHILL_71BDF36" value="71BDF36-02PAJN">
<attribute name="NAME"/>
<attribute name="ALT" value="71ADF36-02PAJN"/>
</element>
<element name="R8" library="QuantumOptics" package="VISHAY_WSC4527" value="out">
<attribute name="NAME"/>
</element>
<element name="R9" library="QuantumOptics" package="VISHAY_WSC4527" value="WSC452710R00F">
<attribute name="NAME"/>
</element>
<element name="R10" library="QuantumOptics" package="VISHAY_WSC4527" value="WSC4527100R0F">
<attribute name="NAME"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="392">
<attribute name="NAME"/>
</element>
<element name="R18" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R66" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R45" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R12" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R13" library="QuantumOptics" package="2012(0805)" value="475">
<attribute name="NAME"/>
</element>
<element name="R14" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R15" library="QuantumOptics" package="2012(0805)" value="475">
<attribute name="NAME"/>
</element>
<element name="R16" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="R17" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="R19" library="QuantumOptics" package="2012(0805)" value="10">
<attribute name="NAME"/>
</element>
<element name="R20" library="QuantumOptics" package="2012(0805)" value="10">
<attribute name="NAME"/>
</element>
<element name="R21" library="QuantumOptics" package="2012(0805)" value="1">
<attribute name="NAME"/>
</element>
<element name="R22" library="QuantumOptics" package="2012(0805)" value="1">
<attribute name="NAME"/>
</element>
<element name="R23" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="R24" library="QuantumOptics" package="2012(0805)" value="out">
<attribute name="NAME"/>
</element>
<element name="IC6" library="QuantumOptics" package="SOT23-5" value="OP184FS">
<attribute name="NAME"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="F2" library="QuantumOptics" package="FUSE" value="0.4A">
<attribute name="NAME"/>
</element>
<element name="FUSE2" library="QuantumOptics" package="MISC" value="100056">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="FUSE3" library="QuantumOptics" package="MISC" value="100056">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C49" library="QuantumOptics" package="2012(0805)" value="39nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R50" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="C41" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C42" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C43" library="QuantumOptics" package="2012(0805)" value="short">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R53" library="QuantumOptics" package="2012(0805)" value="delete">
<attribute name="NAME"/>
</element>
<element name="R29" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
</element>
<element name="IC19" library="QuantumOptics" package="MSOP8" value="ADR444ARM">
<attribute name="NAME"/>
</element>
<element name="C53" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R61" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="C52" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R60" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R47" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="C38" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC14" library="QuantumOptics" package="SOIC-8" value="OP284ES">
<attribute name="NAME"/>
</element>
<element name="C40" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R51" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="R52" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="F1" library="QuantumOptics" package="FUSE" value="???">
<attribute name="PN" value="100056"/>
<attribute name="NAME"/>
</element>
<element name="FUSE1" library="QuantumOptics" package="MISC" value="???A">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C36" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
</element>
<element name="C37" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R62" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R64" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="IC13" library="QuantumOptics" package="SOIC-8" value="AD8221BR">
<attribute name="NAME"/>
</element>
<element name="C34" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C35" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R43" library="QuantumOptics" package="2012(0805)" value="5.49K">
<attribute name="NAME"/>
</element>
<element name="R46" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="IC23" library="QuantumOptics" package="MSOP8" value="AD7694BRM">
<attribute name="NAME"/>
</element>
<element name="C66" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
<attribute name="NAME"/>
</element>
<element name="C65" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C56" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R70" library="QuantumOptics" package="2012(0805)" value="332K">
<attribute name="NAME"/>
</element>
<element name="C64" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R77" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="R78" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="IC22" library="QuantumOptics" package="MSOP10" value="AD8253ARM">
<attribute name="NAME"/>
</element>
<element name="C62" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C63" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R71" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="IC24" library="QuantumOptics" package="MSOP8" value="AD7694BRM">
<attribute name="NAME"/>
</element>
<element name="C69" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
<attribute name="NAME"/>
</element>
<element name="C68" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R80" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="R81" library="QuantumOptics" package="2012(0805)" value="499">
<attribute name="NAME"/>
</element>
<element name="C67" library="QuantumOptics" package="2012(0805)" value="39nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R72" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="C59" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C60" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C61" library="QuantumOptics" package="2012(0805)" value="short">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R75" library="QuantumOptics" package="2012(0805)" value="delete">
<attribute name="NAME"/>
</element>
<element name="IC25" library="QuantumOptics" package="MSOP8" value="ADR444ARM">
<attribute name="NAME"/>
</element>
<element name="C71" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R83" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="C70" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R82" library="QuantumOptics" package="2012(0805)" value="1M">
<attribute name="NAME"/>
</element>
<element name="R69" library="QuantumOptics" package="2012(0805)" value="29.4K">
<attribute name="NAME"/>
</element>
<element name="C55" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC20" library="QuantumOptics" package="SOIC-8" value="OP284ES">
<attribute name="NAME"/>
</element>
<element name="C57" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R73" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="R74" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
</element>
<element name="C54" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
</element>
<element name="C58" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="SW3" library="QuantumOptics" package="SWITCH,C&amp;K_7000_4PDT" value="7401MD9AV2BE"/>
<element name="J4" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="364A2595">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R67" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="J1" library="QuantumOptics" package="CONN:BNC,DUAL(BOMAR)" value="364A2595">
<attribute name="DESC" value=""/>
<attribute name="MFG" value="Bomar"/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="R44" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R63" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="R65" library="QuantumOptics" package="2012(0805)" value="100">
<attribute name="NAME"/>
</element>
<element name="IC9" library="QuantumOptics" package="DPAK(CASE369C)" value="L4941">
<attribute name="NAME"/>
</element>
<element name="C31" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEF-UD0J101R"/>
<attribute name="NAME"/>
</element>
<element name="IC10" library="QuantumOptics" package="DPAK(CASE369C)" value="L4941">
<attribute name="NAME"/>
</element>
<element name="C32" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEF-UD0J101R"/>
<attribute name="NAME"/>
</element>
<element name="IC11" library="QuantumOptics" package="DPAK(CASE369C)" value="L4931ABDT33">
<attribute name="NAME"/>
</element>
<element name="R32" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="+6V" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="6V-RET" library="QuantumOptics" package="TP-0.042B" value="">
<attribute name="NAME"/>
</element>
<element name="PWR1" library="QuantumOptics" package="DC-DC:CC3-XXXXX-R-E(TDK/LAMBDA)" value="CC3-0505SR-E">
<attribute name="NAME"/>
</element>
<element name="C28" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEF-UD0J101R"/>
<attribute name="NAME"/>
</element>
<element name="R31" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="C24" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C22" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C25" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C26" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C23" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C20" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="C27" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC12" library="QuantumOptics" package="TO263" value="LM2990SX-5.0">
<attribute name="NAME"/>
</element>
<element name="C33" library="QuantumOptics" package="EIA-7343" value="100uF">
<attribute name="MFG" value="Panasonic"/>
<attribute name="PN" value="EEF-UD0J101R"/>
<attribute name="NAME"/>
</element>
<element name="C29" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="HS3" library="QuantumOptics" package="HEATSINK:274-2AB(WAKEFIELD,25C/W)" value="274-2AB">
<attribute name="NAME"/>
</element>
<element name="CAT1" library="QuantumOptics" package="MISC" value="???">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="DB1" library="QuantumOptics" package="MISC" value="???">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
</element>
<element name="IC15" library="QuantumOptics" package="SOIC-8" value="OP284ES">
<attribute name="NAME"/>
</element>
<element name="R57" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
</element>
<element name="R54" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="RLY1" library="QuantumOptics" package="RELAY:DPDT-LATCHING(OMRON_G6SK-2F)" value="TX2SA-LT-5V-Z">
<attribute name="ALT" value="G6SK-2F-DC5"/>
<attribute name="NAME"/>
</element>
<element name="IC8" library="QuantumOptics" package="SOIC-24-0.3" value="TLE7230G">
<attribute name="NAME"/>
</element>
<element name="C17" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="Q1" library="QuantumOptics" package="SOT23" value="ZXMP10A13F">
<attribute name="NAME"/>
</element>
<element name="IC21" library="QuantumOptics" package="SOIC-8" value="OP284ES">
<attribute name="NAME"/>
</element>
<element name="R79" library="QuantumOptics" package="2012(0805)" value="20K">
<attribute name="NAME"/>
</element>
<element name="R76" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
</element>
<element name="RLY2" library="QuantumOptics" package="RELAY:DPDT-LATCHING(OMRON_G6SK-2F)" value="TX2SA-LT-5V-Z">
<attribute name="ALT" value="G6SK-2F-DC5"/>
<attribute name="NAME"/>
</element>
<element name="R25" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
</element>
<element name="R26" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
</element>
<element name="R27" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
</element>
<element name="R28" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
</element>
<element name="R30" library="QuantumOptics" package="2012(0805)" value="2K">
<attribute name="NAME"/>
</element>
<element name="U$98" library="QuantumOptics" package="CASE:HAMMOND_1598D" value=""/>
<element name="R68" library="QuantumOptics" package="2012(0805)" value="0">
<attribute name="NAME"/>
</element>
<element name="D2" library="QuantumOptics" package="SOT223" value="BAT160S,115">
<attribute name="NAME"/>
</element>
<element name="D1" library="QuantumOptics" package="SOT223" value="BAT160S,115">
<attribute name="NAME"/>
</element>
<element name="D3" library="QuantumOptics" package="SOT223" value="BAT160S,115">
<attribute name="NAME"/>
</element>
<element name="U$96" library="QuantumOptics" package="TITLEBLOCK_PCB" value="">
<attribute name="LAST_DATE_TIME"/>
<attribute name="DRAWING_NAME"/>
</element>
<element name="C72" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="D4" library="QuantumOptics" package="PLACEHOLDER" value=""/>
<element name="D5" library="QuantumOptics" package="PLACEHOLDER" value=""/>
<element name="C73" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="R84" library="QuantumOptics" package="2012(0805)" value="10K"/>
<element name="C74" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="D6" library="QuantumOptics" package="PLACEHOLDER" value=""/>
<element name="C75" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C76" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
</element>
<element name="C77" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
</element>
<element name="C78" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
</element>
<element name="C79" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="MFG" value="Kemet"/>
<attribute name="PN" value="C0805C106K9RACTU"/>
</element>
<element name="R85" library="QuantumOptics" package="2012(0805)" value="10K"/>
<element name="C80" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="D7" library="QuantumOptics" package="PLACEHOLDER" value=""/>
<element name="C81" library="QuantumOptics" package="2012(0805)" value="1nF"/>
<element name="R86" library="QuantumOptics" package="2012(0805)" value="61.9K"/>
<element name="C82" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="DIS1" pad="COM"/>
<contactref element="MOD1" pad="50"/>
<contactref element="MOD1" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="C30" pad="-"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="IC9" pad="2"/>
<contactref element="IC11" pad="2"/>
<contactref element="C32" pad="-"/>
<contactref element="6V-RET" pad="TP"/>
<contactref element="R32" pad="1"/>
<contactref element="PWR1" pad="RC"/>
<contactref element="PWR1" pad="-VIN"/>
<contactref element="C24" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="IC3" pad="9"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC4" pad="4"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="C48" pad="1"/>
<contactref element="C47" pad="1"/>
<contactref element="IC17" pad="4"/>
<contactref element="C39" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="IC18" pad="4"/>
<contactref element="C13" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="R66" pad="1"/>
<contactref element="R45" pad="1"/>
<contactref element="IC5" pad="9"/>
<contactref element="R2" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="R62" pad="1"/>
<contactref element="R64" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="R46" pad="1"/>
<contactref element="C66" pad="1"/>
<contactref element="C65" pad="1"/>
<contactref element="IC23" pad="4"/>
<contactref element="C56" pad="1"/>
<contactref element="C62" pad="1"/>
<contactref element="C63" pad="1"/>
<contactref element="C69" pad="1"/>
<contactref element="C68" pad="1"/>
<contactref element="IC24" pad="4"/>
<contactref element="C59" pad="1"/>
<contactref element="C60" pad="1"/>
<contactref element="C57" pad="1"/>
<contactref element="R67" pad="1"/>
<contactref element="R44" pad="1"/>
<contactref element="R63" pad="1"/>
<contactref element="R65" pad="1"/>
<contactref element="IC10" pad="2"/>
<contactref element="C31" pad="-"/>
<contactref element="R32" pad="2"/>
<contactref element="PWR1" pad="+VOUT"/>
<contactref element="C28" pad="+"/>
<contactref element="C25" pad="1"/>
<contactref element="C33" pad="+"/>
<contactref element="IC12" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC4" pad="12"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R68" pad="1"/>
<contactref element="D2" pad="4"/>
<contactref element="D1" pad="3"/>
<contactref element="D1" pad="1"/>
<contactref element="IC22" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC8" pad="17"/>
<contactref element="IC8" pad="5"/>
<contactref element="IC8" pad="20"/>
<contactref element="IC8" pad="6"/>
<contactref element="IC8" pad="18"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC8" pad="7"/>
<contactref element="IC8" pad="19"/>
<contactref element="C17" pad="1"/>
<contactref element="IC16" pad="2"/>
<contactref element="C72" pad="1"/>
<contactref element="IC7" pad="2"/>
<contactref element="IC7" pad="6"/>
<contactref element="C14" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="C73" pad="1"/>
<contactref element="R71" pad="2"/>
<contactref element="D6" pad="1"/>
<contactref element="C75" pad="1"/>
<contactref element="C76" pad="2"/>
<contactref element="C77" pad="2"/>
<contactref element="C78" pad="2"/>
<contactref element="C79" pad="2"/>
<contactref element="R49" pad="2"/>
<contactref element="D7" pad="1"/>
<contactref element="C82" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="IC3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="DIS1" pad="VDD"/>
<contactref element="C18" pad="1"/>
<contactref element="C30" pad="+"/>
<contactref element="IC9" pad="3"/>
<contactref element="C24" pad="2"/>
<contactref element="IC8" pad="23"/>
<contactref element="IC8" pad="11"/>
<contactref element="IC8" pad="24"/>
<contactref element="C17" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="IC3" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C8" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="!POT_CS">
<contactref element="IC5" pad="8"/>
<contactref element="MOD1" pad="11"/>
</signal>
<signal name="SCLK">
<contactref element="IC5" pad="6"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC17" pad="7"/>
<contactref element="IC16" pad="4"/>
<contactref element="IC18" pad="7"/>
<contactref element="MOD1" pad="14"/>
<contactref element="IC23" pad="7"/>
<contactref element="IC24" pad="7"/>
<contactref element="IC22" pad="4"/>
<contactref element="IC8" pad="13"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="SDATA">
<contactref element="IC5" pad="7"/>
<contactref element="IC3" pad="6"/>
<contactref element="IC4" pad="10"/>
<contactref element="IC16" pad="5"/>
<contactref element="MOD1" pad="15"/>
<contactref element="IC22" pad="5"/>
<contactref element="IC8" pad="14"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="!OSC_CS">
<contactref element="IC3" pad="8"/>
<contactref element="MOD1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="IC3" pad="10"/>
<contactref element="IC5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C72" pad="2"/>
</signal>
<signal name="!DAC_LDAC">
<contactref element="IC4" pad="11"/>
<contactref element="MOD1" pad="13"/>
</signal>
<signal name="!DAC_CS">
<contactref element="IC4" pad="7"/>
<contactref element="MOD1" pad="12"/>
</signal>
<signal name="N$6">
<contactref element="IC6" pad="3"/>
<contactref element="R86" pad="2"/>
<contactref element="C82" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC4" pad="13"/>
<contactref element="R3" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="C81" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="IC6" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC1" pad="6"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC5" pad="10"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="2"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="-5VA">
<contactref element="C12" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="IC16" pad="3"/>
<contactref element="C16" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="IC6" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="IC14" pad="4"/>
<contactref element="C35" pad="2"/>
<contactref element="IC13" pad="5"/>
<contactref element="C63" pad="2"/>
<contactref element="IC22" pad="3"/>
<contactref element="C60" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="IC20" pad="4"/>
<contactref element="IC12" pad="3"/>
<contactref element="C29" pad="1"/>
<contactref element="C33" pad="-"/>
<contactref element="IC15" pad="4"/>
<contactref element="IC21" pad="4"/>
<contactref element="D2" pad="1"/>
<contactref element="D3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="+3.3V">
<contactref element="MOD1" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="IC7" pad="4"/>
<contactref element="R29" pad="2"/>
<contactref element="C32" pad="+"/>
<contactref element="IC11" pad="3"/>
<contactref element="C26" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="!AC-I_CS">
<contactref element="IC16" pad="6"/>
<contactref element="MOD1" pad="8"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="+5VA">
<contactref element="C9" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="C11" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC4" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="IC17" pad="8"/>
<contactref element="C44" pad="2"/>
<contactref element="IC16" pad="8"/>
<contactref element="C50" pad="2"/>
<contactref element="IC18" pad="8"/>
<contactref element="C15" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="IC6" pad="5"/>
<contactref element="C41" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="IC19" pad="2"/>
<contactref element="IC14" pad="8"/>
<contactref element="C34" pad="2"/>
<contactref element="IC13" pad="8"/>
<contactref element="C56" pad="2"/>
<contactref element="IC20" pad="8"/>
<contactref element="C65" pad="2"/>
<contactref element="IC23" pad="8"/>
<contactref element="C62" pad="2"/>
<contactref element="IC22" pad="8"/>
<contactref element="C68" pad="2"/>
<contactref element="IC24" pad="8"/>
<contactref element="C59" pad="2"/>
<contactref element="C71" pad="2"/>
<contactref element="IC25" pad="2"/>
<contactref element="C31" pad="+"/>
<contactref element="IC10" pad="3"/>
<contactref element="C25" pad="2"/>
<contactref element="IC15" pad="8"/>
<contactref element="IC21" pad="8"/>
<contactref element="D2" pad="3"/>
<contactref element="D3" pad="3"/>
<contactref element="C76" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="C78" pad="1"/>
<contactref element="C79" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="DIS1" pad="RXD"/>
<contactref element="MOD1" pad="24"/>
</signal>
<signal name="N$24">
<contactref element="R33" pad="2"/>
<contactref element="SW2" pad="A1"/>
</signal>
<signal name="N$38">
<contactref element="R33" pad="2S"/>
<contactref element="SW2" pad="B1"/>
</signal>
<signal name="N$50">
<contactref element="R34" pad="1"/>
<contactref element="SW2" pad="A2"/>
<contactref element="SW2" pad="B2"/>
</signal>
<signal name="N$51">
<contactref element="R35" pad="1"/>
<contactref element="SW2" pad="A3"/>
<contactref element="SW2" pad="B3"/>
</signal>
<signal name="N$52">
<contactref element="R36" pad="1"/>
<contactref element="SW2" pad="A4"/>
<contactref element="SW2" pad="B4"/>
</signal>
<signal name="N$53">
<contactref element="R37" pad="1"/>
<contactref element="SW2" pad="A5"/>
<contactref element="SW2" pad="B5"/>
</signal>
<signal name="N$54">
<contactref element="R38" pad="1"/>
<contactref element="SW2" pad="A6"/>
<contactref element="SW2" pad="B6"/>
</signal>
<signal name="N$55">
<contactref element="R39" pad="1"/>
<contactref element="SW2" pad="A7"/>
<contactref element="SW2" pad="B7"/>
</signal>
<signal name="ADC-DCI">
<contactref element="IC17" pad="6"/>
<contactref element="MOD1" pad="19"/>
</signal>
<signal name="N$14">
<contactref element="R48" pad="1"/>
<contactref element="R47" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="IC14" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R48" pad="2"/>
<contactref element="C38" pad="1"/>
<contactref element="IC14" pad="1"/>
<contactref element="R51" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="IC17" pad="3"/>
<contactref element="C46" pad="1"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC17" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="R55" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC16" pad="1"/>
<contactref element="R50" pad="2"/>
<contactref element="C37" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="IC16" pad="10"/>
<contactref element="R49" pad="1"/>
<contactref element="C36" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="IC18" pad="3"/>
<contactref element="R59" pad="2"/>
<contactref element="C49" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="IC18" pad="2"/>
<contactref element="R58" pad="2"/>
<contactref element="C49" pad="2"/>
<contactref element="D7" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="IC16" pad="7"/>
<contactref element="R53" pad="1"/>
<contactref element="C80" pad="2"/>
</signal>
<signal name="ADC-ACI">
<contactref element="IC18" pad="6"/>
<contactref element="MOD1" pad="20"/>
</signal>
<signal name="N$19">
<contactref element="MOD1" pad="41"/>
<contactref element="MOD1" pad="27"/>
</signal>
<signal name="ADC-CONVERT">
<contactref element="IC17" pad="5"/>
<contactref element="IC18" pad="5"/>
<contactref element="MOD1" pad="25"/>
<contactref element="R29" pad="1"/>
<contactref element="IC23" pad="5"/>
<contactref element="IC24" pad="5"/>
</signal>
<signal name="N$28">
<contactref element="SW2" pad="B8"/>
<contactref element="R40" pad="2"/>
<contactref element="SW2" pad="A8"/>
</signal>
<signal name="N$29">
<contactref element="SW2" pad="B9"/>
<contactref element="R41" pad="2"/>
<contactref element="SW2" pad="A9"/>
</signal>
<signal name="N$32">
<contactref element="SW2" pad="B10"/>
<contactref element="R42" pad="2"/>
<contactref element="SW2" pad="A10"/>
</signal>
<signal name="ADC-ACV">
<contactref element="MOD1" pad="18"/>
<contactref element="IC24" pad="6"/>
</signal>
<signal name="ADC-DCV">
<contactref element="MOD1" pad="17"/>
<contactref element="IC23" pad="6"/>
</signal>
<signal name="N$45">
<contactref element="MOD1" pad="32"/>
<contactref element="IC7" pad="5"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="IC7" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="IC7" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="IC4" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="SW1" pad="A-COM"/>
<contactref element="C81" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="SW1" pad="A1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="R8" pad="2"/>
<contactref element="SW1" pad="B1"/>
</signal>
<signal name="N$57">
<contactref element="SW1" pad="A2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="R9" pad="2"/>
<contactref element="SW1" pad="B2"/>
</signal>
<signal name="N$59">
<contactref element="SW1" pad="A3"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="R10" pad="2"/>
<contactref element="SW1" pad="B3"/>
</signal>
<signal name="N$61">
<contactref element="SW1" pad="A4"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="R11" pad="2"/>
<contactref element="SW1" pad="B4"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$66">
<contactref element="J3" pad="UPR-COM"/>
<contactref element="R66" pad="2"/>
</signal>
<signal name="N$67">
<contactref element="R45" pad="2"/>
<contactref element="J2" pad="UPR-COM"/>
</signal>
<signal name="N$68">
<contactref element="SW1" pad="A5"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="R13" pad="1"/>
<contactref element="SW1" pad="A6"/>
</signal>
<signal name="N$70">
<contactref element="SW1" pad="A7"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="R15" pad="1"/>
<contactref element="SW1" pad="A8"/>
</signal>
<signal name="N$72">
<contactref element="SW1" pad="A9"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="R17" pad="1"/>
<contactref element="SW1" pad="A10"/>
</signal>
<signal name="N$74">
<contactref element="R17" pad="2"/>
<contactref element="SW1" pad="B10"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$75">
<contactref element="SW1" pad="B9"/>
<contactref element="R16" pad="2"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$76">
<contactref element="R15" pad="2"/>
<contactref element="SW1" pad="B8"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$77">
<contactref element="SW1" pad="B7"/>
<contactref element="R14" pad="2"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$78">
<contactref element="R13" pad="2"/>
<contactref element="SW1" pad="B6"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$79">
<contactref element="SW1" pad="B5"/>
<contactref element="R12" pad="2"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC5" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$83">
<contactref element="C43" pad="1"/>
<contactref element="R53" pad="2"/>
<contactref element="IC15" pad="2"/>
</signal>
<signal name="N$84">
<contactref element="C43" pad="2"/>
<contactref element="IC15" pad="1"/>
<contactref element="R85" pad="1"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="+4VB">
<contactref element="IC19" pad="6"/>
<contactref element="R60" pad="2"/>
<contactref element="C48" pad="2"/>
<contactref element="IC17" pad="1"/>
<contactref element="C51" pad="2"/>
<contactref element="IC18" pad="1"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="+2VB">
<contactref element="R61" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="R60" pad="1"/>
<contactref element="IC15" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="IC13" pad="6"/>
<contactref element="R46" pad="2"/>
<contactref element="IC19" pad="4"/>
<contactref element="C52" pad="1"/>
<contactref element="R61" pad="1"/>
<contactref element="IC16" pad="9"/>
<contactref element="R59" pad="1"/>
<contactref element="R50" pad="1"/>
<contactref element="R56" pad="1"/>
<contactref element="R47" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C53" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="IC14" pad="7"/>
<contactref element="R55" pad="1"/>
<contactref element="IC14" pad="6"/>
</signal>
<signal name="N$33">
<contactref element="IC14" pad="5"/>
<contactref element="R52" pad="1"/>
<contactref element="R51" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="C75" pad="2"/>
</signal>
<signal name="+2VA">
<contactref element="R83" pad="2"/>
<contactref element="C70" pad="2"/>
<contactref element="R82" pad="1"/>
<contactref element="IC21" pad="3"/>
</signal>
<signal name="+4VA">
<contactref element="C69" pad="2"/>
<contactref element="IC24" pad="1"/>
<contactref element="IC25" pad="6"/>
<contactref element="R82" pad="2"/>
<contactref element="R74" pad="2"/>
<contactref element="C66" pad="2"/>
<contactref element="IC23" pad="1"/>
</signal>
<signal name="N$92">
<contactref element="R62" pad="2"/>
<contactref element="J1" pad="LWR-COM"/>
</signal>
<signal name="N$95">
<contactref element="R64" pad="2"/>
<contactref element="J3" pad="LWR-COM"/>
</signal>
<signal name="N$96">
<contactref element="IC13" pad="2"/>
<contactref element="R43" pad="2"/>
</signal>
<signal name="N$97">
<contactref element="R43" pad="1"/>
<contactref element="IC13" pad="3"/>
</signal>
<signal name="N$98">
<contactref element="IC25" pad="4"/>
<contactref element="C70" pad="1"/>
<contactref element="R83" pad="1"/>
<contactref element="IC22" pad="9"/>
<contactref element="R81" pad="1"/>
<contactref element="R72" pad="1"/>
<contactref element="R78" pad="1"/>
<contactref element="R69" pad="1"/>
<contactref element="C58" pad="1"/>
<contactref element="SW3" pad="D-COM"/>
<contactref element="D1" pad="4"/>
<contactref element="C71" pad="1"/>
</signal>
<signal name="N$99">
<contactref element="SW3" pad="C-COM"/>
<contactref element="IC20" pad="3"/>
<contactref element="C54" pad="1"/>
<contactref element="D3" pad="4"/>
</signal>
<signal name="N$102">
<contactref element="R70" pad="1"/>
<contactref element="R69" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="IC20" pad="2"/>
</signal>
<signal name="N$103">
<contactref element="R70" pad="2"/>
<contactref element="C55" pad="1"/>
<contactref element="IC20" pad="1"/>
<contactref element="R73" pad="1"/>
</signal>
<signal name="N$104">
<contactref element="IC23" pad="3"/>
<contactref element="C64" pad="1"/>
<contactref element="R78" pad="2"/>
</signal>
<signal name="N$105">
<contactref element="IC23" pad="2"/>
<contactref element="C64" pad="2"/>
<contactref element="R77" pad="2"/>
</signal>
<signal name="N$106">
<contactref element="IC22" pad="1"/>
<contactref element="R72" pad="2"/>
<contactref element="C58" pad="2"/>
</signal>
<signal name="N$107">
<contactref element="IC22" pad="10"/>
<contactref element="R71" pad="1"/>
<contactref element="C54" pad="2"/>
</signal>
<signal name="N$108">
<contactref element="IC24" pad="3"/>
<contactref element="R81" pad="2"/>
<contactref element="C67" pad="1"/>
</signal>
<signal name="N$109">
<contactref element="IC24" pad="2"/>
<contactref element="R80" pad="2"/>
<contactref element="C67" pad="2"/>
<contactref element="D6" pad="2"/>
</signal>
<signal name="N$110">
<contactref element="IC22" pad="7"/>
<contactref element="R75" pad="1"/>
<contactref element="C74" pad="2"/>
</signal>
<signal name="N$111">
<contactref element="C61" pad="1"/>
<contactref element="R75" pad="2"/>
<contactref element="IC21" pad="2"/>
</signal>
<signal name="N$112">
<contactref element="C61" pad="2"/>
<contactref element="IC21" pad="1"/>
<contactref element="R76" pad="1"/>
<contactref element="R84" pad="1"/>
</signal>
<signal name="N$113">
<contactref element="IC20" pad="7"/>
<contactref element="R77" pad="1"/>
<contactref element="IC20" pad="6"/>
</signal>
<signal name="N$114">
<contactref element="IC20" pad="5"/>
<contactref element="R74" pad="1"/>
<contactref element="R73" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="C73" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="J4" pad="UPR-COM"/>
<contactref element="R67" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="J3" pad="UPR-CTR"/>
<contactref element="SW3" pad="A-UP"/>
</signal>
<signal name="N$36">
<contactref element="J4" pad="UPR-CTR"/>
<contactref element="SW3" pad="A-DN"/>
</signal>
<signal name="N$37">
<contactref element="R44" pad="2"/>
<contactref element="J1" pad="UPR-COM"/>
</signal>
<signal name="N$40">
<contactref element="F2" pad="2A"/>
<contactref element="F2" pad="2B"/>
<contactref element="SW3" pad="B-COM"/>
</signal>
<signal name="N$41">
<contactref element="SW3" pad="B-DN"/>
<contactref element="J2" pad="UPR-CTR"/>
</signal>
<signal name="N$42">
<contactref element="SW3" pad="B-UP"/>
<contactref element="J1" pad="UPR-CTR"/>
</signal>
<signal name="N$43">
<contactref element="R63" pad="2"/>
<contactref element="J2" pad="LWR-COM"/>
</signal>
<signal name="N$44">
<contactref element="R65" pad="2"/>
<contactref element="J4" pad="LWR-COM"/>
</signal>
<signal name="N$64">
<contactref element="SW3" pad="D-UP"/>
<contactref element="J3" pad="LWR-CTR"/>
</signal>
<signal name="N$65">
<contactref element="J4" pad="LWR-CTR"/>
<contactref element="SW3" pad="D-DN"/>
</signal>
<signal name="N$80">
<contactref element="SW3" pad="C-UP"/>
<contactref element="J1" pad="LWR-CTR"/>
</signal>
<signal name="N$81">
<contactref element="J2" pad="LWR-CTR"/>
<contactref element="SW3" pad="C-DN"/>
</signal>
<signal name="N$82">
<contactref element="IC9" pad="1"/>
<contactref element="F1" pad="2A"/>
<contactref element="F1" pad="2B"/>
<contactref element="C21" pad="2"/>
<contactref element="IC10" pad="1"/>
<contactref element="IC11" pad="1"/>
<contactref element="PWR1" pad="+VIN"/>
<contactref element="C20" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
</signal>
<signal name="N$86">
<contactref element="+6V" pad="TP"/>
<contactref element="F1" pad="1B"/>
<contactref element="F1" pad="1A"/>
</signal>
<signal name="N$87">
<contactref element="PWR1" pad="TRM"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$85">
<contactref element="PWR1" pad="COM"/>
<contactref element="R31" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="C28" pad="-"/>
<contactref element="IC12" pad="2"/>
<contactref element="IC12" pad="4"/>
</signal>
<signal name="N$88">
<contactref element="R58" pad="1"/>
<contactref element="IC15" pad="7"/>
<contactref element="R57" pad="2"/>
<contactref element="RLY1" pad="COM2"/>
</signal>
<signal name="!RLY_CS">
<contactref element="MOD1" pad="21"/>
<contactref element="IC8" pad="1"/>
</signal>
<signal name="RLY_ACI_X3">
<contactref element="IC8" pad="4"/>
<contactref element="RLY1" pad="S-"/>
</signal>
<signal name="RLY_ACV_X1">
<contactref element="IC8" pad="21"/>
<contactref element="RLY2" pad="R-"/>
</signal>
<signal name="RLY_ACV_X3">
<contactref element="IC8" pad="22"/>
<contactref element="RLY2" pad="S-"/>
</signal>
<signal name="RLY_ACI_X1">
<contactref element="IC8" pad="3"/>
<contactref element="RLY1" pad="R-"/>
</signal>
<signal name="N$89">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="+5RLY">
<contactref element="Q1" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="RLY1" pad="S+"/>
<contactref element="RLY1" pad="R+"/>
<contactref element="RLY2" pad="S+"/>
<contactref element="RLY2" pad="R+"/>
</signal>
<signal name="N$91">
<contactref element="R79" pad="2"/>
<contactref element="RLY2" pad="NC2"/>
<contactref element="IC21" pad="7"/>
<contactref element="R80" pad="1"/>
</signal>
<signal name="N$93">
<contactref element="R79" pad="1"/>
<contactref element="R76" pad="2"/>
<contactref element="IC21" pad="6"/>
<contactref element="RLY2" pad="COM2"/>
</signal>
<signal name="!RLY_5V">
<contactref element="R1" pad="1"/>
<contactref element="MOD1" pad="22"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R57" pad="1"/>
<contactref element="R54" pad="2"/>
<contactref element="IC15" pad="6"/>
<contactref element="RLY1" pad="NC2"/>
</signal>
<signal name="N$22">
<contactref element="R33" pad="1S"/>
<contactref element="R34" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="R39" pad="2"/>
<contactref element="R41" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="R42" pad="1"/>
<contactref element="R40" pad="1S"/>
<contactref element="R41" pad="1S"/>
<contactref element="R42" pad="1S"/>
<contactref element="IC13" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="IC14" pad="3"/>
<contactref element="C36" pad="1"/>
<contactref element="IC13" pad="7"/>
</signal>
<signal name="SOURCE">
<contactref element="SW1" pad="B-COM"/>
<contactref element="SW2" pad="A-COM"/>
</signal>
<signal name="N$31">
<contactref element="R33" pad="1"/>
<contactref element="F2" pad="1B"/>
<contactref element="F2" pad="1A"/>
</signal>
<signal name="N$39">
<contactref element="SW3" pad="A-COM"/>
<contactref element="R68" pad="2"/>
</signal>
<signal name="N$63">
<contactref element="SW2" pad="B-COM"/>
<contactref element="IC13" pad="4"/>
</signal>
<signal name="!AC-V_CS">
<contactref element="IC22" pad="6"/>
<contactref element="MOD1" pad="9"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$90">
<contactref element="IC21" pad="5"/>
<contactref element="R84" pad="2"/>
<contactref element="C74" pad="1"/>
</signal>
<signal name="N$94">
<contactref element="IC15" pad="5"/>
<contactref element="R85" pad="2"/>
<contactref element="C80" pad="1"/>
</signal>
<signal name="N$100">
<contactref element="IC4" pad="2"/>
<contactref element="R86" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
