<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="52.705" y2="0" width="0" layer="20"/>
<wire x1="52.705" y1="0" x2="52.705" y2="31.115" width="0" layer="20"/>
<wire x1="52.705" y1="31.115" x2="0" y2="31.115" width="0" layer="20"/>
<wire x1="0" y1="31.115" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="QuantumOptics">
<packages>
<package name="TSSOP-20">
<description>&lt;b&gt;TSSOP-20&lt;/b&gt;, pins 0.65mm c-c spacing, nominal 6.4mm rows.</description>
</package>
<package name="2012(0805)">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, 0805 SMT, based on Kemet's description.</description>
</package>
<package name="EIA-6032">
<description>&lt;b&gt;R, C or L&lt;/b&gt;, EIA-6032, SMT.</description>
</package>
<package name="MSOP8@1">
<description>&lt;b&gt;MSOP-8&lt;/b&gt;, A.K.A. RM-8.  Use 0.025" grid.</description>
</package>
<package name="BOURNS_3310">
<description>&lt;b&gt;Pot, Bourns 3310C&lt;/a&gt;, single turn, cheap: tempco ±1,000PPM, 50,000 cycle life.&lt;br&gt;
&lt;a href = "http://www.bourns.com/PDFs/3310.pdf"&gt;
http://www.bourns.com/PDFs/3310.pdf&lt;/a&gt;</description>
</package>
<package name="TP-0.042">
<description>&lt;b&gt;Test Point&lt;/b&gt;, 0.042" hole, to fit small test point.  Has fence around to allow easier soldering.  Drilled 0.0465, plated down to 1.1mm.</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;, on 0.025" grid.  Terminal 4 (case) is not connected here, use a polygon with the connection name as a heatsink.</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;SOT-23-5&lt;/b&gt;, based on TI's version of JEDEC MO-175 Variant AA.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="QuantumOptics" package="TSSOP-20" value="SA575DTB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="QuantumOptics" package="2012(0805)" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="R6" library="QuantumOptics" package="2012(0805)" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="QuantumOptics" package="2012(0805)" value="30.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="QuantumOptics" package="2012(0805)" value="0.47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="QuantumOptics" package="2012(0805)" value="20.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="QuantumOptics" package="2012(0805)" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C6" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="QuantumOptics" package="EIA-6032" value="150uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="QuantumOptics" package="2012(0805)" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="QuantumOptics" package="2012(0805)" value="1.10M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="QuantumOptics" package="2012(0805)" value="10.0M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="QuantumOptics" package="MSOP8@1" value="NCP2890DMR2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C19" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="QuantumOptics" package="EIA-6032" value="150uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="QuantumOptics" package="2012(0805)" value="20.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="R10" library="QuantumOptics" package="BOURNS_3310" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SP1" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="SP2" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="IC3" library="QuantumOptics" package="SOT223" value="LM1117-5.0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="IC4" library="QuantumOptics" package="SOT223" value="LM1117-5.0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MFG" value=""/>
<attribute name="PN" value=""/>
</element>
<element name="C15" library="QuantumOptics" package="EIA-6032" value="150uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="-" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="R8" library="QuantumOptics" package="2012(0805)" value="3.16K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="IN" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="COM" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="IC1" library="QuantumOptics" package="SOT23-5" value="AD8605ART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="QuantumOptics" package="2012(0805)" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="QuantumOptics" package="2012(0805)" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="QuantumOptics" package="2012(0805)" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="QuantumOptics" package="2012(0805)" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="QuantumOptics" package="2012(0805)" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GN1" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
<element name="GN2" library="QuantumOptics" package="TP-0.042" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="10"/>
<contactref element="C11" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="-"/>
<contactref element="C18" pad="1"/>
<contactref element="IC5" pad="7"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="-"/>
<contactref element="C16" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C15" pad="-"/>
<contactref element="-" pad="TP"/>
<contactref element="COM" pad="TP"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C13" pad="1"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$3">
<contactref element="C12" pad="1"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="14"/>
<contactref element="IC2" pad="11"/>
<contactref element="C10" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="C10" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="N$4">
<contactref element="C8" pad="1"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$8">
<contactref element="C14" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C5" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="C6" pad="2"/>
<contactref element="IC2" pad="20"/>
<contactref element="C7" pad="+"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="IN" pad="TP"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC5" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R9" pad="2"/>
<contactref element="IC5" pad="4"/>
<contactref element="R10" pad="W"/>
</signal>
<signal name="N$17">
<contactref element="C19" pad="2"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="6"/>
<contactref element="C20" pad="+"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC5" pad="3"/>
<contactref element="R11" pad="2"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC5" pad="5"/>
<contactref element="SP1" pad="TP"/>
<contactref element="R10" pad="CCW"/>
</signal>
<signal name="N$19">
<contactref element="SP2" pad="TP"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="N$21">
<contactref element="C17" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="C9" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="C15" pad="+"/>
<contactref element="+" pad="TP"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="LED" pad="TP"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="4"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="GN1" pad="TP"/>
</signal>
<signal name="N$24">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="GN2" pad="TP"/>
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
